TRD - Tender Response Document Open Procedure – Supply and Delivery of Re-chassised & Upgrade Works to an Emergency Tender Fire Appliance
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TENDER RESPONSE DOCUMENT

	Title of Procurement

	To Supply and Deliver the Re-chassis & Upgrade Works to an Emergency Tender Fire Appliance to Longford County Council

	Closing Date & Time for Receipt of Tenders
	16:00 on 10th July 2026

	Organisation Name
	Longford Fire & Rescue Service

	Contact Name 
	Austin Concannon

	Contact Email
	firestation@longfordcoco.ie
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[bookmark: _Toc16597912][bookmark: _Toc61968791][bookmark: _Hlk535242154]Instructions for Completion
[bookmark: _Hlk13580347]This document MUST be used for the submission of tenders. Please read the following instructions carefully.
· Tenderers should ensure they have read the Request for Tender before they attempt to complete this Tender Response Document. 
 
· If you consider that the Tender Response Document is missing any sections which would prevent you from preparing a comprehensive response, please contact the Contracting Authority as soon as possible.   

· Where there is a discrepancy between the contents / instructions in this document and the Request for Tender, the Request for Tender will take precedence. 
  
· Tenderers must follow the instructions contained in this document in relation to attachments, format for submission, etc.  

· [bookmark: _Hlk495513867]Where tenderers are relying on other parties to meet the selection criteria, those parties must be available to deliver elements of the contract. 


[bookmark: _Toc16597913][bookmark: _Toc61968792][bookmark: _Hlk13580304]Response to the Selection Criteria
[bookmark: _Toc61968793]General Contact Information
	Organisation Name:
	

	Contact Person:
	

	Position: 
	

	Address: 
	

	Phone:
	

	Email: 
	

	Website: 
	

	Date of Establishment, if applicable:
	VAT Registration No:
	Legal Structure – partnership, limited company, etc.

	
	
	

	Details of any Sub-contractors or Consortium members:

	Name
	Proposed Role in Delivery of the Contract
	Confirmation relevant information is provided for each party (e.g. financial, experience, or other selection criterion where applicable)  

	
	
	

	
	
	

	
	
	



[bookmark: _Toc16597916][bookmark: _Toc61968794]SELECTION CRITERIA - Pass/Fail Criteria
Financial Information
	
Tax Clearance

	I confirm and declare being tax compliant.  The Contracting Authority can verify your tax clearance status through Revenue’s online facility at http://www.revenue.ie/en/online/tax-clearance.html To this end, please confirm:
	Yes
	

	(A) 
	No
	

	Tenderer Name:
	

	Tenderer PPSN/ Tax Reference Number:
	

	Access Number:
	

	OR, I confirm that I hold a current valid paper Tax Clearance Certificate (generally relates to Non-Residents)

	Registration Number:
	
	Certificate Number:
	

	OR, 
I confirm that I have applied for Tax Clearance status or a Tax Clearance Certificate which will be made available on request
	Yes
	

	
	No
	

	Turnover

	I confirm that we have the requisite qualification to be considered for the contract of a minimum annual financial turnover (ex VAT ) required of €540,000.


	Year
	2025
	2024
	2023

	Month End (e.g July)
	

	
	

	Turnover in €
	

	
	

	We Confirm that we have the financial capacity to pay our debts identified on the current statement of assets and liabilities as being the debts as they fall due. 
	Yes
	

	
	No
	

	I confirm that I will provide evidence of turnover and capacity to pay our debts promptly on request.
NOTE #1:  In the case of sole traders or partnerships this condition may be satisfied by a letter of confirmation from a senior partner.
	Yes
	

	
	No
	

	
Insurances 

	I confirm that we have the following insurances in place 

	Insurance Type
	Level required if successful
	Level in Place
	Details of Any Excess
	Renewal Date

	Employers Liability
	€13,000,000
	€
	
	

	Public Liability
	€6,500,000
	€
	
	

	Product Liability
	€6,500,000
	€
	
	

	Professional Indemnity
	€1,000,000
	€
	
	

	AND

	I confirm that if successful, where the levels required under the contract/framework are higher than those currently in our possession, I will be in a position to put the required forms and levels of insurances required in place. 
	

	AND

	I confirm that I will provide the following promptly on request:
· evidence of insurances in place
      or 
· letter from Insurance Broker confirming that the required levels can be put in place if successful 
	









[bookmark: _Toc16597917][bookmark: _Toc61968795]Declaration Re Personal Circumstances – Pass/Fail Criteria
	DECLARATION RE PERSONAL CIRCUMSTANCES AS PER ART. 57 OF DIRECTIVE 2014/24/EU
Economic Operators will be excluded from the procurement process if, within the past five (5) years, there is evidence of a conviction relating to a specific criminal offence listed below (see 1.1) or if they have been the subject of a binding legal decision which found a breach of legal obligations to pay tax or social security contributions (see 1.2) (except where this is disproportionate e.g. where only minor amounts are involved).

	1.1 	Has the Economic Operator or a member of their proposed 	consortium, (if applicable), Director, or Partner or any other 	person who has powers of representation, decision or 	control, been convicted of any of the following offences?
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box 

	1.1.a
	participation in a criminal organisation, as defined in Article 2 of Council Framework decision 2008/841/JHA;
	
	

	1.1.b
	corruption, as defined in Article 3 of the Convention on the fight against corruption involving officials of the European Communities or officials of Member States of the European Union and Article 2(1) of Council Framework Decision 2003/568/JHA as well as corruption as defined in Irish Law or the jurisdiction in which the Economic Operator is established;
	
	

	1.1.c
	fraud within the meaning of Article 1 of the Convention on the protection of the European Communities’ financial interests;
	
	

	1.1.d
	the subject of a conviction for terrorist offences or offences linked to terrorist activities or for inciting or aiding or abetting or attempting to commit an offence; 
	
	

	1.1.e
	the subject of a conviction for money laundering or terrorist financing; 
	
	

	1.1.f
	the subject of a conviction of child labour and other forms of trafficking in human beings;
	
	

	Non-payment of taxes or social security obligations
1.2 Has it been established by a judicial or administrative decision having final and binding effect in accordance with Irish law or the legal provisions of the country in which the Economic Operator is established (if outside Ireland), that the Economic Operator is in breach of obligations related to the payment of tax and social security contributions?
Note: If the response to 1.2 above is in the affirmative, please provide further information on the decision and the amounts involved
	
	



	2.1 	Please indicate if any of the following situations have applied, 	within the past three (3) years, or currently apply, to your 	organisation.
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box

	2.1.a
	has, in the performance of any public contract, failed to comply with applicable obligations in the field of environmental, social and labour law applying at the place where the works were carried out or the services provided, as established by EU law, national law, collective agreements or by international, environmental, social and labour law listed in Annex X of Directive 2014/24/EU;
	
	

	2.1.b
	is bankrupt or the subject of insolvency or winding-up proceedings, its assets are being administered by a liquidator or by the court, or has entered into an arrangement with creditors, suspended its business activities or is in any analogous situation arising from a similar procedure under national laws and regulations;  
	
	

	2.1.c
	is guilty of grave professional misconduct which renders its integrity questionable;
	
	

	2.1.d
	has entered into agreements with other economic operators aimed at distorting competition;
	
	

	2.1.e 
	has a conflict of interest within the meaning of Article 24 of 2014/24/EU that cannot be effectively remedied by other, less intrusive, measures; 
	
	

	2.1.f 
	confirms that it has had prior involvement in the preparation of the procurement procedure which has resulted in a distortion of competition, as referred to in Article 41 of 2014/24/EU, that cannot be remedied by other, less intrusive, measures;
	
	

	2.1.g
	has shown significant or persistent deficiencies in the performance of a substantive requirement under a prior public contract, a prior contract with a contracting entity, or a prior concession contract, which led to early termination of that prior contract, damages or other comparable sanctions. 
	
	

	2.1.h
	· is guilty of serious misrepresentation in supplying the information required for the verification of the absence of grounds for exclusion or the fulfilment of the selection criteria; or
	
	

	
	· has withheld such information or is not able to submit supporting documents required under Article 59 of Directive 2014/24/EU; or 
	
	

	2.1.i
	has undertaken to:
· unduly influence the decision-making process of the contracting entity, or
· obtain confidential information that may confer upon the Tenderer undue advantages in the procurement procedure; or
· negligently provide misleading information that may have a material influence on decisions concerning exclusion, selection or award.
	
	

	3.
	Comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same);
	
	

	4.
	The origin of goods connected to the Tender, if any, are subject to the prohibitions set out in Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same)
	
	

	5.
	Any subcontractor, supplier or other entity on whose capacity the organization relies as part of the Tender comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	


[bookmark: _Toc487559492]

[bookmark: _Toc16597918][bookmark: _Toc61968796]Declaration Re Statutory Obligations – Pass/Fail Criteria
	We confirm that we are fully compliant with the following legislation, or equivalent legislation in our country of establishment/operation:
	YES
	NO

	(a) 
	Safety, Health and Welfare at Work Act 2005 and Safety, Health and Welfare at Work (General Application) Regulations 2007
	
	

	(b) 
	Do you comply with Longford County Council Health and Safety Systems including policies and procedures (i.e. Contractors Prequalification questionnaire requirements(available on request))? 
	
	

	(c) 
	Employment Equality Acts 1998-2011 
	
	

	(d) 
	Equal Status Acts 2000-2011
	
	

	(e) 
	National Minimum Wage Act 2000 as amended 
	
	

	(f) 
	Organisation of Working Time Act 1997 as amended
	
	

	(g) 
	Disability Act 2005
	
	

	(h) 
	Regulation (EU) 2016/679 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data, the Data Protection Act, 2018
	
	

	(i) 
	We further confirm that all Data Subjects whose Personal Data is provided in our Tender have consented to the processing of such Personal Data by us, the Contracting Authority, the Evaluation Team and the supplier of the etenders.gov.ie website, for the purposes of our participation in this Competition or that we otherwise have a legal basis for providing such Personal Data to the Contracting Authority for the purposes of our participation in this Competition and that we will provide evidence of such consent and / or legal basis to the Contracting Authority upon request.
	
	

	(j) 
	We have procedures in place to ensure that our subcontractors, if any are used for this contract, apply the same standards.
	
	

	This Declaration is made for the benefit of the Contracting Authority. 
I certify that the information provided in the Declaration re Personal Circumstances and the Declaration re Statutory Obligations is accurate and complete to the best of my knowledge and belief.  I understand that the provision of inaccurate or misleading information in these Declarations will lead to my organisation being excluded from participation in this and future tenders and I am signing on behalf of: 

	Name of Tenderer
	


	Name of Authorised Signatory
	


	Position
	


	Signature
	




Workshop Facility - Pass/Fail Criteria
Tenderers must operate, either directly or via an agent, at least one workshop facility with the capacity and capability to carry out repairs/servicing to the fire appliance and the ancillary equipment procured under this Contract. 
Please provide details of the workshop:
	







Call-out Service - Pass/Fail Criteria
Tenderers must have the capability to provide a call-out service within 24 hours on a nationwide basis in the Republic of Ireland. Any costs associated with collection and transport of fire appliances to the Tenderer’s workshop must be borne by the Tenderer.
Please provide details of your call-out service:
	






[bookmark: _Toc16597921][bookmark: _Toc61968797]Previous Contracts / Experience - Pass/Fail Criteria
	Reference Contract #1

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	







	Any other relevant information 

	

	Reference Contract #2

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	


	Reference Contract #3

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	



[bookmark: _Toc16597922][bookmark: _Toc61968798]Health & Safety - Pass/Fail Criteria
	Do you comply with the Safety Health & Welfare at Work Act 2005 
	Yes
	
	No
	

	Do you comply with Longford County Council Health and Safety Systems including policies and procedures (i.e. Contractors Prequalification questionnaire requirements)?
	Yes
	
	No
	

	Name of Manager responsible for Health and Safety 
	

	Is it 3rd party certified or managed in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	I confirm that evidence of compliance will be provided promptly on request.
	Yes
	

	
	No
	





[bookmark: _Toc16597923][bookmark: _Toc61968799]Quality Assurance – Pass/Fail Criteria 
	Do you operate a quality management system? 
	Yes
	
	No
	

	Name of Manager responsible for Quality 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	If in-house, please provide summary of system: 
	







[bookmark: _Toc16597924][bookmark: _Toc61968800]Environmental Management Systems – Pass/Fail Criteria 
[bookmark: _Toc488834423][bookmark: _Toc460518593][bookmark: _Toc474254483]
	Do you operate an Environmental Management System / Policy? 
	Yes
	
	No
	

	Name of Manager responsible for Environmental Management 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	  

	If in-house, please provide summary of system: 
	




















[bookmark: _Toc16597925][bookmark: _Toc61968802]Response to the Award Criteria
Award Criterion 1 – Compliance with Technical Specifications & Minimum Warranty Requirements 
	Criterion 1:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Compliance with Technical Specifications & Minimum Warranty Requirements 
	
	
	

	
	Pass/Fail
	N/A
	N/A

	Instructions
	The Tenderer must detail here the compliance of the tendered vehicle with the technical specifications and minimum warranty requirements set out in Appendix 1.
Longford County Council will review various proposed solutions along with variations and will determine if the solution proposed broadly meets their requirements as set out in the RFT.
Only Tenders that receive a “Pass” mark for this award criterion will proceed to be evaluated under the remaining award criteria.
As a minimum tenderers are requested to carry out the following;
· Complete requested technical detail in the areas provided below
· Ensure Comments/Variations are included in the column provided where applicable. Insert ‘N/A’ if not applicable
· Ensure boxes labelled ‘ Tenderers to fill in details Here ‘ are completed with the required information




1. [bookmark: _Toc61968804]General 

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	1.1
	The appliance must be re-chassied and refurbished in accordance with all relevant sections of the most recent edition of all parts of EN 1846 (or equivalent) for rescue service vehicles, and any subsequent amendments of same on the date this tender was advertised (unless specifically stated otherwise within this RFT). The objective of the process is to upgrade the current Emergency Tender appliance re-using as many components as possible from the current appliance.
	
	

	1.2
	The appliance must be constructed in accordance with all relevant parts of the ‘Road Traffic (Construction, Equipment and Use of Vehicles) (Amendment) Regulations’ – (http://www.irishstatutebook.ie) and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.3
	The appliance must be constructed in accordance with the most recent edition of the Council Directive 2003/20/EEC on the approximation of the laws of the Member States relating to safety belts and restraint systems of motor vehicles and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.4
	The design of an appliance and the stowage of equipment shall be in accordance with the Safety, Health and Welfare at Work Act 2005 and the Safety, Health and Welfare at Work General Application (Amendment) Regulations (and latest editions), with particular regard to Manual Handling of Loads, and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.5
	The cab construction must conform to ECE R29 (or equivalent) Standards and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.6
	Man-made fibres used in the construction of the appliance shall have a fire-retardant additive so that, as a minimum, the material conforms to the latest relevant sections of standard BS476/EN 13501-1.
	
	

	1.7
	The current appliance shall be collected by the supplier from the Brigade Headquarters at the following location (or alternate Fire Station nominated at the time of placing the official order);

Longford Fire Station HQ, 
Templemichael,
Longford, 
Co. Longford, Ireland.
N39 FW96

It will be a matter for the supplier to transport the existing appliance to their own workshop and to the workshops of the Hiab Crane, winch suppliers and any other suppliers as deemed appropriate. The old chassis along with the new appliance must be delivered to the Brigade. Note, all costs associated with this transportation of both the old and new appliances shall be borne by the supplier. 
	
	

	1.8
	1 No. set of Test Certificates shall be supplied in English with the appliance for the following:
a)	Proof of pre-delivery inspection, including confirmation of appliance road worthiness, by the chassis manufacturer;
b)	Test Certificates shall be provided as appropriate for any ancillary equipment supplied;
	
	

	1.9
	1 No. complete Operator Manual shall be supplied in English in both hard and soft copy with each appliance.
1 No. Maintenance Manual shall be supplied in English in both hard and soft copy with each appliance to include the following:
a)	Finished vehicle including the chassis;
b)	Detailed and complete Wiring Diagrams – all relays and fuses numbered and detailed on both the circuit diagram and on the appliance;
c)	Engineering Drawings of the appliance;
 
d)	User and Installation Manual for each electrical component;
e)	All ancillary systems and equipment supplied;
1 No. dossier must be supplied in English in both hard and soft copy with each appliance containing all relevant certificates and documentation pertaining to the commissioning, inspection and customer acceptance and/or final sign-off of the vehicle.
The above may be provided in both hard and electronic format. A label showing the registration number of the appliance shall be placed on the front of all manuals and soft data supplied.
	
	


[bookmark: _Toc471745508][bookmark: _Toc471814382][bookmark: _Toc471827365]


2. Chassis

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	2.1 
	A chassis must be proposed such that will fully comply with all items contained in this Section 2. 
Make, model & BHP of truck chassis proposed:,
Tenderers to fill in details Here:




	
	

	2.2 
	The total weight of the appliance with equipment and crew must be within the permitted axle loading and permissible total laden mass – details of equipment stowed can be provided on request.
	
	

	2.3 
	Right Hand Drive 4 X 2 Rear Wheel Drive
	
	

	2.4 
	The appliance must be minimum Euro 6 compliant.
	
	

	2.5 
	The appliance shall have an engine power output of not less than 320 BHP.
The appliance at the gross laden mass shall have a minimum top road speed of 120kph and shall reach the following speeds within the following timescales on a flat road;
•	65kph in less than 20 seconds
•	80kph in less than 30 seconds
•	100kph in less than 50 seconds
•	110kph in less than 65 seconds
•	120kph in less than 75 seconds

	
	

	2.6 
	A water scan kit shall be fitted (if non-standard with the chassis) to remove water / sediment in the fuel and shall have a warning light on the dash which shall alert the driver if the water level is too high in the fuel sediment bowl.
	
	

	2.7 
	The appliance speed limiter shall be set at 90kph and interlinked to the 999 lights such that the appliance cannot exceed the set speed limiter when the 999 lights are turned off. The appliance speed shall slow down back to 90kph each time the 999 lights are turned off if it is exceeding the legal limit when the 999 lights are turned off.
	
	

	2.8 
	The appliance must either:
Have no Tachograph installed, which results in no warning lights on the dash; or
The Appliance shall be fitted with a Tachograph simulator: A tachograph 1391 Siemens VDO interface (or equivalent). Please note that the 1391 Siemens VDO tachograph is not a standard type tachograph and for example does not accept driver cards.
	
	

	2.9 
	The appliance shall be fitted with a clutch-less fully automatic Allison Automatic Transmission (or equivalent) with Fully Automatic Integral Retarder.
The name and model of transmission must be detailed at Schedule B Specification. It shall only be possible to start the appliance in neutral with the handbrake on.
	
	

	2.10 
	The vehicle shall be fitted with LED Chassis Lights.
	
	

	2.11 
	The vehicle shall be fitted with Front Cornering Lights.
	
	

	2.12 
	A visual and audible alarm shall activate on the dash if the driver’s door is opened and the handbrake is released.
	
	

	2.13 
	The rear axle must have twin wheels. The appliance must be supplied with new Michelin XZE (or equivalent) tyres that are approved by the chassis manufacturer.
The name and model of the tyres must be detailed at Schedule B Specification.
Yellow Wheel Nut position indicators shall be fitted to all external wheels. A label stating the appropriate tyre pressure must be located on each wheel arch. It must be possible to easily check the tyre pressures of the inside tyres without removing the outside tyres. A new spare wheel and tyre must be supplied with the appliance (Note: the spare wheel and tyre must not be carried on the appliance).
	
	

	2.14 
	The appliance shall have Rear Air Suspension with a default to ride height on release of the handbrake.
	
	

	2.15 
	Electronic ABS must be fitted to the appliance.
	
	

	2.16 
	ASR Traction control must be fitted to the appliance.
	
	

	2.17 
	Advanced Emergency Braking shall be fitted with a facility to turn it off on the dash console.
	
	

	2.18 
	Lane Departure Warning shall be fitted with a facility to turn it off on the dash console.
	
	

	2.19 
	An electronic stability control system / programme shall be fitted to the appliance.
	
	

	2.20 
	An automatic Chassis Lubrication System must be fitted to the chassis to operate on a time phased basis when the appliance is turned on. Damage to one feed line must not render the system inoperable.
	
	

	2.21 
	The fuel tank, and any alterations, must be manufactured from a corrosion resistant material and must not encroach into the locker areas. An anti-spill device is to be located between the filler cap and the fuel tank. The fuel tank must have a minimum capacity of 130 litres.
	
	

	2.22 
	The air intake must be located at least 1.3m above ground level.
	
	

	2.23 
	The exhaust system must be manufactured from a corrosion resistant material. A low level exhaust must be high enough to not get caught on traffic calming measures when fully laden. Details shall be provided of the required location of the end of the exhaust system at the time of placing the official order. The transponder shall be removed from the existing chassis and shall be supplied by the Contracting Authority for fitting to individual appliances.
	
	

	2.24 
	Electric heated and electrically adjustable side mirrors must be provided on both sides of the vehicle.
A nearside Kerb Mirror and a Wide Angled Mirror located above the centre of the windscreen showing the ground area immediately in front of the full cab width must be fitted.
	
	

	2.25 
	Each door shall be fitted with a suitable strap to prevent the hinges being damaged in the event of wind or other suddenly forcing the door to a fully open position.
Central locking operated from a button on the dash shall be provided for all doors. Central locking shall automatically activate when the appliance speed exceeds 15kph.
	
	

	2.26 
	The vehicle shall be fitted with an Electro-pneumatic parking brake.
	
	

	2.27 
	The appliance must be equipped with two towing devices at both the front and rear, which will provide anchorage for winches and facilitate vehicle recovery. These devices shall be of sufficient strength to allow the vehicle to be towed on road at its permitted Total Laden Mass and no undue pressure shall be exerted on the chassis by these devices. A label shall be attached adjacent to each towing eye stating the capacity of each eye.
	
	

	2.28 
	Anti-Bandit windscreen glazing to be provided for both windscreen and side glazing. The appliance shall be fitted with electric windows for the driver and officer position.
	
	

	2.29 
	The appliance must be fitted with a cab visor with spotlights incorporated into the cab visor.
	
	

	2.30 
	The appliance must be fitted with side curtain airbags
	
	

	2.31 
	Automatically deployable snow chains must be fitted to the appliance. The chains must be easily removable from the deploying arm for care and maintenance. An easily accessible and identified isolation mechanism must be provided underneath the body to prevent accidental engagement of the snow chains.
	
	

	2.32 
	The chassis shall be fitted with a tyre pressure monitoring system that will alert the driver in the event of the tyre pressure being low in any tyre.
	
	

	2.33 
	All chassis preparation works (e.g. re-sighting air reservoirs etc.) shall be included. All chassis rails, crossmembers, air tanks, axles and suspension systems shall be sprayed with a polymerised bitumen coating (QLine 650B or equivalent). This coating shall provide corrosive protection from water contact and road salt. The tenderer shall ensure that all chassis rail arrangements, ancillary equipment etc. on the new chassis are suitable for remounting the body from the old chassis onto. Tenderers may inspect the existing bodywork at its current location – see 1.7 above.
	
	

	2.34 
	The chassis manufacturer shall approve any modifications made to the chassis.
	
	

	2.35 
	A Breakdown Triangle, a Dry Powder Fire Extinguisher and a First-Aid Kit shall be fitted in the drivers’ cab. A Hydraulic Jack Kit and a complete chassis toolkit shall be supplied with the appliance.
	
	

	2.36 
	1 Day Driver Familiarisation Training shall be delivered by the chassis supplier for up to 16 personnel at the station that the appliance will be based.
1 Day Mechanical and Electrical Maintenance training for 2 maintenance personnel shall be provided at the Brigade Headquarters.
The cost of the provision of the above training shall be borne by the supplier.
	
	





3. Cab

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	3.1 
	The cab shall be a new day cab. There shall be a bed area behind the front seats of minimum depth 500mm, this area shall be used for stowage of equipment and PPE.
	
	

	3.2 
	An Electro/Hydraulic Cab Tilt mechanism with a manual override must be fitted to the Cab. Full access must be provided to the engine and gearbox for maintenance.
	
	

	3.3 
	The drivers and officers seat shall be fully adjustable both fore and aft, for height and rake. The officer and driver seats shall have a leatherette finish. The seats shall have suitable head restraint included.
	
	

	3.4 
	Grab Handles shall be provided in yellow to assist with access / egress from all cab doors.
	
	

	3.5 
	Both seat positions shall be fitted with three point high-conspicuity seat belts.
	
	

	3.6 
	A seat belt warning device shall indicate which personnel are not wearing seat belts.
	
	

	3.7 
	A storage unit 400mm wide by 500mm deep by 250mm high with a lockable lid shall be provided for documents and small equipment between the driver and the officer seat. It shall be constructed of material and furnishings to blend in with the manufacturer’s crew cab.
In addition, suitable storage for 1 No. Fire-fighter helmet shall be provided in the cab.
	
	

	3.8 
	An adjustable Universal Tablet Holder with multi-angle adjustment for viewing shall be fitted in the offside front side of the crew cab.
	
	

	3.9 
	A Flexi Map Reading Light shall be fitted in the offside front side of the cab.
	
	

	3.10 
	An hour meter for engine running time shall be installed in the cab.
	
	

	3.11 
	A 24-hour vehicle powered digital clock visible to both the driver and the officer in daylight and darkness.
	
	

	3.12 
	A notice shall be fixed in the cab visible to the driver giving details of the height (highest point of cab/ ladders/mast etc.), width, length and gross laden mass of the appliance.
	
	

	3.13 
	All internal finishings shall be to a factory finish and any amendments to the interior of the cab shall be made good.
	
	

	3.14 
	All Cab Stepwells shall be fitted with Tread Kicker Plates to prevent paint damage from kicking. All Cab steps shall be painted with yellow high conspicuity non-slip paint.
	
	

	3.15 
	The appliance shall be registered by the tenderer.
1 no. reflective registration number plate shall be fixed to the front of each appliance and 1 no. reflective registration number plate shall be fixed to the rear of each appliance. A light shall be placed to illuminate each rear registration number plate. Details of the Local Authority that the appliances are to be registered to shall be provided when the official order is being placed.
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4. Body Construction and Design

	Item
	Description
	Complies
(Y/N)
	Comments/
Variations

	4
	Longford Fire & Rescue Service reserves the right to amend the design of the Body layout during the design phase of the build without incurring extra costs for redesign. 
	
	

	4.1 
	A new composite material body shall be built for the appliance.
The body frame and rear end panels of the bodywork shall have an aluminium edge striping of a minimum thickness of 3mm, and capable of taking a 25mm strip.
	
	

	4.2 
	The body design, shall be profiled to match the cab profile, including the provision of chassis side air deflectors to completely close the gap between the crew cab and the body. The finished body height mounted on the chassis shall be the same height as the cab.
	
	

	4.3 
	The body shall be mounted onto the chassis strictly in accordance with the chassis manufacturer’s guidelines
	
	

	4.4 
	The main body shall incorporate nine stowage lockers, four each side and one full width to the front to house 4 No Breathing Apparatus Sets or suitably designed retractable shelving to house RTC Cutting equipment etc. There will also be 3 stowage lockers at the rear of the appliance underneath the Hiab Crane for stowage of the rear winch and ancillary equipment.
	
	

	4.5 
	The overall height of the appliance shall be profiled to match the cab.
The minimum depth of all lockers shall be such that it will store a box 600mm deep but should maximise all available free space.
	
	

	4.6 
	The following section outlines the dimensions and requirements for the lockers.
	
	

	4.6.1
	The shutters shall have a strap fitted to the bottom of them hanging down to assist closing of the lockers when fully opened. 
Tenderers to fill in details Here:


	
	

	4.6.2
	The following new shelving shall be provided in the Nearside front locker:
3 No. Slide out Trays
1 No. Tilt and Slide Tray on top;
	
	

	4.6.3
	The following shelving from the current bodywork shall be removed from that appliance and re-fitted into the Nearside Front Locker No. 2 new bodywork:
a)	3 No. Slide out Trays
b)	1 No. Tilt and Slide Tray on top;
The current shelves shall be acid cleaned and polished. The roller mechanisms on the sliding trays will require replacement.
	
	

	4.6.4
	The following new shelving shall be provided in the Offside Locker No. 3 (note, due to the nature of equipment to be stowed in this locker, it shall be deeper than the other lockers on the nearside (the exact depth of this locker shall be determined at pre-build stage):
a)	1 No. Stainless Steel Floor shall be applied to the bottom of this locker to allow a HGV Platform to be stowed and easily slide in and out of this locker.
b)	A second stainless false floor shelf shall be fitted into this locker approximately 500mm above the stainless steel floor described in a) above (the exact height of this shelf shall be determined at pre-build stage)
c)	1 No. Tilt and Slide Tray on top;
	
	

	4.6.5
	The following new shelving shall be provided in the Nearside rear locker:
2 No. Slide out Trays;
1 No. Tilt and Slide Tray on top;

	
	

	4.6.6
	The following shelving from the current bodywork shall be removed from that appliance and re-fitted into the Offside Front Locker bodywork :
a)	3 No. Slide out Trays
b)	1 No. Tilt and Slide Tray on top;
The current shelves shall be acid cleaned and polished. The roller mechanisms on the sliding trays will require replacement.
	
	

	4.6.7
	The following shelving from the current bodywork shall be removed from that appliance and re-fitted into the Offside Locker No. 2 bodywork :
a)	3 No. Slide out Trays
b)	1 No. Tilt and Slide Tray on top;
The current shelves shall be acid cleaned and polished. The roller mechanisms on the sliding trays will require replacement.
	
	

	4.6.8
	The following new shelving shall be provided in the Offside locker No. 3 (note, due to the extra depth of the Offside Locker No. 3, it shall be shallower than the other lockers on the offside (the exact depth of this locker shall be determined at pre-build stage):
a)	2 No. Slide out Trays
b)	1 No. Tilt and Slide Tray on top;
	
	

	4.6.9
	The following new shelving shall be provided in the Nearside rear locker:
a)	2 No. Slide out Trays;
b)	1 No. Tilt and Slide Tray on top;
	
	

	4.6.10
	1 No. Full Body Depth Breathing Apparatus external stowage locker as follows;
a)	The stowage box shall be located between the front lockers and the crewcab
b)	The stowage box shall continue the profile height of the remainder of the bodywork and blend in with chassis side air deflectors
c)	The locker shall have suitable sliding cradles included for the stowage of 4 No. BA Sets
d)	The cradles shall slide out of the locker (2 on the nearside and 2 on the offside) and shall allow for the height of the BA set to be adjusted (raised / lowered) while stowed on the cradle to allow the operator to don the BA set at a suitable height for them before releasing the BA set from the stowage cradle
 
e)	The space underneath where the BA sets are stowed shall also be full depth but may be narrower to accommodate air tanks / diesel tanks etc. on the chassis
f)	The locker shall have access doors fitted to the nearside and offside of the locker. There shall be either 1 profiled door each side of the locker or else a wider top door and narrower lower door to each side of the locker. Each door shall be fitted with 2 no. quick release locks and with sensors that will alert the driver in the event of the doors not being fully closed
g)	LED white strip lighting shall be provided in the locker and operate in the same manner as the other locker lights
h)	The provision of this locker should not impinge on the width of other lockers
	
	

	4.6.11
	There shall be 3 No. Stowage Lockers at the rear of the appliance in the space underneath the Hiab Crane. The lockers shall maximise use of all free space. The bottom of these lockers shall be at the same height as the bottom of all other side lockers. The middle of these 3 locker shall be used to accommodate the rear winch (see Section 7.2 below). The lockers at either side of the winch shall be the same height as the winch locker and shall be used to stow all winch and hiab crane ancillary equipment including winches, shackles, chains etc. and will be required to be structurally adequate to stow heavy equipment.
a)	The 3 lockers shall have access doors fitted. Each door shall be fitted with 2 no. quick release locks and with sensors that will alert the driver in the event of the doors not being fully closed
b)	LED white strip lighting shall be provided in the locker and operate in the same manner as the other locker lights
c)	The finished lockers shall be painted red to match the colouring of the remainder of the appliance
	
	

	4.6.12
	All sliding trays and cradles shall have automatic locking in the ‘IN’ and ‘OUT’ position.
	
	

	4.6.13
	All new bottom shelves shall have a minimum capacity of 150Kgs. The height of any individual shelf (apart from the bottom shelves) shall be easily adjustable.
All shelves shall be of peg board construction.
High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) yellow reflective tape shall be placed on the front of all shelves. High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) yellow reflective tape shall be placed on the side of all cradles, sliding and tilt and slide shelves that protrude more than 25mm outside the vehicle bodyline.
The name and model of the reflective tape must detailed at Schedule B Specification.
	
	

	4.6.14
	8 No. Aluminium Lift-Out Stowage Box, approximate dimensions (will vary depending on shelf size) 230mm high x 600mm Deep x 600mm wide. Stowage Boxes shall have one lifting handle cut out of each side of the box with an edge strip placed around the cut out. These stowage boxes shall have holes punched out in a patterned fashion to reduce the weight of them.
	
	

	4.6.15
	8 No. RTC Tool kits shall be supplied with the appliance for stowage of Battery operated RTC Tools (subject to Longford Fire & Rescue Service details at design stage).
	
	

	4.7 
	‘Cat’s Whiskers’ shall be fitted to the wheel arches for spray suppression. Mud Flaps shall be fitted behind the rear wheels for spray suppression. All free space in the wheel arches shall be converted into locker stowage There shall be a capability of stowing one BA cylinder either side of the rear wheel on both sides of the appliance (total 4). The lockers shall have access doors fitted. There shall be either 1 profiled door each side of the wheel arches or else a wider top door and narrower lower door to each side of the locker. Each door shall be fitted with 2 no. quick release locks and with sensors that will alert the driver in the event of the doors not being fully closed.
	
	

	4.8.1
	Roof access ladder support brackets to be fitted to the nearside of the appliance.
	
	

	4.8.2
	Anti-slip adhesive tape shall be placed on the roof of the body of the appliance in any areas where an operator could potentially walk.
	
	

	4.8.3
	1 No. rated Safety Harness anchor point on the roof
	
	

	4.9
	The manufacturer shall visit the station on delivery of the appliance and shall securely fit all Brigade RTC hydraulic equipment and all other equipment on the appliance using a combination of straps and bollards – tenderers can assess what equipment is to be secured when inspecting the current appliance at tender stage.
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5 Paint & Conspicuity Markings

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	
	All conspicuity markings must conform to ECE 104 (or equivalent) Standard. 

	
	

	5.1
	The appliance, including the bodywork header panels, front grille closure, the step well areas, diesel tank, the winch frame, BA Stowage locker and the 3 rear stowage lockers shall be painted in Red to BS 381C-538 (or equivalent) applied in a wet effect finish.
	
	

	5.2
	All metal fabrications must be thoroughly degreased.
	
	

	5.3
	The area between the windscreen and the grill shall have a High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow Reflective Strip with the wording FIRE (forward and reversed) on top of the 150mm Reflective Yellow Strip in Red Writing. The Chassis badge name shall be painted in red as appropriate to match the appliance colour. 25mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow Reflective Strips shall be placed on the grill bars on the front of the appliance.
	
	

	5.4
	The existing hi-visibility striping on the appliance lockers shall be removed and new High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow and Red Day-Glo Reflective Battenburg Pattern shall be applied to both sides of the appliance. The Battenburg pattern shall be applied to the crew cab to blend in with the cab contours whilst maintaining the overall profile of the Battenburg pattern along the full length of the appliance. Individual squares in the Battenburg pattern shall measure between 700mm and 900mm square.
150mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Reflective Yellow strips shall be positioned along the length of the Header Panel overhead the lockers on either side of the appliance. The name of the Brigade shall be applied in English on the nearside header panel and in Irish on the offside header panel in red writing – the wording for the name of the Brigade in English and Irish shall be supplied at the time of placing the official order for the appliance.
	
	

	5.5
	100mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Reflective strips in inverted V style shall be applied.
	
	

	5.6
	A 1” High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) silver reflective strip shall be placed around the outer profile of the bodywork on both sides of the appliance to provide additional conspicuity for the appliance when lockers are opened.
	
	

	5.7
	A 1” Diamond Grade (or equivalent) yellow reflective strip shall be placed around the outer edge of all sliding and tilting trays, shelves and cradles to provide additional conspicuity for the appliance when trays, shelves and cradles are opened.
	
	

	5.8
	A High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) yellow reflective strip shall be placed on each side of the Winch Frame to provide additional conspicuity for the appliance.
	
	

	5.9
	Brigade Crest Transfers shall be placed on either side of the appliance – the digital file for printing the transfers shall be supplied by the Brigade when placing the official order.
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6 Electrical Systems

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	6.1 
	All electrical wiring shall be of adequate gauge and insulation for the designed load, and where exposed shall be waterproof and corrosion free.
All electrical wiring shall be suitably protected from damage and from the elements. All electrical wires and small air pipes shall be run in conduit within the bodywork. The conduit shall be fixed to the bodywork, easily accessible for maintenance and remain in place for the life span of the appliance.
All important electrical circuits shall have separate circuit breakers, suitably indicated and grouped into a common box located in an accessible position within the cab.
	
	

	6.2 
	The electrical system shall be 24V negative earth with 2 no. 180 amp hour heavy-duty maintenance free batteries in series fitted in an accessible position.
	
	

	6.3 
	LED lighting of the cab doors and steps to aid access/egress shall illuminate automatically when the corresponding door is opened.
Red LED strip lighting shall be provided on the edge of the doors to increase the conspicuity of the doors when they are opened at night-time. The LED strip shall illuminate automatically on a particular door if that door is opened when the sidelights are turned on.
	
	

	6.4 
	A new Low Profile full width Blue Light bar shall be fitted on the roof of the cab that is visible to oncoming traffic containing the following:
LED in a rotation pattern at either end of the light bar;
4 No. Independent forward and rear facing LED alternating flashing lights, two either side of the centre of the Light bar;
Alley lights on either side of the Light bar;

The name and model of the Light Bar must be detailed at Schedule B Specification.
Make & model of Light Bar proposed:
Tenderers to fill in details Here:


	
	

	6.5 
	The existing remote electronic siren shall be removed from the old chassis and re-fitted to the new chassis.
Tenderers to fill in details Here:


	
	

	6.6 
	The existing air operated two tone horns shall be removed from the existing chassis and shall be re-fitted to the new chassis along with all ancillary switching. The horns shall be re-fitted in a location behind the front grille in an area that does not affect their effectiveness in the new chassis.
	
	

	6.7 
	2 No. new White alternating LED’s shall be fitted to the front of the appliance which when switched on will only function when:
the handbrake is off;
the vehicle lights are off;
	
	

	6.8 
	New LED Blue alternate flashing lights shall be fitted as follows:
a)	2 No. on both sides of the appliance (these lights shall be removed from the current appliance and fitted to the new bodywork);
b)	2 No. on the rear of the appliance;
c)	2 No. Blue RSG (or equivalent) alternate flashing intersector lights on each side of the number plate mount
d)	2 No. new Blue alternating LED’s on the front of the applianceMake & model of LED Blue Lights proposed:
Tenderers to fill in details Here:


	
	

	6.9 
	LED Scene Lights shall be fitted as follows:
The existing 2 No. Scene Lights on each side of the current appliance shall be removed and fitted to the new bodywork;
2 No. new LED Scene lights shall be fitted on the rear of the appliance (note, these 2 No. rear scene lights should also automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected);
1 No. fitted overhead the winch;

Scene lights shall be interlocked with the handbrake so that they automatically switch off when the handbrake is released. Manual operation of the scene light shall be possible at speeds less than 20kph. There shall be a facility to switch on the LED Scene lights from the pump bay.
The name and model of the LED Scene Lights must be detailed at Schedule B Specification.
Make & model of scene light proposed:
Tenderers to fill in details Here:


	
	

	6.10 
	Circular orange LED Marker Lights shall be fitted to the pillars in between each locker at mid-height.
	
	

	6.11 
	The Woodway Nightowl light-mast on the existing appliance shall be removed and re-fitted to the new chassis including all mechanical and electrical requirements. The light mast shall be interlocked to the handbrake. A light shall illuminate on the dash when the light mast is engaged.
	
	

	6.12 
	A new Night Vision Reversing Camera shall be mounted on the rear of the appliance with a flat screen colour display located on the dash. The display shall be at the same eye-line height as the appliance mirrors and shall not interfere with the drivers view and the camera shall automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected. There shall be a manual override facility to leave the camera switched on permanently also.
	
	

	6.13 
	A new Reversing Proximity Sensor with an audible alert shall be fitted in the dash.
An Audible Alarm warning that the vehicle is reversing shall be fitted. A Facility to turn off this alarm shall be fitted on the dash. The switch shall be reset once the appliance is switched off.
Low Level Rear light clusters shall be LED and repeated at roof level and all rear lights shall be flush mounted.
	
	

	6.14 
	New White LED strip lighting shall be provided in both frames on either side of all stowage lockers the full height of the frames. Locker lights shall automatically switch on in a particular locker when that locker is opened if the sidelights are turned on.
	
	

	6.15 
	An Electronic Management System shall be fitted with the following characteristics;
•	The programming of various patterns shall be included
•	Diagnostics shall be displayed / controlled by a suitably sized, installed display screen in the cab or by auxiliary switches. The display screen shall be suitably backlit / the auxiliary switches shall be illuminated which shall be linked to switching on the side lights of the appliance.
•	The System is to be compatible with hand held diagnostic devices.
•	The System BUS communication architecture to be standard automotive cable (no twisted wires or screened cable required).
•	The System must monitor dual voltage levels.
•	The System must monitor internal or external temperature.
•	The System must be capable of Dual event monitoring, logging and flagging of any system input or output.
•	The System must be expandable by means of easy to update Boolean logic.
•	The System must have the ability to integrate with third party peripheral devices via RS232 communication.
•	The System must have the ability to integrate with third party peripheral devices via RS232 communication.
•	An accessory load management system shall be included to isolate circuits should the vehicle not be generating sufficient power to run the accessories, without using battery power. The system shall reintroduce the accessories, automatically, when power is available. The system shall not interfere with the standard vehicle equipment required for road driving.
•	A suitable Training course must be available for all aspects of software and hardware with certification from ISO9001 – 2015 provider for Brigade Maintenance personnel (or equivalent)
•	The Hardware must be CE marked for automotive use 2004/104/EC.

The name and model of the Electronics Management System must be detailed at Schedule B Specification.
Make & model of Electronics Management System proposed:
Tenderers to fill in details Here:
	
	

	6.16 
	Switching shall be centrally located on the dash to perform pre-programmed Audio / Visual warning patterns such as ‘999’ and ‘In Attendance’ and to individually control all blue lights, scene lights, etc.
 
The programming of various patterns shall be included. Illumination of all auxiliary switches shall be incorporated into the vehicle sidelights switch.
Make & model of Electronics Management System proposed:
Tenderers to fill in details Here:


	
	

	6.17 
	The 220 Volt input socket with an Auto-Eject System shall be removed from the current appliance and fitted to the appliance to keep the batteries automatically charged in situ.
The supply voltage shall be specified at the time of placing the official order.
	
	

	6.18 
	The 220V Top-Up compressor complete with wiring and socket shall be removed from the existing appliance and fitted to the new appliance.
	
	

	6.19 
	An Auxiliary Battery Charging device, Antares Assured Start (or equivalent) shall be fitted to the appliance to allow the appliance to start even in the event of flat chassis batteries. The auxiliary battery can temporarily connect to the main chassis batteries when activated through a dash mounted button, providing enough combined battery power to start the vehicle.
	
	

	6.20 
	A Run lock and Keyless running facility shall be fitted where available from the chassis supplier. Where not provided by the chassis supplier, the supplier shall retrofit an electronic solution to provide a keyless running solution.
	
	

	6.21 
	Accidental turning off, of the master switch when the appliance is moving should not turn off the appliance and should not affect the driving of the appliance. A time delay (duration to be recommended by the chassis supplier) shall be fitted to the Master Switch.
	
	

	6.22 
	The following sockets shall be provided with the vehicle;
· 2 No. High Quality Marine Specification 12 V Charging points in the cab.
· 2 No. USB charging sockets in the cab
· 2 No. USB-C charging sockets in the cab
· 2 No. USB in the equipment compartment in the rear (including fused wiring).

	
	

	6.23 
	If possible, the Aerial Bases shall be removed from the existing appliance and fitted by the tenderer on the new chassis to the ground plate.
	
	

	6.24 
	Warning lights with an audible device shall be mounted on the dash to indicate the following:
a)	Locker open (for each locker door);
b)	Cab door open;
c)	Mast elevated;
d)	What seat belts are not in use
e)	When snow chains are deployed
	
	

	6.25 
	The supplier shall arrange for a third party approved supplier to supply and fit all necessary Tetra Hardware to the appliance other than the radio base (the radio base will be provided Free Issue by the Fire Authority). This shall include the supply and fitting of all Control Heads, Microphone Heads, Speakers, Antennas, all necessary cabling, brackets, clips and pump bay kits. The current C Trí approved third parties are Tetra Ireland and Sigma Wireless. In addition
a)	The supplier shall run a wiring loom from the agreed location of the radio to the agreed location of the control head
b)	The supplier shall run a wiring loom from the agreed location of the radio to the agreed location of the Pump Bay Voice Terminal in the pump Bay
c)	The supplier shall run a wiring loom from the agreed location of the radio to the agreed location of the aerials (Tetra & GPS)
d)	The supplier shall provide a 12V DC supply at the agreed location of the radio
Note, the supplier shall be responsible for all costs associated with the above items in this Section, including payment to the Third Party Supplier.
	
	

	6.26 
	1 No. Standalone 2.5KvA generator capable of delivering both 110V and 220V shall be supplied with the appliance.
Tenderers must state the name, and model of the 2.5KvA Generator in the required field at Schedule B Specification.
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7. Winches

	Item
	Description
	Complies
(Y/N)
	Comments/
Variations

	7.1 
	1 No. front-mounted electric winch, capable of hauling a minimum of 5 Tonnes, complete with wander lead and remote control shall be mounted on the front of the appliance. A free spool facility shall be fitted to the winch. The winch shall be mounted such that it will not encroach into the approach angle. The winch shall be mounted in an easily accessible location for maintenance, and it shall be easy to reach the free spool switch. The winch shall be fitted with a certified rope. A red leatherette cover shall be provided for the winch with suitable fastenings. A test certificate for the winch mounting, SWL, winch cut off and rope shall be supplied at the time of delivery of the appliance. Emergency Stop Isolation Buttons for the winch shall be fitted inside the winch supporting frame either side of the winch. A suitable light shall be fitted over the front winch position to operate on activation of the winch.
A heavy-duty manual pulley shall be supplied with the winch to increase pulling capacity to 10 Tonnes.
The name and model of the winch and heavy-duty pulley must be detailed at Schedule B Specification.Make & model of PTO proposed:
Tenderers to fill in details Here:


	
	

	7.2 
	1 No. front-mounted electric winch, capable of hauling a minimum of 5 Tonnes, complete with wander lead and remote control shall be mounted in the mid stowage lockers underneath the Hiab Crane in the rear of the appliance. A free spool facility shall be fitted to the winch. The winch shall be mounted such that it will not encroach into the approach angle. The winch shall be mounted in an easily accessible location for maintenance, and it shall be easy to reach the free spool switch. The winch shall be fitted with a certified rope. A test certificate for the winch mounting, SWL, winch cut off and rope shall be supplied at the time of delivery of the appliance. Emergency Stop Isolation Buttons for the winch shall be fitted in a suitable easily accessible location either side of the winch.
A heavy-duty manual pulley shall be supplied with the winch to increase pulling capacity to 10 Tonnes.
a) The name and model of the winch and heavy-duty pulley must be detailed at Schedule B Specification.

Make & model of Pump proposed:
Tenderers to fill in details Here:


	
	





8. HIAB Crane

	Item

	Description
	Complies
(Y/N)
	Comments/
Variations

	8.1 
	The PTO on the current appliance shall be removed and re-fitted to the new appliance. The supplier shall ensure the current PTO is compatible with the gearbox on the new Chassis. Any moving part of the PTO shall be guarded against contact by the operator during use.
 
The PTO shall be interlocked to the handbrake. A light shall illuminate on the dash when the PTO is engaged.
	
	

	8.2 
	The Hiab Crane on the existing chassis, along with all ancillary equipment such as hydraulic oil tanks etc. shall be removed and re-mounted onto the new chassis. The existing crane shall be completely re-furbished as deemed appropriate and shall include the following works at a minimum, along with any other works deemed appropriate;

•	Repainting of all Boom, Frame, all metal exposed parts and Jack Beams
•	Full Service of the Hiab and Test Certificates for same
•	Replacement of all Decals with new ones
•	Replacement of all Hi-Visibility Markings on the Jack Legs
•	Safety mechanism to prevent overloading of the crane / winch
All of the these works must be completed by a Hiab approved service agent (current service provider is Cahir House Machinery).
	
	

	
	
	
	


9. [bookmark: _Toc471827372]Spare Parts, Warranties and Delivery

	Item

	Description
	Complies
(Y/N)
	Comments/
Variations

	9.1
	It is a requirement that the bodywork must have a minimum of 15 Years Warranty.
The Tenderer must supply evidence and confirmation of compliance with this requirement at Schedule B Specification.
	
	

	9.2
	It is a requirement that all other parts of the appliance (including ancillary equipment) other than the chassis must have a minimum of 2 years warranty.
The Tenderer must supply evidence and confirmation of compliance with this requirement at Schedule B Specification.
	
	

	9.3
	It is a requirement that the chassis vehicle systems and driveline must have a minimum of 2 years warranty (other than standard serviceable items).
The Tenderer must supply evidence and confirmation of compliance with this requirement at Schedule B Specification.
	
	

	9.4
	Spare Parts and Technical Assistance shall be available for a minimum of 15 years for the appliance and all ancillary equipment. Suppliers should have a network of support throughout the Republic of Ireland for both chassis and fire engineering support including trained technical personnel based in the Republic of Ireland and appropriate transport for these personnel and spare parts. A complete stock of all commonly used spare parts should be available at a store in the Republic of Ireland.
Suppliers should have the ability to have a trained technical person present at any Fire Station throughout the Republic of Ireland within 12 hours from receipt of call-out.
	
	

	9.5
	Tenderers must state their delivery lead time (in weeks) for a complete solution for each chassis option.
The lead time shall be taken as the period from the date of the official order placement to the delivery on station of a fully approved appliance.
State the delivery lead times (in weeks) at Schedule B Specification.
	
	




Award Criteria 2 – Experience & Qualifications of Staff
	Criterion 2:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Experience & Qualifications of Staff
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must provide details and examples of the relevant qualifications and experience of its employees engaged in the build/assembly of Class B Water Tender, Emergency Tender, Aerial Appliance, Water Tanker or Incident Command Unit, and also of any subcontractors engaged in the process.
Include details of the number of
i. technicians/mechanics employed and their qualifications; 
ii. their experience building fire appliances;
iii. ongoing training/upskilling; and any other information which demonstrates that its staff have the requisite skills and experience. 

	Tenderers’ Response

















[bookmark: _Hlk217996479]Award Criterion 3 – Aftersales Support & Technical Assistance 
	Criterion 3:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Aftersales & Technical Assistance 
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must set out the quality of its proposal in relation to its capacity and capability for the provision of maintenance, repair and technical assistance from its workshop facilities, and its capacity and capability for      repair/maintenance services on-site at Longford County Council. Tenderers must provide details of workshops, if any, they have in the Republic of Ireland to carry out both chassis and Fire Engineering repairs. The Tenderer should also provide details of the process by which clients’ repair issues are managed from the time a fault is reported through to   successful conclusion. If sub-contracting after sales support to another supplier, full details must be provided of that sub-contractor, including their workshop details (for both chassis and Fire Engineering repairs), network details, technical capabilities of their employees in relation to fire-engineering support and their qualifications for same, and details of stock they carry and where the stock is located.


	Tenderers’ Response











Award Criterion 4 – Availability of Spare Parts
	Criterion 4:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Availability of Spare Parts 
	
	
	

	
	10%
	100
	60

	Instructions
	
The Tenderer must set out the quality of its proposal for ensuring the availability of all spare parts for the appliance and ancillary equipment for the minimum expected lifespan of the vehicle (15 years). 
The Tenderer should include details of its process and lead times for obtaining spare parts; how it manages this supply chain to ensure parts are delivered on time; and how it manages instances of order delays and parts being out-of-stock.


	Tenderers’ Response
















Award Criterion 5 – Ordering & Delivery
	Criterion 5:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Ordering & Delivery  
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative demonstrating its high-level process and timescales for the successful delivery of a Emergency Tender - from the time of the official order through to full commissioning and handover of the appliance.
The Tenderer should Include details of the tenderer’s methodology for ensuring that all appliances are supplied and delivered in accordance with the requirements specified by the client.


	Tenderers’ Response

















Award Criterion 6 – Environmental & Sustainability Efficiencies
	Criterion 6:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Environmental & Sustainability Efficiencies 
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative to demonstrate how it incorporates environmental and sustainability efficiencies/measures during the build   process. For example:
· Energy optimisation initiatives in the              warehouse/premises including rain harvesting, use of PV Panels, fabric of the building including insulation, efficiency of lighting and heating, EV charging capabilities etc.
· Use of recycled and/or recyclable material
· Waste management/disposal/recycling
· Minimisation of waste
· Transport and logistics measures
· Corporate Social Responsibility policies
· Proposed Targets for Environmental Sustainability
· Sustainable purchasing


	Tenderers’ Response













Award Criterion 7  – Cost
	Criterion 7:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Cost  
	
	
	

	
	60%
	600
	N/A

	Instructions
	
The Tenderer must give the total cost, in Euros , of the vehicle as specified in Appendix 1
· Including delivery to Longford
· Including all expenses/ tariffs/ custom charges
· Excluding VAT 



	Total Cost  ( ex. VAT )
	€



I/We confirm that I/we: 

1. Will keep this offer for the contract open for acceptance by you for a period of 12 months from the date of deadline for submission of Tenders,
2. Agree that you are not bound to accept the most economically advantageous or any Tender you may receive,
3. Have read and thoroughly examined the Tender Document,
4. Fully understand the Tender Document and the Client’s requirements,
5. Undertake to treat the details of this Invitation to Tender, its Tender and any subsequent agreements as private and confidential,
6. Acknowledge that acceptance by the Contracting Authority of this tender will not constitute a binding and enforceable agreement and that a legally enforceable agreement will not exist until and unless the contract is awarded between the Contracting Authority and the Tenderer,
7. Have availed of all offers for additional information or have otherwise satisfied myself/ourselves as to conditions that may in any manner affect the performance of the contract,
8. Have included all elements necessary for the performance of the specified requirements, which are either expressly stated in the Tender Document or contained in any supplementary information or which could reasonably be inferred therefrom,
9. Have found no errors, omissions, conflicts or ambiguities in the Tender Document except those which I/We have brought to the attention of the Contracting Authority before the latest date for submitting queries,
10. Have included for compliance with all statutory requirements applicable in Ireland and those applicable in any country where parts of the contract may be performed that are in force 7 days prior to the deadline for receipt of Tenders, 
11. Will not, if awarded a contract employ labour in a manner that is discriminatory in relation to gender, civil/family status, sexual orientation, religion, age, disability, race, or membership of the traveller community.
12. [bookmark: _Hlk491592638]Agree that as a condition of award, it shall be our sole responsibility to fulfil the obligations under the Contract, notwithstanding any changes in circulars, laws, regulations, taxation, duties or other factors which might arise following the withdrawal of the United Kingdom from membership of the EU.
	Signed:
	

	Name (in Capital Letters):
	

	On behalf of:	
	

	Address:
	

	Telephone:
	
	Mobile:
	

	Email:
	
	Date:
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