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[bookmark: _Toc227064010]Instructions for Completion
Tenderers should ensure they have read the Request for Tender before they attempt to complete this Tender Response Document.  
If you consider that the Tender Response Document is missing any sections which would prevent you from preparing a comprehensive response, please contact the Contracting Authority as soon as possible.     
Where there is a discrepancy between the contents / instructions in this document and the Request for Tender, the Request for Tender will take precedence.   
Tenderers must follow the instructions contained in this document in relation to attachments, format for submission, etc.  

[bookmark: _Hlk495513867]Where tenderers are relying on other parties to meet the selection criteria, those parties must be available to deliver elements of the contract. 


[bookmark: _Toc227064011]RESPONSE TO SELECTION CRITERIA


TENDERERS SHOULD NOTE THESE CRITERIA ARE ASSESSED ON A PASS/FAIL BASIS


[bookmark: _Toc488834418][bookmark: _Toc227064012]General Contact Information
	Organisation Name:
	

	Contact Person:
	

	Position: 
	

	Address: 
	

	Phone:
	

	Email: 
	

	Website: 
	

	Date of Establishment, if applicable
	VAT Registration No:
	Legal Structure – partnership, limited company, etc.

	
	
	

	Details of any sub-contractors or consortium members: 

	Name
	Proposed Role in Delivery of the Contract
	Confirmation relevant information is provided for each party (e.g. financial, experience, or other selection criterion where applicable)  

	
	
	

	
	
	

	
	
	


[bookmark: _Toc227064013]Financial Information – Pass/Fail Criteria
	
Tax Clearance
	Please confirm YES/NO

	I confirm and declare being tax compliant.  The Contracting Authority can verify your tax clearance status through Revenue’s online facility at http://www.revenue.ie/en/online/tax-clearance.html  To this end, please confirm:
	Yes
	

	(A) 
	No
	

	Tenderer Name:
	

	Tenderer PPSN/ Tax Reference Number
	

	Access Number
	

	OR I confirm that I hold a current valid paper Tax Clearance Certificate (generally relates to Non-Residents)

	Registration Number
	
	Certificate Number
	

	OR, 
I confirm that I have applied for Tax Clearance status or a Tax Clearance Certificate which will be made available on request
	Yes
	

	
	No
	

	Turnover

	I confirm that we have the requisite turnover to be considered for the contract/framework.

	Year
	2025
	2024
	2023

	Month End (e.g. July)

	
	
	

	Turnover €
	

	
	

	I confirm that I will provide evidence of turnover promptly on request.
NOTE #1:  In the case of sole traders or partnerships this condition may be satisfied by a letter of confirmation from a senior partner.

	Yes
	

	
	No
	




	Insurances

	I confirm that we have the following insurances in place and are authorised for the  jurisdiction of the Republic of Ireland.

	Insurance Type
	Level required if successful
	Level in Place
	Details of Any Excess
	Renewal Date

	Employers Liability
	€13,000,000
	€
	
	

	Public Liability
	€6,500,000
	€
	
	

	Product Liability
	€6,500,000
	€
	
	

	Professional Indemnity 
	€1,000,000
	€
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	AND

	I confirm that if successful, where the levels required under the contract/framework are higher than those currently in our possession, I will be in a position to put the required forms and levels of insurances required in place. 
	

	AND
	

	I confirm that I will provide the following promptly on request:
· evidence of insurances in place      or
· letter from Insurance Broker confirming that the required levels can be put in place if successful 
	














[bookmark: _Toc227064014]Declaration Re Personal Circumstances – Pass/Fail Criteria
	DECLARATION RE PERSONAL CIRCUMSTANCES AS PER ART. 57 OF DIRECTIVE 2014/24/EU

Economic Operators will be excluded from the procurement process if, within the past five (5) years, there is evidence of a conviction relating to a specific criminal offence listed below (see 1.1) or if they have been the subject of a binding legal decision which found a breach of legal obligations to pay tax or social security contributions (see 1.2) (except where this is disproportionate e.g. where only minor amounts are involved).

	1.1 Has the Economic Operator or a member of their proposed consortium, (if applicable), Director, or Partner or any other person who has powers of representation, decision or control, been convicted of any of the following offences?
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box 

	1.1.a
	participation in a criminal organisation, as defined in Article 2 of Council Framework decision 2008/841/JHA;
	
	

	1.1.b
	corruption, as defined in Article 3 of the Convention on the fight against corruption involving officials of the European Communities or officials of Member States of the European Union and Article 2(1) of Council Framework Decision 2003/568/JHA as well as corruption as defined in Irish Law or the jurisdiction in which the Economic Operator is established;
	
	

	1.1.c
	fraud within the meaning of Article 1 of the Convention on the protection of the European Communities’ financial interests;
	
	

	1.1.d
	the subject of a conviction for terrorist offences or offences linked to terrorist activities or for inciting or aiding or abetting or attempting to commit an offence;
	
	

	1.1.e
	the subject of a conviction for money laundering or terrorist financing; 
	
	

	1.1.f
	the subject of a conviction of child labour and other forms of trafficking in human beings;
	
	

	Non-payment of taxes or social security obligations
1.2 Has it been established by a judicial or administrative decision having final and binding effect in accordance with Irish law or the legal provisions of the country in which the Economic Operator is established (if outside Ireland), that the Economic Operator is in breach of obligations related to the payment of tax and social security contributions?
Note: If the response to 1.2 above is in the affirmative, please provide further information on the decision and the amounts involved
	
	



	2.1 Please indicate if any of the following situations have applied, within the past three (3) years, or currently apply, to your organisation.
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box

	2.1.a
	has, in the performance of any public contract, failed to comply with applicable obligations in the field of environmental, social and labour law applying at the place where the works were carried out or the services provided, as established by EU law, national law, collective agreements or by international, environmental, social and labour law listed in Annex X of Directive 2014/24/EU;
	
	

	2.1.b
	is bankrupt or the subject of insolvency or winding-up proceedings, its assets are being administered by a liquidator or by the court, or has entered into an arrangement with creditors, suspended its business activities or is in any analogous situation arising from a similar procedure under national laws and regulations;  
	
	

	2.1.c
	is guilty of grave professional misconduct which renders its integrity questionable;
	
	

	2.1.d
	has entered into agreements with other economic operators aimed at distorting competition;
	
	

	2.1.e 
	has a conflict of interest within the meaning of Article 24 of 2014/24/EU that cannot be effectively remedied by other, less intrusive, measures; 
	
	

	2.1.f 
	confirms that it has had prior involvement in the preparation of the procurement procedure which has resulted in a distortion of competition, as referred to in Article 41 of 2014/24/EU, that cannot be remedied by other, less intrusive, measures;
	
	

	2.1.g
	has shown significant or persistent deficiencies in the performance of a substantive requirement under a prior public contract, a prior contract with a contracting entity, or a prior concession contract, which led to early termination of that prior contract, damages or other comparable sanctions. 
	
	

	2.1.h
	· is guilty of serious misrepresentation in supplying the information required for the verification of the absence of grounds for exclusion or the fulfilment of the selection criteria; or
	
	

	
	· has withheld such information or is not able to submit supporting documents required under Article 59 of Directive 2014/24/EU; or 
	
	

	2.1.i
	has undertaken to:
· unduly influence the decision-making process of the contracting entity, obtain confidential information that may confer upon the Tenderer undue advantages in the procurement procedure; or
· negligently provide misleading information that may have a material influence on decisions concerning exclusion, selection or award.
	
	


[bookmark: _Toc487559492]

[bookmark: _Toc227064015]Declaration Re Statutory Obligations – Pass/Fail Criteria
	We confirm that we are fully compliant with the following legislation, or equivalent legislation in our country of establishment/operation:
	YES
	NO

	(a) 
	Employment Equality Acts 1998-2011 
	
	

	(b) 
	Equal Status Acts 2000-2011
	
	

	(c) 
	National Minimum Wage Act 2000 as amended 
	
	

	(d) 
	Organisation of Working Time Act 1997 as amended
	
	

	(e) 
	Safety, Health and Welfare at Work Act 2005 and Safety, Health and Welfare at Work (General Application) Regulations 2007
	
	

	(f) 
	Disability Act 2005
	
	

	(g) 
	We have procedures in place to ensure that our subcontractors, if any are used for this contract, apply the same standards.
	
	

	This Declaration is made for the benefit of the Contracting Authority 
I certify that the information provided in the Declaration re Personal Circumstances and the Declaration re Statutory Obligations is accurate and complete to the best of my knowledge and belief.  I understand that the provision of inaccurate or misleading information in these Declarations will lead to my organisation being excluded from participation in this and future tenders and I am signing on behalf of: 


	Name of Tenderer
	


	Name of Authorised Signatory
	


	Position

	

	Signature

	










[bookmark: _Toc227064016]Manpower Levels – Pass/Fail Criteria
	Skillset Required
	Full Time Equivalent (FTE)
Numbers in Tendering Entity
	FTEs provided via 3rd Parties
	Minimum Number Required

	Maintenance Personnel for service & repair of  Battery operated RTC tools  
	2 personnel 
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	Please attach an organisation chart, clearly identifying all relevant departments, divisions, and 3rd parties, if applicable.

	Organisation Chart Attached 
	Yes
	
	No
	




[bookmark: _Toc227064017]Technical Resources – Pass/Fail Criteria
	Resource Required
	Minimum Level
	Tenderer’s Response


	Workshop, Garage Equipment & Electronics Equipment to Maintain and repair Battery Operated RTC tools   
	Adequate Workshop, Garage Equipment & Electronics Equipment to Maintain and repair Battery Operated RTC tools   
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	





[bookmark: _Toc227064018]Previous Contracts
	Reference Contract #1

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	Fit out of storage, shelving, electrical installation and vehicle Markings to fire service or similar work vehicles   
	

	
	

	
	

	
	

	Any other relevant information 

	

	Reference Contract #2

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	Fit out of storage, shelving, electrical installation and vehicle Markings to fire service or similar work vehicles   
	

	
	

	
	

	
	

	Any other relevant information 

	


	Reference Contract #3

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	Fit out of storage, shelving, electrical installation and vehicle Markings to fire service or similar work vehicles   
	

	
	

	
	

	
	

	Any other relevant information 


[bookmark: _Toc227064019]Health & Safety
	Do you comply with the Safety Health & Welfare at Work Act 2005 
	Yes
	
	No
	

	Name of Manager responsible for Health and Safety 
	

	Is it 3rd party certified or managed in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	I confirm that evidence of compliance will be provided promptly on request.
	Yes
	

	
	No
	


[bookmark: _Toc227064020][bookmark: _Toc497207932][bookmark: _Toc488834423][bookmark: _Toc460518593][bookmark: _Toc474254483]
Quality Assurance – Pass/Fail Criteria 
	Do you operate a quality management system? 
	Yes
	
	No
	

	Name of Manager responsible for Quality 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	If in-house, please provide summary of system: 
	







[bookmark: _Toc227064021]Response to Specification	
	Requirement
	Compliant
(Yes / No)
	Comment

	Warranty: The tools and ancillary equipment including batteries shall have a minimum warranty of 2 years.
	
	

	Samples for Field Trials: The tenderer shall, upon request, provide a sample of each rescue tool being tendered. These samples must be:
· Supplied within 15 working days of the request, and
· Made available for a minimum period of 10 working days to facilitate field trials and operational evaluation.
	
	

	Documentation: A full set of documentation shall be provided to include as a minimum: 
· Operating and safety manuals;
· Cleaning, servicing, maintenance, and repair instructions; and
· Relevant risk assessments.
This documentation must be supplied in either Irish or English, or both, and may be provided in hard copy or electronic format.
	
	

	Certification: The tenderer shall provide certification documentation with the tender demonstrating the equipment complies with EN 13204:2025 (and any subsequent amendments).
	
	

	Training: The tenderer shall provide full details on how training will be delivered at both station level and for Brigade maintenance personnel. A minimum of a half-day training session shall be provided for all operational personnel at each of 20 stations. Additionally, a minimum of a half-day inspection and light maintenance training shall be provided for Brigade maintenance personnel. All costs associated with the training including labour, travel, and subsistence must be included in the overall supply of the equipment and shall not incur any additional charges.
	
	

	Parts & Servicing: The tenderer shall provide a detailed breakdown of all annual and multiannual replacement parts required for servicing, as recommended by the manufacturer. The tenderer shall include the current cost of these parts, along with the estimated total cost of annual servicing over a four-year period. This estimate must include all associated costs, including labour, travel, and subsistence, for servicing the tools at the stations where they will located – details to be provided.
	
	





[bookmark: _Toc220052595]A 1.3.2 Tool Requirements 

	Requirement
	Compliant
(Yes / No)
	Comment

	Operating Life: All tools and ancillary equipment must have a minimum operating life of 15 years.
	
	

	
Ergonomics: The tools shall be designed to deliver a high power-to-weight ratio, ensuring ease of manual handling and operation by a diverse workforce. The tools must incorporate:
· Ergonomically designed handles that allow for secure grip and control in multiple operating positions;
· Capability of operation by one or two personnel; 
· Usability across a range of working heights, including:
· Calf/knee level – e.g. car sill level;
· Waist level – e.g. base of car at A and C post level; and
· Chest level – e.g. top of car at A, B, and C post level.
These design features shall facilitate efficient and safe operation during extrication tasks in varied and challenging environments.
	
	

	CE Marking: All tools and ancillary equipment must be individually CE marked. 
	
	

	Serial Number: All tools and ancillary equipment, including batteries, must be individually marked with a unique traceable serial number.
	
	

	LED lighting: All tools must have integral LED lighting to facilitate use in restricted light conditions with an on/ off switch, the lights must be powered by the main battery.
	
	

	Control Handle and Actuator: The rescue tools shall be equipped with a manual control actuator, which must:
· Be easily accessible in all operating positions; and
· Feature an automatic return to neutral position for enhanced safety and control.
The control handle shall:
· Have a minimum length of 75 mm to ensure a full and secure grip for the operator’s hand;
· Be designed for operation from all angles by a single operator, including in confined spaces such as those encountered inside vehicles during road traffic collisions; and
· Support use in varied body positions and orientations, ensuring ergonomic and safe handling in challenging environments.
	
	

	IP Ratings: Each tool and its associated battery must be suitable for underwater use and meet the following minimum Ingress Protection (IP) ratings:
· Tools: Minimum protection rating of IP57, ensuring protection against dust ingress and temporary immersion in water.
· Batteries: Minimum protection rating of IP54, ensuring protection against limited dust ingress and water spray from any direction.
	
	

	Noise: Under full load conditions, the noise emission levels of each tool shall not exceed:
· 75 dB(A) at a distance of 1 metre; and
· 66 dB(A) at a distance of 4 metres
	
	

	Auto Stop/Start: Each tool shall be equipped with an auto start/stop function to optimise battery efficiency, to reduce wear on components and support efficient and operational safety. The motor/drive system must automatically stop when:
· The tool is not in use, or
· The tool has reached its maximum operating pressure.
The tool must automatically restart when the control handle is turned again, allowing seamless reactivation by the operator without additional steps.
	
	




[bookmark: _Toc220052596](a) 1.3.3 Battery Requirements 

	
Requirement
	Compliant
(Yes / No)
	Comment

	Standards: All batteries must conform to EN 62133-2:2017 and A1:2021 (or any subsequent amendments of same).
	
	

	Interfacing:  The batteries shall meet the following minimum requirements:
· They must fit securely to the tool to prevent accidental separation or damage during operation;
· They must be easily connectable to the tool by a single operator wearing fire-fighter gloves;
· Their replacement must not cause any unintended movement of the tool’s jaws, arms, or rams (as applicable); and
· They must be capable of interfacing with diagnostic software to provide detailed information on the battery’s health status.
	
	

	Status: Each battery must be equipped with a visual charge status indicator that is clearly visible and readable while the battery is connected to the rescue tool, and while the battery is connected to the charger.
	
	

	Rating: All batteries must be Lithium-Ion type with a minimum capacity rating of 5 ampere-hours (5Ah).
	
	

	Charging Time: Batteries must be capable of reaching a full charge from a fully discharged state within a maximum of 120 minutes. This requirement applies when using either a mains-powered AC charger, or a vehicle-powered DC charger.
	
	

	Continuous Charging: The equipment must be designed to remain on continuous charge without risk of damage to either the battery or the charger.
	
	

	Durability: All batteries must be capable of withstanding a minimum of 500 full charge-discharge cycles (i.e., from fully discharged to fully charged) without significant degradation in performance or capacity. Tenderers must provide verifiable documentation from the battery manufacturer confirming compliance with this requirement, including test data or certification where available.
	
	

	

	
	

	
Requirement
	Compliant
(Yes / No)
	Comment

	Supply Voltage: Battery chargers must be available for use with a standard mains socket supply (220–240V AC). Chargers must provide clear indication of the battery’s state of health both visually on the battery unit, and via diagnostic software, enabling detailed performance monitoring and maintenance planning. Station chargers must be capable of charging a minimum of two batteries simultaneously 
	
	

	On-board charging: The on-board charger shall meet the following criteria:
· Operate at 24V DC;
· Include a battery level indicator for real-time monitoring;
· Be supplied with all necessary ancillary equipment, including a sufficient length of charging cable;
· Be suitable for mounting within a fire appliance;
· Be capable of charging a minimum of one battery;
· Include suitable inline surge protection fuses that are easily accessible for replacement,
or alternatively, be fitted with a resettable circuit breaker that is easily accessible for resetting.
· Be capable of charging a minimum of one battery 
	
	

	Availability: Replacement batteries must be available for 15 years.
	
	


 

[bookmark: _Toc220052597]A 1.3.4 Tool Specifications
A 1.3.4.1 Cutter – Type A

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The cutter must have a minimum jaw opening of 180mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The rescue cutter must meet a minimum cutting performance classification of 1K-2K-3K-4K-5K in accordance with EN 13204:2025 (or any amendments to same). 
	
	

	Weight: The cutter, including the connected battery, shall have a maximum total weight of 25.0 kg
	
	

	General: The design and materials used in the manufacture of the cutting blades must ensure optimum cutting performance is maintained over repeated use, while also providing high durability and resistance to wear. Blades should be engineered to withstand the demands of frequent operational deployment without significant loss of effectiveness.
	
	


 

A 1.3.4.2 Cutter – Type B

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The cutter must have a minimum jaw opening of 200mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The rescue cutter must meet a minimum cutting performance classification of 1K-2K-3K-4K-5K in accordance with EN 13204:2025 (or any amendments to same). 
	
	

	Weight: The cutter, including the connected battery, shall have a maximum total weight of 28.0 kg
	
	

	General: The design and materials used in the manufacture of the cutting blades must ensure optimum cutting performance is maintained over repeated use, while also providing high durability and resistance to wear. Blades should be engineered to withstand the demands of frequent operational deployment without significant loss of effectiveness.
	
	




A 1.3.4.3 Spreader – Type A

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The spreader must have a minimum  opening width of 725mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The spreader must meet or exceed the following performance criteria, in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force: Greater than 40 kN, measured 25 mm from the tips and greater than 320 kN at the steel tips;
· Pulling Force: Greater than 50 kN;
· Pulling Distance: Greater than 610 mm; and
· Squeezing Force: Greater than 100 kN.
	
	

	Weight: The spreader, including the connected battery, shall have a maximum total weight of 22.0 kg
	
	

	General: The spreader must be designed to meet the following operational and functional criteria:
· Accessory Compatibility: The tool must be designed to allow for the secure attachment and use of accessories such as chains or other approved fittings, enhancing its versatility in rescue operations.
· Tip Grip Performance: The spreader tips must be engineered to provide effective grip on a wide range of surfaces during spreading operations, ensuring stability and control under load.
· Tip Profile for Access: The tip design must be suitably fine and tapered to allow insertion into narrow gaps enabling effective initial access in confined or obstructed spaces.
	
	



A 1.3.4.4 Spreader – Type B

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The spreader must have a minimum  opening width of 800mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The spreader must meet or exceed the following performance criteria, in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force: Greater than 60 kN, measured 25 mm from the tips and greater than 450 kN at the steel tips;
· Pulling Force: Greater than 60 kN;
· Pulling Distance: Greater than 600 mm; and
· Squeezing Force: Greater than 110 kN.
	
	

	Weight: The spreader, including the connected battery, shall have a maximum total weight of 25.0 kg
	
	

	General: The spreader must be designed to meet the following operational and functional criteria:
· Accessory Compatibility: The tool must be designed to allow for the secure attachment and use of accessories such as chains or other approved fittings, enhancing its versatility in rescue operations.
· Tip Grip Performance: The spreader tips must be engineered to provide effective grip on a wide range of surfaces during spreading operations, ensuring stability and control under load.
· Tip Profile for Access: The tip design must be suitably fine and tapered to allow insertion into narrow gaps enabling effective initial access in confined or obstructed spaces.
	
	


A1.3.4.5 Combination Tool 

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: Must have a minimum spreader opening of greater than 350 mm and a minimum cutting opening greater than 300mm under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The combination tool shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force: Greater than 40 kN, measured 25 mm from the tips.
· Cutting Force: The combination tool must achieve a minimum cutting performance classification of Class ‘J’ in accordance with EN 13204:2025 (or any amendments to same). 
· Squeezing Force:  Greater than 75 kN.
	
	

	Weight: The combination tool, including the connected battery, shall have a maximum total weight of 25.0 kg
	
	



A 1.3.4.6 Telescopic Ram

	[bookmark: _Hlk204344883]
Requirement
	Compliant
(Yes / No)
	Comment

	Stroke and Dimensions:
The ram shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· Total stroke: Greater than 700 mm
· Retracted length: Less than 600 mm and less than the maximum opening of the proposed spreader.
· Extended length: Greater than 1200 mm
(This may be achieved using an extension poles.)
	
	

	Performance: The ram shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force:
· First stage: Minimum 100 kN
· Second stage: Minimum 60 kN
	
	

	General: The ram must be designed for safe and effective use in conjunction with compatible accessories, including but not limited to ram supports and sill clamps.
	
	

	Weight: The ram including the connected battery, shall have a maximum total weight of 22.0 kg
	
	



A 1.3.4.7 Mini Cutter

	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: Must have a minimum cutter opening of greater than 50 mm under EN 13204:2025 (or any amendments to same).
	
	

	Performance: The cutter shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· A minimum cutting performance classification of 1C-2C-3B in accordance with EN 13204:2025 (or any amendments to same).
	
	

	Accessories: The Mini Cutter must be supplied with a suitable battery, mains charger and charging lead if battery powered.
	
	

	

Requirement
	Compliant
(Yes / No)
	Comment

	Weight: The combination tool, including any connected battery / drive unit, shall have a maximum total weight of 12.0 kg.
	
	

	Battery Charge: If battery powered, the battery must be capable of at least 50 cuts.
	
	



A 1.3.4.8 Ram Support

	
Requirement
	Compliant
(Yes / No)
	Comment

	Performance: Each ram support must be specifically designed to maximise and evenly distribute the load exerted by the ram, particularly during cross-ramming techniques.
	
	

	Size: Each ram support shall have a maximum footprint of 500 mm x 500 mm with a maximum height/depth of 200 mm.
	
	

	Weight: Each ram support should weigh no more than 14.0 kg
	
	

	Gripping surface: Each ram support must be fitted with a suitable gripping surface to ensure secure anchoring and stability during operation.
	
	

	Material & Finishing: Each ram support must be manufactured from a suitable high-strength metal or alloy to ensure structural integrity under load and treated for corrosion resistance, preferably by zinc coating. If painting is used as the protective method, the supports must be rust-proofed prior to painting to ensure long-term durability.
	
	


4


	
Diagnostic Equipment 1.3.4.9
 Requirement
	Compliant
(Yes / No)
	Comment

	Performance: Diagnostic software shall be capable of undertaking the following 
	
	

	Provide detailed information on the battery’s operating state, including:
· The number of charge cycles completed;
· The state of health of the battery; and
· Any potential faults or anomalies detected.

	
	

	Offer diagnostic capabilities for the tools themselves, including:
· A health status report on tool performance and operational capability; and
· Integration with the annual service process to assess tool condition

	
	

	Generate a written or electronic record of each tool’s performance and status following its annual service: Ensure the Brigade:
· Has direct access to these service records, or
· Is provided with the records annually by the supplier or service provider.

	
	

	Be capable of been access by at least  3 Laptops 
	
	














[bookmark: _Toc227064022]RESPONSE TO THE AWARD CRITERIA

FORM OF TENDER
Tenders for supply of Fire Service Water Tanker  
I/We have examined the tender documentation and hereby offer to provide the supplies in accordance with the details contained within the Specification of the Request for Tender Contract Open Procedure. 

Specification Section 3 of the Request for Tender Contract Open Procedure  . 
	Battery-Operated Rescue Tools and Ancillary Equipment Pricing Cost Table (Ex. VAT)

	Ref
	Type (See Appendix A for detailed specification requirements)
	A. Cost Per Unit (EX VAT)
	B. Notional Volume Units
	Total (A X B)    Ex VAT

	1.3.4.1
	Medium Duty Battery Operated Hydraulic Cutters Type A
	
	20
	

	1.3.4.2
	Heavy  Duty Battery Operated Hydraulic Cutters Type B
	
	4
	

	1.3.4.3
	Medium Duty Battery Operated Hydraulic Spreaders Type A 
	
	20
	

	1.3.4.4
	Heavy  Duty Battery Operated Hydraulic Spreaders Type B
	
	4
	

	1.3.4.5
	Battery Operated Combi Tool
	
	20
	

	1.3.4.6
	Battery Operated Telescopic Ram
	
	48
	

	1.3.4.7
	Battery Operated Mini Cutters
	
	24
	

	1.3.4.8
	Ram/Cill  Supports 
	
	48
	

	1.3.4.9
	Diagnostics software 
	
	3
	

	1.3.3
	Batteries 
	
	140
	

	1.3.3
	In-vehicle battery charger and wiring
	
	24
	

	1.3.3
	Station desktop charger 
	
	24
	

	Total
	
	
	
	

	
	







I/We confirm that I/we: 

· Will keep this offer for the contract / framework open for acceptance by you for a period of 12 months from the date of deadline for submission of Tenders,
· Agree that you are not bound to accept the most economically advantageous or any Tender you may receive,
· Have read and thoroughly examined the Tender Document,
· Fully understand the Tender Document and the Client’s requirements,
· Undertake to treat the details of this Invitation to Tender, its Tender and any subsequent agreements as private and confidential,
· Acknowledge that acceptance by the Contracting Authority of this tender will not constitute a binding and enforceable agreement and that a legally enforceable agreement will not exist until and unless the contract is awarded / framework agreement has been established between the Contracting Authority  and the Tenderer,
· Have availed of all offers for additional information or have otherwise satisfied myself/ourselves as to conditions that may in any manner affect the performance of the contract,
· Have included all elements necessary for the performance of the specified requirements, which are either expressly stated in the Tender Document or contained in any supplementary information or which could reasonably be inferred there from,
· Have found no errors, omissions, conflicts or ambiguities in the Tender Document except those which I/We have brought to the attention of the Contracting Authority before the latest date for submitting queries,
· Have included for compliance with all statutory requirements applicable in Ireland and those applicable in any country where parts of the contract may be performed that are in force 7 days prior to the deadline for receipt of Tenders, 
· [bookmark: _Hlk491592638]Will not, if awarded a contract employ labour in a manner that is discriminatory in relation to gender, race, religious beliefs, age etc.,
· Agree that as a condition of award, it shall be our sole responsibility to fulfil the obligations under the Contract, notwithstanding any changes in circulars, laws, regulations, taxation, duties or other factors which might arise following the withdrawal of the United Kingdom from membership of the EU.
	Signed:
	

	Name (in Capital Letters):
	

	On behalf of:	
	

	Address:
	

	Telephone:
	
	Fax:
	

	Email:
	
	Date:
	









#













[bookmark: _Toc227064029]Response to Qualitative Award Criteria
	Criterion A:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Compliance with Technical Specifications and Minimum Warranty Requirements

	
	
	

	
	Pass/Fail 
	Pass
	Pass 

	Instructions
	The Tenderer must detail in The Tender Response Document the compliance of the tendered equipment with the technical specifications and minimum warranty requirements set out in Appendix 1.
Cork County Fire Service will review various proposed solutions along with variations and will determine if the solution proposed broadly meets their requirements as set out in the RFT.
Only Tenders that receive a “Pass” mark for this award criterion will proceed to be evaluated under the                 remaining award criteria.


	Tenderers’ Response

	Criterion B:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Cost Criterion  
	
	
	

	
	50%
	500
	NA

	Instructions
	Overall Cost inclusive of Delivery and all additional taxation and custom and excise duties that may occur as a consequence of the withdrawal of the UK form the European Union. 

	Tenderers’ Response


Please use this free text page(s) (i.e. don’t type in the box) for your response. 

	[bookmark: _Hlk195019625]
Criterion C:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Field Trials 

	
	
	

	
	20%
	200
	100

	Instructions
	Cork County  Fire Service will carry out a practical assessment to test the operational effectiveness of the equipment. The methodology for this and the scoring system is outlined in Appendix 1 Requirements & Specification

	Tenderers’ Response


Please use this free text page(s) (i.e. don’t type in the box) for your response. 
	Criterion D:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Aftersales Support & Technical Assistance

	
	
	

	
	10%
	100
	50

	Instructions
	The Tenderer must set out the quality of its proposal in relation to its capacity and capability for the provision of maintenance, repair and technical assistance from its maintenance facilities, and its capacity and capability for repair/maintenance services. Tenderers must provide details of maintenance facilities, if any, they have in the Republic of Ireland to carry out repairs. The Tenderer should also provide details of the process by which clients’ repair issues are managed from the time a fault is reported through to   successful conclusion. If sub-contracting after sales support to another supplier, full details must be provided of that sub-contractor, including their maintenance facility details, network details, technical capabilities of their employees in relation to support and their qualifications for same, and details of stock they carry and where the stock is located.
Please provide all detail in the Tender Response Document


	Tenderers’ Response



	Criterion E:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Availability of Spare Parts

	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must set out the quality of its proposal for ensuring the availability of all spare parts for the equipment  and ancillary equipment for the minimum expected lifespan of the equipment  (15 years). 
The Tenderer should include details of its process and lead times for obtaining spare parts; how it manages this supply chain to ensure parts are delivered on time; and how it manages instances of order delays and parts being out-of-stock.
Please provide all detail in the Tender Response Document


	Tenderers’ Response



	Criterion F:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Ordering & Delivery

	
	
	

	
	5%
	50
	30

	Instructions
	The Tenderer must provide a detailed narrative demonstrating its high-level process and timescales for the successful delivery of  the RTC Equipment  - from the time of the official order through to full commissioning and handover of the appliance.
The Tenderer should Include details of the tenderer’s methodology for ensuring that all appliances are supplied and delivered in accordance with the requirements specified by the client.
Please provide all detail in the Tender Response Document


	Tenderers’ Response



	Criterion G:  
	Weighting 
	Maximum Marks
	Minimum Marks Required

	Title: Environmental & Sustainabilitilty Efficiencies  

	
	
	

	
	5%
	50
	30

	Instructions
	The Tenderer must provide a detailed narrative to demonstrate how it incorporates environmental and sustainability efficiencies/measures during the build   process. For example:
· Energy optimisation initiatives in the              warehouse/premises including rain harvesting, use of PV Panels, fabric of the building including insulation, efficiency of lighting and heating, EV charging capabilities etc.
· Use of recycled and/or recyclable material
· Waste management/disposal/recycling
· Minimisation of waste
· Transport and logistics measures
· Corporate Social Responsibility policies
· Proposed Targets for Environmental Sustainability
· Sustainable purchasing 

Please provide all detail in the Tender Response Document


	Tenderers’ Response



NOTE 1:	Tenderers should ensure in their tenders that they provide detailed information in respect of all aspects of the contract award criteria as stated above.  This will enable the awarding authority to assess fully the extent of their offers.
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