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TENDER RESPONSE DOCUMENT
	Subject Matter of Request for Tender

	Supply of Battery-Operated Hydraulic Rescue Equipment and Ancillary Rescue Support Equipment

	Closing Date and Time for Receipt of Tenders:
	As per eTenders

	Organisation Name:
	Donegal County Council

	Contact Name: 
	As per eTenders

	Contact Email:
	As per eTenders

	NOTES
•	Note #1: Please read this document in conjunction with the separate RFT document and other relevant documentation provided including Pricing Documents where relevant.
•	Note #2: This Tender Response Document (and other mandatory documents provided) must be used for responding to the Request for Tenders. Tenderers must not personalise or modify the current format.
•	Note #3: Tenderers are recommended to upload this completed response as a Zip file in order to protect the integrity of file names.
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[bookmark: _Toc232693376]Instructions for Completion
Tenderers should ensure they have read the Request for Tender before they attempt to complete this Tender Response Document.  
If you consider that the Tender Response Document is missing any sections which would prevent you from preparing a comprehensive response, please contact the Contracting Authority as soon as possible (prior to the closing date for queries).  
Where there is a discrepancy between the contents / instructions in this document and the Request for Tender, the Request for Tender will take precedence.   
Tenderers must follow the instructions contained in this document in relation to attachments, format for submission, etc.  

Where tenderers are relying on other parties to meet the selection criteria, those parties must be available to deliver elements of the contract. 












[bookmark: _Toc232693377]Response to Selection Criteria

TENDERERS SHOULD NOTE THESE CRITERIA ARE ASSESSED ON A PASS/FAIL BASIS

[bookmark: _Toc232693378]General Contact Information
	Organisation Name:
	

	Contact Person:
	

	Position: 
	

	Address: 
	

	Phone:
	

	Email: 
	

	Website: 
	

	Small and Medium Enterprise (SME)
	Yes
	☐	No
	☐
	Date of Establishment, if applicable
	VAT Registration No:
	Legal Structure – partnership, limited company, etc.

	
	
	

	Details and contributions of other parties (if applicable) 

	Official name of entity
	Selection criterion where Tenderer is relying on their resources to qualify 
and/or 
Service/element to be delivered by third party
	The third-party is clearly identified throughout the response

	
	
	Yes
	No

	
	
	☐	☐
	
	
	☐	☐




[bookmark: _Toc232693379]Financial Information – Pass/Fail Criteria
	
Tax Clearance
	Please confirm YES / NO

	Option 1: I confirm and declare being tax compliant.  The Contracting Authority can verify your tax clearance status through Revenue’s online facility at http://www.revenue.ie/en/online/tax-clearance.html  To this end, please confirm:
	Yes
	☐
	(A) 
	No
	☐
	Tenderer Name:
	

	Tenderer PPSN/ Tax Reference Number
	

	Access Number
	

	Option 2: I confirm that I hold a current valid paper Tax Clearance Certificate (generally relates to Non-Residents)

	Registration Number
	
	Certificate Number
	

	Option 3: I confirm that I have applied/or will apply for Tax Clearance status or a Tax Clearance Certificate which will be made available on request
	Yes
	☐
	
	No
	☐
	Turnover

	I confirm that we have the requisite turnover to be considered for the contract/framework.

	Year
	2025
	2024
	2023

	Month End (e.g. July)
	
	
	

	Turnover €
	

	
	

	I confirm that I will provide evidence of turnover promptly on request.
NOTE #1:  In the case of sole traders or partnerships this condition may be satisfied by a letter of confirmation from a senior partner.
	Yes
	☐
	
	No
	☐



	Insurances

	I confirm that we have the following insurances in place 

	Insurance Type
	Level required if successful
	Level in Place
	Details of Any Excess
	Renewal Date

	Employers Liability
	€13,000,000
	€
	
	

	Public Liability
	€6,500,000
	€
	
	

	Product Liability
	€6,500,000
	€
	
	

	AND

	I confirm that if successful, where the levels required under the contract/framework are higher than those currently in our possession, I will be in a position to put the required forms and levels of insurances required in place. 
	

	AND

	I confirm that I will provide the following promptly on request:
· evidence of insurances in place      
or 
· letter from Insurance Broker confirming that the required levels can be put in place if successful 
Note: insurance policies where relevant must have jurisdiction in Ireland.
	














[bookmark: _Toc232693380]Declaration Re Personal Circumstances – Pass/Fail Criteria
	DECLARATION RE PERSONAL CIRCUMSTANCES AS PER ART. 57 OF DIRECTIVE 2014/24/EUEconomic Operators will be excluded from the procurement process if, within the past five (5) years, there is evidence of a conviction relating to a specific criminal offence listed below (see 1.1) or if they have been the subject of a binding legal decision which found a breach of legal obligations to pay tax or social security contributions (see 1.2) (except where this is disproportionate e.g. where only minor amounts are involved). 

	1.1 Has the Economic Operator or a member of their proposed consortium, (if applicable), Director, or Partner or any other person who has powers of representation, decision or control, been convicted of any of the following offences?
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box 

	1.1.a
	participation in a criminal organisation, as defined in Article 2 of Council Framework decision 2008/841/JHA;
	
	

	1.1.b
	corruption, as defined in Article 3 of the Convention on the fight against corruption involving officials of the European Communities or officials of Member States of the European Union and Article 2(1) of Council Framework Decision 2003/568/JHA as well as corruption as defined in Irish Law or the jurisdiction in which the Economic Operator is established;
	
	

	1.1.c
	fraud within the meaning of Article 1 of the Convention on the protection of the European Communities’ financial interests;
	
	

	1.1.d
	the subject of a conviction for terrorist offences or offences linked to terrorist activities or for inciting or aiding or abetting or attempting to commit an offence; 
	
	

	1.1.e
	the subject of a conviction for money laundering or terrorist financing; 
	
	

	1.1.f
	the subject of a conviction of child labour and other forms of trafficking in human beings;
	
	

	Non-payment of taxes or social security obligations
1.2 Has it been established by a judicial or administrative decision having final and binding effect in accordance with Irish law or the legal provisions of the country in which the Economic Operator is established (if outside Ireland), that the Economic Operator is in breach of obligations related to the payment of tax and social security contributions?
Note: If the response to 1.2 above is in the affirmative, please provide further information on the decision and the amounts involved
	
	



	2.1 Please indicate if any of the following situations have applied, within the past three (3) years, or currently apply, to your organisation.
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box

	2.1.a
	has, in the performance of any public contract, failed to comply with applicable obligations in the field of environmental, social and labour law applying at the place where the works were carried out or the services provided, as established by EU law, national law, collective agreements or by international, environmental, social and labour law listed in Annex X of Directive 2014/24/EU;
	
	

	2.1.b
	is bankrupt or the subject of insolvency or winding-up proceedings, its assets are being administered by a liquidator or by the court, or has entered into an arrangement with creditors, suspended its business activities or is in any analogous situation arising from a similar procedure under national laws and regulations;  
	
	

	2.1.c
	is guilty of grave professional misconduct which renders its integrity questionable;
	
	

	2.1.d
	has entered into agreements with other economic operators aimed at distorting competition;
	
	

	2.1.e 
	has a conflict of interest within the meaning of Article 24 of 2014/24/EU that cannot be effectively remedied by other, less intrusive, measures; 
	
	

	2.1.f 
	confirms that it has had prior involvement in the preparation of the procurement procedure which has resulted in a distortion of competition, as referred to in Article 41 of 2014/24/EU, that cannot be remedied by other, less intrusive, measures;
	
	

	2.1.g
	has shown significant or persistent deficiencies in the performance of a substantive requirement under a prior public contract, a prior contract with a contracting entity, or a prior concession contract, which led to early termination of that prior contract, damages or other comparable sanctions. 
	
	

	2.1.h
	· is guilty of serious misrepresentation in supplying the information required for the verification of the absence of grounds for exclusion or the fulfilment of the selection criteria; or
	
	

	
	· has withheld such information or is not able to submit supporting documents required under Article 59 of Directive 2014/24/EU; or 
	
	

	2.1.i
	has undertaken to:
· unduly influence the decision-making process of the contracting entity, obtain confidential information that may confer upon the Tenderer undue advantages in the procurement procedure; or
· negligently provide misleading information that may have a material influence on decisions concerning exclusion, selection or award.
	
	


[bookmark: _Toc487559492]
[bookmark: _Toc232693381]Declaration Re Statutory Obligations – Pass/Fail Criteria
	We confirm that we are fully compliant with the following legislation, or equivalent legislation in our country of establishment/operation:
	YES
	NO

	(a) 
	Employment Equality Acts 1998-2011 
	
	

	(b) 
	Equal Status Acts 2000-2011
	
	

	(c) 
	National Minimum Wage Act 2000 as amended 
	
	

	(d) 
	Organisation of Working Time Act 1997 as amended
	
	

	(e) 
	Safety, Health and Welfare at Work Act 2005 and Safety, Health and Welfare at Work (General Application) Regulations 2007
	
	

	(f) 
	Disability Act 2005
	
	

	(g) 
	Regulation (EU) 2016/679 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data, the Data Protection Act, 2018
	
	

	(h) 
	We further confirm that all Data Subjects whose Personal Data is provided in our Tender have consented to the processing of such Personal Data by us, the Contracting Authority, the Evaluation Team and the supplier of the etenders.gov.ie website, for the purposes of our participation in this Competition or that we otherwise have a legal basis for providing such Personal Data to the Contracting Authority for the purposes of our participation in this Competition and that we will provide evidence of such consent and / or legal basis to the Contracting Authority upon request.
	
	

	(i) 
	We have procedures in place to ensure that our subcontractors, if any are used for this contract, apply the same standards.
	
	


[bookmark: _Toc232693382]Declaration Re International Procurement Instrument  & Article 5k of 2022/576 (context of Russian Actions in the Ukraine) – Pass/Fail Criteria
	(j) 
	The Contracting Authority would refer Tenderers in particular to the provisions of Regulation (EU) 2022/1031 on the access of third country economic operators, goods and services to the Union’s public procurement and concession markets and procedures supporting negotiations on access of Union economic operators, goods and services to the public procurement and concession markets of third countries (International Procurement Instrument – IPI), and to their obligation to comply therewith. In particular, tenderers and candidates should note in Article 6 of Regulation (EU) 2022/1031, the obligations for a Contracting Authority in the context of a procurement procedure where the EU Commission has adopted an IPI measure.  
	
	

	(k) 
	The Contracting Authority may decide to examine tenders before verifying the absence of exclusion grounds in Regulation 57 of the regulations (the “Exclusion Grounds”) and the fulfilment of the Selection Criteria. 
However, notwithstanding anything contrary in this part 2.4, The Contracting Authority reserves the right to ask Tenderers at any moment during the Competition to submit any of the following for the purposes of verification of the status of the tenderer (including Prime Contractor and any Subcontractor).
(i) information concerning the Tenderer, and any proposed subcontractors, for the purposes of Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same) including, but not limited to, in respect of natural persons, copies of identity documents and, in respect of legal persons, a certificate or extract from the commercial register or other competent authority of the country in which the legal person is established.
(ii) and information concerning the origin of goods, if any, for the purposes of assessing compliance with Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	

	(l) 
	If a Tenderer does not, upon request by the Contracting Authority, provide evidence which is considered by the Contracting Authority as sufficient to demonstrate (i) its fulfilment of the Selection Criteria (or any one of them) in accordance with this RFT and (ii) the absence of Exclusion Grounds, or its reliability despite the existence of a relevant Exclusion Ground and (iii) that it does not come within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576) and (iv) that the origin of goods, if any, are not subject to the prohibitions set out in Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same) then it shall be excluded from further participation in this Competition.
	
	

	(m) 
	If a Tenderer does not, upon request by the Contracting Authority, provide evidence which is considered by the Contracting Authority as sufficient to demonstrate (i) the fulfilment by any Subcontractor on whose capacity the Prime Contractor relies of the Selection Criteria (or any one of them) in accordance with this RFT and (ii) the absence of Exclusion Grounds in respect of any Subcontractor, or the reliability of any Subcontractor despite the existence of a relevant Exclusion Ground and (iii) that any proposed Subcontractor on whose capacity the Tenderer relies (where the value of that subcontract exceeds 10% of the value of the Services Contract) does not come within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576) then, it shall be excluded from further participation in this Competition unless it replaces the Subcontractor with one which meets all relevant requirements of this RFT.
	
	

	(n) 
	We do not come within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU regulation 2022/576 or any subsequent amendments to same). 
	
	

	(o) 
	The origin off goods connected to our Tender, if any, are not subject to the prohibitions set out in Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	

	(p) 
	The subcontractor(s) on whose capacity we rely as part of our Tender (where the value of that subcontract exceeds 10% of the value of the Services Contract) does not come within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	

	This Declaration is made for the benefit of the Contracting Authority 
I certify that the information provided in the Declarations above are accurate and complete to the best of my knowledge and belief.  I understand that the provision of inaccurate or misleading information in these Declarations will lead to my organisation being excluded from participation in this and future tenders and I am signing on behalf of: 


	Name of Tenderer      
	


	Name of Authorised Signatory
	


	Position

	

	Signature
	








[bookmark: _Toc232693383][bookmark: _Hlk199064604][bookmark: _Hlk523749692]Previous Contracts / Experience – Pass/Fail Criteria
	Reference Contract #1

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement.  Please note mere confirmation will not suffice:  

	Details of contract for the supply of battery-operated hydraulic rescue equipment 
	



	Any other relevant information 

	






	Reference Contract #2

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	Details of contract for the supply of battery-operated hydraulic rescue equipment
	



	Any other relevant information 

	






	Reference Contract #3

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract / scope of the framework agreement, please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	Details of contract for the supply of hydraulic rescue equipment
	



	Any other relevant information 

	






















[bookmark: _Toc232693384]Personnel and Skills – Pass/Fail Criteria
	Minimum requirement to remain eligible in the competition:  Tenderers must demonstrate access to at least the minimum numbers of skilled personnel stated. Please note that the skills outlined may reside in the same person.   

	Skillset Required
	Number of Full Time Equivalent (FTE)
	Number of FTEs provided by 3rd Parties – based on parties identified in Section on General Contact Information
	Minimum Number Required

	No of competent service personnel 
	
	
	2

	Total
	
	
	n/a

	Tenderers are reminded that they may rely on the resources of other entities on condition that they are fully described, and that Tenderers can prove that they will have these resources at their disposal when required.
Please attach an organisation chart, clearly identifying all relevant departments, divisions, and 3rd parties, if applicable.












[bookmark: _Toc232693385]Technical Equipment and Resources – Pass/Fail Criteria
See Appendix 1 for full requirements details.

	
Requirement
	Compliant
(Yes / No)
	Comment

	Table A.1 Battery Operated Rescue Equipment General Requirements
	
	

	Table A.2 Battery Requirements
	
	

	Table A.3 Type A Cutter Requirements
	
	

	Table A.4 Type B Cutter Requirements
	
	

	Table A.5 Type A Spreader Requirements
	
	

	Table A.6 Type B Spreader Requirements
	
	

	Table A.7 Telescopic Ram Requirements
	
	

	Table A.8 Mini-cutter Requirements
	
	

	Table A.9 Ram Support Requirements
	
	



Appendix 1 must be completed first and subsequently summarised above .

[bookmark: _Toc232693386]Health & Safety – Pass/Fail Criteria
	Minimum requirement to remain eligible in the competition: Tenderers must demonstrate compliance with all the relevant Health & Safety legislation.  The Contracting Authority reserves the right to seek further information to verify compliance.

	Do you comply with the Safety Health & Welfare at Work Act 2005? 
	Yes
	
	No
	

	Manager responsible for Health and Safety: 
	

	Is it externally certified or managed in-house? 
	Externally Certified
	

	
	In-House
	

	If externally certified, please provide the following information: 
	Date of most recent certification:
	

	
	Scope of Certification:
	

	
	Name of Certification Body:
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	


[bookmark: _Toc232693387][bookmark: _Toc488834423][bookmark: _Toc460518593][bookmark: _Toc474254483]Response to the Award Criteria

[bookmark: _Toc232693388]Form of Tender – Supplies – Cost Criterion A 
	To: 
	 

	From: 
	

	Re: 
	


I/We have examined the tender documentation and hereby offer to provide the supplies (and  in accordance with the details contained within the Request for Tender Document.
[bookmark: _Toc232693389]Criterion 1 - Cost
	[bookmark: _Hlk480561427][bookmark: _Hlk157165601]Criterion 1
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	40%
	400
	N/A

	Title
	COST

	Description
	Tenderers must complete the Cost Criterion below. 



Cost Criterion Table
	  Battery Tool Pricing Cost Table (Ex VAT)

	Ref
	Type
	A. Cost Per Unit (Ex. VAT)
	B. Notional Volume Units
	Total (A X B)
Ex VAT

	1
	Batteries (minimum 8Ah) – 5 per set
	
	85
	

	2
	Battery mains power connector
	
	17
	

	3
	Battery Charger (220-240V) – 3 per set
	
	51
	

	4
	Cutter Type A
	
	16
	

	5
	Cutter Type B
	
	1
	

	6
	Spreader Type A
	
	16
	

	7
	Spreader Type B
	
	1
	

	8
	Ram (including extensions where required) – 2 of each per set
	
	34
	

	9
	Ram Support – 2 per set
	
	34
	

	10
	Mini Cutter - 2 batteries and 1 charger per set
	
	17
	

	Total
	


Options Cost Table
	  Options Cost Table (Ex VAT) Will not be considered when assessing cost criterion.

	Ref / Description
	A. Cost Per Unit (Ex. VAT)
	B. Notional Volume Units
	Total (A X B) Ex VAT

	Option 1 / Equipment Diagnostics
Supplier should quote for supply of two sets of Diagnostic software and all associated hardware which can provide information to maintenance personnel on the operating state of the tools (excluding mini-cutters).
The diagnostic software should be capable of:
· providing information on the number of charges the battery has undergone, the state of health of the battery and indicate any potential fault.
· providing health status on the tools in terms of their performance and operating capability as part of the tools annual service.
· generating a written / electronic record of the performance and status of each tool after annual service and the system should be such that Donegal County Fire Service either has access to the service record or will be provided with the service record annually.


	
	2
	

	Option 2 – Spreader Pulling Chain Sets
Supplier should quote for supply of 17 sets of pulling chains (minimum pulling capacity of 60kN) and all associated accessories/tip adaptors to ensure the correct operation of the pulling chains.
· The pulling chains should be supplied in suitable box


	
	17
	

	Option 3 – Forcible Entry Tools
Supplier should quote for supply of 17 no. manual forcible entry tools
· maximum weight of 10kg
· minimum spreading force of 30kN

	
	17
	

	Option 4 – On-tool Charging
Supplier should quote for supply of:
a) 3 no. on-tool charging cords 
b) 3 no. daisy chain cords
per set (17 sets)
	
	51
51
	

	Option 5 – Rescue Platforms
Supplier should quote for supply of 4 no. HGV Rescue Platforms
· Maximum permissible load: 500kg
· Working height required: Up to 1.4m

	
	4
	

	Option 6 – Maintenance Costs
Supplier should quote for the estimate of annual, maintenance costs, including labour, consumables travel and subsistence at 15 stations for all items in Table 5a.

	
	
	



Note 1:
Tenderers must complete all required inputs in the pricing schedule to remain eligible in this competition.
Any alteration or amendment to the pricing schedule may result in that tenderer’s bid being rejected.

I/We confirm that I/we: 

· In relation to daily/hourly fees all rates are inclusive of out of pocket (i.e. mileage, subsistence, phone, postage, etc.) and account / contract management related costs. 
· Will keep this offer for the contract / framework open for acceptance by you for a period of 12 months from the date of deadline for submission of Tenders,
· Agree that you are not bound to accept the most economically advantageous or any Tender you may receive,
· Have taken account of all obligations under the Contract including supply chain and related risk factors.   
· Have read and thoroughly examined the Tender Document,
· Fully understand the Tender Document and the Client’s requirements,
· Undertake to treat the details of this Invitation to Tender, its Tender and any subsequent agreements as private and confidential,
· Acknowledge that acceptance by the Contracting Authority of this tender will not constitute a binding and enforceable agreement and that a legally enforceable agreement will not exist until and unless the contract is awarded / framework agreement has been established between the Contracting Authority and the Tenderer,
· Have availed of all offers for additional information or have otherwise satisfied myself/ourselves as to conditions that may in any manner affect the performance of the contract,
· Have included all elements necessary for the performance of the specified requirements, which are either expressly stated in the Tender Document or contained in any supplementary information or which could reasonably be inferred therefrom,
· Have found no errors, omissions, conflicts or ambiguities in the Tender Document except those which I/We have brought to the attention of the Contracting Authority before the latest date for submitting queries,
· Have included for compliance with all statutory requirements applicable in Ireland and those applicable in any country where parts of the contract may be performed that are in force 7 days prior to the deadline for receipt of Tenders, 
· Will not, if awarded a contract employ labour in a manner that is discriminatory in relation to gender, race, religious beliefs, age etc.
· [bookmark: _Hlk491592638]Agree that as a condition of award, it shall be our sole responsibility to fulfil the obligations under the Contract.
	Signed:
	

	Name (in Capital Letters):
	

	On behalf of:	
	

	Address:
	

	Telephone:
	
	Mobile:
	

	Email:
	
	Date:
	













[bookmark: _Toc232693390]Response to Qualitative Award Criteria

[bookmark: _Toc232693391]Criterion 2 – Field Trials of Sample Tools
	[bookmark: _Hlk157165626]Criterion 2
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	20%
	200
	N/A

	Title
	Operational Quality Field Trials of Sample Tools 
(Tool Ergonomic Assessment, battery usability and Battery Performance Assessment, and Tool-specific Performance Assessments).

	Description
	Donegal County Fire Service will carry out a practical assessment to test the operational effectiveness of the equipment. 
The methodology for this and the scoring system is outlined in Appendix B. 


As per the Section 2.22 of the RFT:
A sample of rescue tools (cutter, spreader, rams, mini-cutter and ancillary items being tendered for) to be provided on request, within 15 working days and to be available for 15 working days to facilitate field trials to Donegal County Council (Fire Service).                                                                                                         
Delivery to: Fire Brigade HQ, High Road, Letterkenny, Co. Donegal. F92 XV50
Sample items must be as per the specification of requirements. 
Copies of technical and compliance certification showing compliance with appropriate standards must be available with the samples provided.










[bookmark: _Toc232693392]Criterion 3 – Warranty
	Criterion 3
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	10%
	100
	N/A

	Title
	Warranty

	Description
	Tenderers must complete the table below and provide documentary evidence of warranty for each item. 


Tenderers’ Response
	Item
	Warranty Offered (Specify in Months)

	Cutters Type A & B (20 Marks)
	

	Spreaders Type A & B (20 Marks)
	

	Ram (20 Marks)
	

	Battery for items above (10 Marks)
	

	220v Battery Charger (10 Marks)
	

	Mini cutter (15 marks)
	

	Mini cutter battery and charger (5 Marks)
	


Warranty offered must be for a minimum of 24 months. 
Any tender offering a shorter warranty period will receive no marks under this criterion.














[bookmark: _Toc232693393]Criterion 4 – Availability of Spare Parts
	Criterion 4
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	10%
	100
	N/A

	Title
	The Tenderer must set out the quality of its proposal for ensuring the availability of all spare parts for the equipment, for the minimum expected lifespan of the equipment (15 years). 

	Description
	The Tenderer should include details of its process and lead times for obtaining spare parts; how it manages this supply chain to ensure parts are delivered on time; and how it manages instances of order delays and parts being out-of-stock.



Tenderers Response:
Please use this free text page(s) (i.e. do not type in the box) for your response. 




















[bookmark: _Toc232693394]Criterion 5 – Green/Environmental Procurement Requirements
	Criterion 5
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	10%
	100
	N/A

	Title
	Green/Environmental Procurement Requirements

	Description
	The Tenderer must provide a detailed narrative to demonstrate how it incorporates environmental and sustainability efficiencies/measures during the build   process. For example:
· Energy optimisation initiatives in the warehouse/premises including rain harvesting, use of PV Panels, fabric of the building including insulation, efficiency of lighting and heating, EV charging capabilities etc.
· Use of recycled and/or recyclable material
· Waste management/disposal/recycling
· Minimisation of waste
· Transport & logistics measures
· Corporate Social Responsibility policies
· Proposed Targets for Environmental Sustainability
· Sustainable purchasing




Tenderers Response:
Please use this free text page(s) (i.e. do not type in the box) for your response. 












[bookmark: _Toc232693395]Criterion 6 – After Sales Support, Service and Maintenance
	Criterion 6
	Weighting
	Maximum Marks
	Minimum Marks Required

	
	10%
	100
	N/A

	Title
	After Sales Support, Service & Maintenance

	Description
	The Tenderer must set out the quality of its proposal in relation to its capacity and capability for the provision of maintenance, repair and technical assistance from its maintenance facilities, and its capacity and capability for repair/maintenance services. 
· Tenderers must have servicing and maintenance facilities in the Republic of Ireland and they must provide details of these maintenance facilities and personnel they have to carry out repairs. 
· The Tenderer should also provide details of the process by which clients’ repair issues are managed from the time a fault is reported through to successful conclusion. 
Sub-contracting after sales support, servicing or maintenance is not acceptable.



Tenderers Response:
Please use this free text page(s) (i.e. do not type in the box) for your response. 














[bookmark: _Toc232693396]Appendix A - Minimum Specification Requirements

Table A.1 Battery Operated Rescue Equipment General Requirements
	Requirement
	Compliant
(Yes / No)
	Comment

	Warranty: The tools and ancillary equipment including batteries shall have a minimum warranty of 2 years.
	
	

	Samples for Field Trials: The tenderer shall, upon request, provide a sample of each rescue tool being tendered. These samples must be:
· Supplied within 15 working days of the request, and
· Made available for a minimum period of 15 working days to facilitate field trials and operational evaluation.
	
	

	Documentation: A full set of documentation shall be provided to include as a minimum: 
· Operating and safety manuals.
· Cleaning, servicing, maintenance, and repair instructions; and
· Relevant risk assessments.
This documentation must be supplied in either Irish or English, or both, and may be provided in hard copy or electronic format.
	
	

	Certification: The tenderer shall provide certification documentation with the tender demonstrating the equipment complies with EN 13204:2025 (and any subsequent amendments).
	
	

	Training: The tenderer shall provide full details on how training will be delivered at station level. 
· A minimum of a half-day training session shall be provided for all operational personnel at each of the 15 stations. 
· Additionally, a minimum of a half-day inspection and light maintenance training shall be provided for Brigade maintenance personnel. 
· All costs associated with the training including labour, travel, and subsistence must be included in the overall supply of the equipment and shall not incur any additional charges.
	
	

	Operating Life: All tools and ancillary equipment must have a minimum operating life of 15 years.
	
	

	Parts & Servicing: The tenderer shall provide a detailed breakdown of all annual and multiannual replacement parts required for servicing, as recommended by the manufacturer. The tenderer shall include the current cost of these parts, along with the estimated total cost of annual servicing over a four-year period. This estimate must include all associated costs, including labour, travel, and subsistence, for servicing the tools at the stations where they will be located – details to be provided.
	
	

	
Ergonomics: The tools shall be designed to deliver a high power-to-weight ratio, ensuring ease of manual handling and operation by a diverse workforce. The tools must incorporate:
· Ergonomically designed handles that allow for secure grip and control in multiple operating positions;
· Capability of operation by one or two personnel; 
· Usability across a range of working heights, including:
· Calf/knee level – e.g. car sill level;
· Waist level – e.g. base of car at A and C post level; and
· Chest level – e.g. top of car at A, B, and C post level.
These design features shall facilitate efficient and safe operation during extrication tasks in varied and challenging environments.
	
	

	CE Marking: All tools and ancillary equipment must be individually CE marked. 
	
	

	Serial Number: All tools and ancillary equipment, including batteries, must be individually marked with a unique traceable serial number.
	
	

	LED lighting: All tools must have integral LED lighting to facilitate use in restricted light conditions with an on/ off switch, the lights must be powered by the main battery.
	
	

	Control Handle and Actuator: The rescue tools shall be equipped with a manual control actuator, which must:
· Be easily accessible in all operating positions; and
· Feature an automatic return-to-neutral position for enhanced safety and control.
The control handle shall:
· Have a minimum length of 75 mm to ensure a full and secure grip for the operator’s hand;
· Be designed for operation from all angles by a single operator, including in confined spaces such as those encountered inside vehicles during road traffic collisions; and
Support use in varied body positions and orientations, ensuring ergonomic and safe handling in challenging environments.
	
	

	Noise: Under full load conditions, the noise emission levels of each tool shall not exceed:
· 75 dB(A) at a distance of 1 metre; and
· 66 dB(A) at a distance of 4 metres
	
	

	IP Ratings: 
· Cutters, Spreaders and Rams, and their associated battery must be suitable for underwater use and have a minimum IP rating of IP57.
· Mini-cutters (including batteries) must have a minimum IP rating of IP54.
	
	

	Auto Stop/Start: Each tool shall be equipped with an auto start/stop function to optimise battery efficiency, to reduce wear on components and support efficient and operational safety. The motor/drive system must automatically stop when:
· The tool is not in use, or
· The tool has reached its maximum operating pressure.
The tool must automatically restart when the control handle is turned again, allowing seamless reactivation by the operator without additional steps.
	
	



Table A.2 Battery Requirements
	
Requirement
	Compliant
(Yes / No)
	Comment

	Standards: All batteries must conform to EN 62133-2:2017 and A1:2021 (or any subsequent amendments of same).
	
	

	Interfacing:  The batteries shall meet the following minimum requirements:
· They must fit securely to the tool to prevent accidental separation or damage during operation;
· They must be easily connectable to the tool by a single operator wearing fire-fighter gloves;
· Their replacement must not cause any unintended movement of the tool’s jaws, arms, or rams (as applicable); and
· They must be capable of interfacing with diagnostic software to provide detailed information on the battery’s health status.
	
	

	Status: Each battery must be equipped with a visual charge status indicator that is clearly visible and readable while the battery is connected to the rescue tool, and while the battery is connected to the charger.
	
	

	Rating: 
· Batteries for Cutters, Spreaders and Rams must be Lithium-Ion type with a minimum capacity rating of 8 ampere-hours (8Ah).
· Batteries for Mini-cutters must be Lithium-Ion type with a minimum capacity rating of 5 ampere-hours (5Ah).
	
	

	Charging Time: Batteries must be capable of reaching a full charge from a fully discharged state within a maximum of 240 minutes. This requirement applies when using either a mains-powered AC charger, or a vehicle-powered DC charger.
	
	

	Continuous Charging: The equipment must be designed to remain on continuous charge without risk of damage to either the battery or the charger.
	
	

	Durability: All batteries must be capable of withstanding a minimum of 500 full charge-discharge cycles (i.e., from fully discharged to fully charged) without significant degradation in performance or capacity. Tenderers must provide verifiable documentation from the battery manufacturer confirming compliance with this requirement, including test data or certification where available.
	
	

	Supply Voltage: Battery chargers must be available for use with a standard mains socket supply (220–240V AC). Chargers must provide clear indication of the battery’s state of health both visually on the battery unit, and via diagnostic software, enabling detailed performance monitoring and maintenance planning.
	
	

	On-board charging: The on-board charger shall meet the following criteria:
· Operate at 24V DC;
· Include a battery level indicator for real-time monitoring;
· Be supplied with all necessary ancillary equipment, including a sufficient length of charging cable;
· Be suitable for mounting within a fire appliance;
· Be capable of charging a minimum of one battery;
· Include suitable inline surge protection fuses that are easily accessible for replacement,
or alternatively, be fitted with a resettable circuit breaker that is easily accessible for resetting.
	
	

	Availability: 
Replacement batteries must be available for 15 years.
	
	



Table A.3 Cutter – Type A
	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The cutter must have a minimum jaw opening of 180mm, as classified under EN 13204:2025 (or any amendments to same).
	
	

	Performance: The rescue cutter must meet a minimum cutting performance classification of 1K-2K-3K-4K-5K in accordance with EN 13204:2025 (or any amendments to same). 
	
	

	Weight: The cutter, including the connected battery, shall have a maximum total weight of 25.0kg.
	
	

	General: The design and materials used in the manufacture of the cutting blades must ensure optimum cutting performance is maintained over repeated use, while also providing high durability and resistance to wear. Blades should be engineered to withstand the demands of frequent operational deployment without significant loss of effectiveness.
	
	



Table A.4 Cutter – Type B
	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The cutter must have a minimum jaw opening of 200mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The rescue cutter must meet a minimum cutting performance classification of 1K-2K-3K-4K-5K in accordance with EN 13204:2025 (or any amendments to same). 
	
	

	Weight: The cutter, including the connected battery, shall have a maximum total weight of 25.0kg.
	
	

	General: The design and materials used in the manufacture of the cutting blades must ensure optimum cutting performance is maintained over repeated use, while also providing high durability and resistance to wear. Blades should be engineered to withstand the demands of frequent operational deployment without significant loss of effectiveness.
	
	



Table A.5 Spreader – Type A
	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The spreader must have a minimum opening width of 725mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The spreader must meet or exceed the following performance criteria, in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force: Greater than 40kN, measured 25mm from the tips and greater than 320kN at the steel tips.
· Pulling Force: Greater than 50kN.
· Pulling Distance: Greater than 610mm.
· Squeezing Force: Greater than 100kN.
	
	

	Weight: The spreader, including the connected battery, shall have a maximum total weight of 22.0kg
	
	

	General: The spreader must be designed to meet the following operational and functional criteria:
· Accessory Compatibility: The tool must be designed to allow for the secure attachment and use of accessories such as chains or other approved fittings, enhancing its versatility in rescue operations.
· Tip Grip Performance: The spreader tips must be engineered to provide effective grip on a wide range of surfaces during spreading operations, ensuring stability and control under load.
· Tip Profile for Access: The tip design must be suitably fine and tapered to allow insertion into narrow gaps enabling effective initial access in confined or obstructed spaces 
· door opening tips to be included in price along with standard tips.
	
	



Table A.6 Spreader – Type B
	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: The spreader must have a minimum opening width of 800mm, as classified under EN 13204:2025 (or any amendments to same)
	
	

	Performance: The spreader must meet or exceed the following performance criteria, in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force: Greater than 60kN, measured 25mm from the tips and greater than 450kN at the steel tips.
· Pulling Force: Greater than 60kN.
· Pulling Distance: Greater than 645mm.
· Squeezing Force: Greater than 110kN
	
	

	Weight: The spreader, including the connected battery, shall have a maximum total weight of 25.0kg
	
	

	General: The spreader must be designed to meet the following operational and functional criteria:
· Accessory Compatibility: The tool must be designed to allow for the secure attachment and use of accessories such as chains or other approved fittings, enhancing its versatility in rescue operations.
· Tip Grip Performance: The spreader tips must be engineered to provide effective grip on a wide range of surfaces during spreading operations, ensuring stability and control under load.
· Tip Profile for Access: The tip design must be suitably fine and tapered to allow insertion into narrow gaps enabling effective initial access in confined or obstructed paces 
· door opening tips to be included in price along with standard tips.
	
	



Table A.7 Telescopic Ram
	[bookmark: _Hlk204344883]
Requirement
	Compliant
(Yes / No)
	Comment

	Stroke and Dimensions:
The ram shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· Total stroke: Greater than 700mm
· Retracted length: Less than 600mm and less than the maximum opening of the proposed spreader.
· Extended length: Greater than 1200mm
(This may be achieved using extension poles)
	
	

	Performance: The ram shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· Spreading Force:
· First stage: Minimum 100kN
· Second stage: Minimum 60kN
	
	

	General: The ram must be designed for safe and effective use in conjunction with compatible accessories, including but not limited to ram supports and sill clamps.
	
	

	Weight: The ram including the connected battery, shall have a maximum total weight of 22.0kg
	
	




Table A.8 Mini Cutter
	
Requirement
	Compliant
(Yes / No)
	Comment

	Opening: Must have a minimum cutter opening of greater than 50mm under EN 13204:2025 (or any amendments to same).
	
	

	Performance: The cutter shall meet the following minimum performance criteria in accordance with EN 13204:2025 (or any amendments to same):
· A minimum cutting performance classification of 1C-2C-3B in accordance with EN 13204:2025 (or any amendments to same).
	
	

	Accessories: The Mini Cutter must be supplied with two suitable batteries, a mains charger and charging lead, if battery powered.
	
	

	Weight: The tool, including any connected battery / drive unit, shall have a maximum total weight of 12.0kg.
	
	

	Battery Charge: If battery powered, the battery must be capable of at least 50 cuts.
	
	



Table A.9 Ram Support
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Requirement
	Compliant
(Yes / No)
	Comment

	Performance: Each ram support must be specifically designed to maximise and evenly distribute the load exerted by the ram, particularly during cross-ramming techniques.
	
	

	Size: Each ram support shall have a maximum footprint of 500 mm x 500 mm with a maximum height/depth of 200 mm.
	
	

	Weight: Each ram support should weigh no more than 15kg
	
	

	Gripping surface: Each ram support must be fitted with a suitable gripping surface to ensure secure anchoring and stability during operation.
	
	

	Material & Finishing: Each ram support must be manufactured from a suitable high-strength metal or alloy to ensure structural integrity under load and treated for corrosion resistance, preferably by zinc coating. If painting is used as the protective method, the supports must be rust-proofed prior to painting to ensure long-term durability.
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Assessment Process
This evaluation will be conducted by a minimum of 5 Donegal County Council (Fire Service) operational personnel, who will assess the performance of the proposed equipment through a series of controlled, real-world tests. Marks will be awarded based assessment criteria which include Tool Ergonomic Assessment, Battery Usability and Battery Performance Assessment, and Tool-specific Performance Assessments. Tenderers should ensure that their equipment is suitable for use in the conditions specified and that all required components are provided for testing.

FORMAT
The practical evaluation will be conducted by an evaluation panel from Donegal County Council (Fire Service), including Senior Fire Officers and Station Officers, will facilitate and oversee the evaluation. The assessment will take place at Dungloe Fire Station, with the tenderers required to provide a full set of their proposed battery-operated rescue equipment for evaluation.
INSTRUCTIONS	
· Tenderers must ensure that the battery-operated hydraulic rescue equipment provided for evaluation is what they submitted in their bid. One full set of equipment must be supplied.
· Donegal County Council (Fire Service) will not incur any costs for the equipment or accessories used during the practical evaluation.
· The practical evaluation is mandatory for the assessment process. Failure to provide the equipment will result in disqualification.


ASSESSMENT
The assessment will cover the following components:

1. Tool ergonomic assessment.
Each tool will be evaluated by one and two personnel to assess:
· Handling: The ease of handling, including grip, balance, and positioning of the tool handles.
· Ease of Operation: Tools will be lifted to various heights (calf, waist, and shoulder) and rotated through 90°, simulating realistic usage to assess comfort and ease of operation.
· Controls: Access to and ease of use of the tool’s controls during operation.

2. Battery usability & battery performance assessment
Each tool will be tested in realistic operational scenarios to simulate usage under load. This includes:
· Battery Replacement: Swapping the battery while the tool is under load.
· Endurance Test: A random tool from each set will be operated (opening and closing) for 20 minutes without load to assess operational stability and battery life.

3. Tool-specific performance assessments
Cutters:
· Cut rear door hinges (4 activities)
· Cut A posts (2 activities)
· Cut B posts (2 activities)
· Cut roof bars for roof flap simulation (2 activities)
· Relief cut at the base of A posts (2 activities)

Spreaders:
· Lift a vehicle by 150mm (2 activities)
· Crimp front wings (2 activity)
· Spread front door hinges (4 activities)
· Open bonnet or boot (1 activity)

Ram:
· Position horizontally between A and B post and extend (2 activities)
· Position between C and B post and extend (2 activities)
· Extend between centre console and A post (2 activities)
· Perform dashboard roll at base of B post (1 activity)














Marking Sheet for Field Trial of Sample Tools Assessment

	Assessment Criteria
	Max Marks
	Score
	Comments

	1. Tool Ergonomic Assessment
	
	
	

	Grip and Handle Positioning
	15
	
	

	Balance of Tool
	15
	
	

	Access to Controls
	10
	
	

	Ease of Operation at Calf Height
	10
	
	

	Ease of Operation at Waist Height
	10
	
	

	Ease of Operation at Shoulder Height
	10
	
	

	Comfort of use over extended periods
	10
	
	

	2. Battery Usability & Performance Assessment
	
	
	

	Ease of Battery Change
	10
	
	

	Tool Endurance (20 min operation)
	20
	
	

	3. Tool-Specific Performance Assessments
	
	
	

	Performance of Cutters (all activities)
	25
	
	

	Performance of Spreaders (all activities)
	25
	
	

	Performance of Ram (all activities)
	20
	
	

	Performance of Mini cutter
	20
	
	

	Total
	200
	
	

	[bookmark: _Toc188005661]Assessor Name
	

	Assessor Rank
	

	Date
	

	Weather Conditions During Testing
	

	Additional Equipment Used (e.g., PPE)
	

	Signature
	




Explanation of Marking Scheme for Field Trial of Sample Tooles
A tool will achieve maximum marks by excelling in all aspects of the evaluation criteria. 
· During the Tool Ergonomic Assessment, the tool should demonstrate comfort during extended use, areas such as grip, balance and ease of control across various heights will be considered. 
· Battery Usability & Battery Performance Assessment, the tool must efficiently balance battery performance and power, lasting the full 20-minute test. The efficiency with which a battery change can be performed will assessed. 
· During the Tool-Specific Performance Assessments, the tool must perform all tasks listed, such as cutting and spreading, without issue.
A tool will receive minimum marks if it fails to meet the basic requirements in any category.
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