COMPLIANCE TO SPECIFICATION 

DN150 (6 inch) Trailer Mounted Mobile Dewatering Pumps – Diesel Powered

PLEASE NOTE: If you are offering different model PUMPS you must fill out a separate compliance form for each PUMP offered.

Company tendering: _________________________ (insert name of company)

	Description
	Please complete in respect of your offer
	Confirm your level of compliance with any additional remarks / notes necessary
	For OPW use only

	1. General:
DN150 (6 inch) Trailer Mounted Diesel engine powered mobile dewatering pump. 


Minor variances to the specifications may be taken into account and considered at competition assessment stage.
This must be solely at the discretion of the evaluation committee.

Note: All equipment must be supplied with Manufacturer approval and compliance.

	
Confirm: 
Make: 
Model: 

Confirm: 

	
	

	2. Duty:
All pumps must be capable of dry priming to 7-metre suction lift.

The pump must be capable of operating in a range of conditions and be capable of pumping unscreened raw sewage water and water with small debris. 

The pump must be capable of running dry or ‘snoring’ for long periods of operation. 

The pump will be used in areas from sea level up to 100m above sea level.



	
Confirm:

Confirm:



Confirm:


Confirm:
	

	

	3. Engine:
Pump must be diesel engine powered and comply with Stage 5 emissions.

The pump must have a maximum noise level in operation of 75 dB (A) sound pressure at 10 metres.

	
Confirm:

Confirm: 
	

	

	4. Performance:
Minimum delivery of 100l/s @ 10m Total Dynamic Head (THD) @ 1600-1900 rpm.

	
Confirm:
	


	

	5. Fuel:
The pump must be capable of operating continuously as per performance criteria as outlined in section 4 – Performance for a minimum of 24 hours (from its in-built fuel tank).

The pump must be capable of running on 100% HVO.

	
Confirm:



Confirm:
	

	

	6. Weight:
The pump must have an operating weight ≤ 2,200kg (including full tank of fuel).

	
Confirm:
	
	

	7. Impeller:
The pump must have a screw type impeller or similar which must be clog resistant and must have free passage of 65mm.

	
Confirm:
	
	

	8. Enclosure:
The pump must be an all enclosed, trailer-mounted unit and must be manufactured from hot dip galvanised steel.

· Lockable with locks and keys provided.
· Fitted with central lifting point
· Fitted with forklift lifting slot
· Fully bunded design 
(Please note the pumps will be stored outdoors and must be sufficiently weather resistant to cope with this environment.)

	
Confirm All:
	
	

	9. Ports:
The suction and discharge ports must be DN150/6” in size. 

The suction and discharge ports must be mounted to the rear of the pump/trailer (side suction and/or discharge not accepted). 
	
Confirm:

Confirm:

	
	

	10. Controls:
The pump must be fitted with electric (12V) start and supplied with a 12V battery.
Solar panels must be installed to ensure 12V battery remains charged during long periods of down time. 

The pump must be fitted with a key controlled control panel, which will display all operating information and capable of being programmed to operate the automatic level switching.

The pump must be fitted with an hour-meter.

The pump must be fitted with a main battery isolator/switch.

The pump must be fitted with an OE telematics system to include the following;
The pump must have the capability to be controlled and monitored remotely. The system must monitor and log operational information and store this information on a hosted secure server for a minimum of 5 years. 

The system must allow the user to set up alarm notifications via text or emails. 

The system must monitor and record the following data:
· Geo-location 
· Ignition on/off
· Outlet pressure
· All available engine data
· Fuel level status 
· Engine speed 

The system must allow the user to control the following:
· Stop/start
· Change to auto-mode for float control
· Speed control 
	
Confirm:

Confirm all equipment:


Confirm:



Confirm:

Confirm:

Confirm:





Confirm:


Confirm All:







Confirm All:



	



	

	11. Level Switching:
The pump must be fitted with automatic level switching (The engine must start and stop automatically as required) and provided with suitable level probes for the purpose.

	
Confirm:
	
	

	12. Pipe Connections:
Bauer or similar quick release for all connections and suction and discharge pipework.

	
Confirm:
	
	

	13. Pipework:
The pump must be supplied with the following pipes and fittings:
· [bookmark: _Hlk78301928]12m of reinforced suction pipe in 4 x 3m lengths.
· The pump must be supplied with 3 x 45deg, 2 x 90 bends and 1 x suction strainer
· 20 metres of lay flat delivery pipe DN150 in 10m long sections and must be coupled using a quick release system, Bauer or similar.

	
Confirm all equipment: 
	

	

	14. Trailer Spec:
A galvanised, steel-bodied, twin axle, 02 type, van/4x4 drawn trailer. The pump must be permanently fixed to the trailer.
· Weight
· The trailer must be capable of carrying a payload of minimum 2.7 tonnes and maximum 2.9 tonnes. 
· The trailer un-laden weight must not exceed 650kg. 
· The trailer must have a Design Gross Vehicle Weight of ≤3,500kg. 
· Body Size/Type:
· The minimum internal dimension acceptable must be suitable to accommodate the permanent storage of the pump and pipework. 
· Front and rear mounted height adjustable “prop-stands” must be fitted (total of 4).  
· Storage: 
· The trailer must incorporate storage compartments for the pipework and fittings as per section 13-Pipework.



· Hitch:
· The trailer hitch must be of the standard “ball” type. The trailer must be supplied with a heavy-duty fully adjustable jockey wheel.
· Axles:
· The trailer must be supplied with new 4/5 stud commercial type axles which will be spring suspended and braked.  

· Wheels/Tyres:
· The trailer must be fitted with low profile new tyres e.g.: 185/70 R13 or similar. Tyres supplied must be new (not remoulds). The trailer must be supplied with a spare wheel and tyre.
· Mudguards:
· The trailer will have plastic/metal rear mudguards fitted. 
· Lighting:
· Full LED road lighting with protective guarding must be fitted to comply with current regulations.
· Two “strobe” type flashing beacons shall be fitted to the tailgate/rear bumper. They may be wired via the tail-lamp circuit but must be fitted with a separate weatherproof switch located at the rear of the trailer to allow the beacons to be switched off when not in use.
· Brakes:
· The trailer will be fitted with an “over-run” (inertia) type braking system operating on both axles. 
· The braking circuit should incorporate a “breakaway” system that applies the trailer brakes should it become detached from the towing vehicle.
· Speed Rating:
· The trailer must be capable of being towed at ≥ 80km/hr.
· Compliance:
· The trailer will comply with all National and EU regulations and Legislation pertaining to its construction and its use. 
	
Confirm:


Confirm:

Confirm:
Confirm:


Confirm:


Confirm:


Confirm:





Confirm:



Confirm:



Confirm:




Confirm:

Confirm:

Confirm:





Confirm:

Confirm:



Confirm:

Confirm:

	
	

	15. Conformity:
The EU Declaration of Conformity certificate must be provided.  

The pump and trailer must comply with current Irish and EU legislation and comply with relevant EU machinery directives.

	
Confirm:


Confirm:
	



	

	16. Warranty:
A minimum 2 years parts and labour warranty must be provided.

	
Confirm: 
	

	

	17. Finish:
The pump must be rustproofed and have a durable painted finish in the manufacturers original colour. 
	
Confirm: 

	

	

	18. Manuals/Documentation:
The following literature must be supplied:-

1 x Operator’s Manual.
1 x Spare Parts Manual 
1 x Workshop Manual

in both electronic and hard copy versions.

	
Confirm:
	

	

	19. [bookmark: _GoBack]Training:	
Two Familiarisation Training Sessions (up to 10 people per session) must be included for at each of the nominated local authority depots (Sligo / Galway City / Mallow / Cavan / Portlaoise). 

The training should be in-depth, focusing on correct set up and running of the pump.

Service and maintenance training (given by dedicated trainer) for up to 10 mechanical maintenance personnel must also be provided.

The training content recorded in writing, signed by the person giving the training and recorded on a signed attendance sheet. 

Training certificates must be issued to successful attendees. 

A video containing the set up and operation must be provided in mp4 format.
	
Confirm:



Confirm:


Confirm:


Confirm:


Confirm:

Confirm:

	














	

	20. Delivery:
Delivery to a nominated depot.

Tenderers must state the best available lead delivery time on the pricing schedule.
Delivery lead-time no longer than 16 weeks from date of order.

	
Confirm:

Confirm lead time for delivery:

Confirm:
	
	

	21. Product Information:
The specification, technical data information and after sales terms and conditions in the catalogues and brochures provided for reference purposes, will be considered as being representative of the pump offered.

Where a particular specification or terms and conditions, which are superior to normal, are confirmed as being offered in the “compliance to specification” section, these must be deemed to take precedence over those normally available.

The pump curve data sheet must be provided to demonstrate the pump meets the specification, including the total dynamic head and engine operation characteristics at flow rates outline in section 4-Performance. 

Full dimensional drawings for pump and trailer must be provided.

	
Confirm:



Confirm:




Confirm:



Confirm:
	











	

	22. Supplier After Sales Service:
An estimated run time of 500 hours per annum for each pump is assumed.

Each pump supplied, for a period of five years after delivery, must be maintained in accordance with the following:
• All routine Servicing according to Manufacturer’s Requirements, including    
   oils and filters. 
· Pumps must be serviced annually regardless of hours. This service must take place between July 1st and September 30th. 
· As part of the annual service, functional checks must be carried out on the pump to ensure it is ready for deployment in emergency situation. 
• Provision of all records for servicing and repair to the relevant local authorities. 


The contractor must have workshop facilities on the island of Ireland. 

Pumps supplied under this contract must be reliable in use and have reasonable servicing, maintenance and inspection requirements for their period in the client fleet.

Where an individual pump requires additional time out of service due to a high incidence of mechanical or system defects (1 week downtime), this will be brought to the attention of the Contractor who will arrange an appropriate detailed inspection and full rectification of all faults with the pump.

In the event of persistent failures within the first 24 months from delivery of that pump, the client reserves the right to reject it and receive in its place a suitable replacement pump of similar type and specification, and of similar age and hours worked.

The contractor will be responsible to the client for ensuring that all appointed dealers work to the highest standards of technical expertise for all maintenance and repair work carried out to machines delivered under this contract.

	




Confirm:

Confirm:

Confirm:

Confirm:



Confirm:

Confirm:



Confirm: 




Confirm:




Confirm:



	

























	




