Appendix 1E – Environmental Technical and Professional Ability (Self-Declaration):
Motorcycle Suits, Motorcycle Protective Clothing, Motorcycle Footwear and Motorcycle Helmets

Appendix 1E – Environmental Technical and Professional Ability (Self-Declaration):
The successful Tenderer shall be required to provide on request prior to contract award, and at any time over the term of the Contract, the following assurances that over the term of the contract Goods are manufactured in accordance with best practice environmental standards and that environmental impacts under this competition are kept as low as possible.
By submitting a Tender response for this competition, Tenderers confirm that, prior to contract award, they will obtain and hold the required Certificate(s) demonstrating compliance with all elements as specified under section 3.2.B(v) of the RFT.  Formal Certificate(s) for tests carried out by an accredited independent test-house to this effect will be requested from the preferred Tenderer prior to the award of (and shall be a condition of) any Contract awarded as part of this RFT.  
The successful Tenderer will, during the term of the Contract, be required to:  
a) immediately advise the Contracting Authority and any interested party of any material change to its manufacturers and / or their manufacturers’ subcontractors and fabric producers; 
b) produce proof of test reports upon request over the term of the contract.
Environmental Technical and Professional Ability (Self Declaration):
	
	Details
	Declaration
	Comment

	
	
	Yes
	No
	

	1
	Substances on REACH candidate list:

	
	Does the Tenderer confirm that all Goods will conform with the Substances on REACH candidate list;
	
	
	

	2
	Substances to be tested for on the final product:

	
	Does the Tenderer confirm that the final supplied Goods will not contain the substances listed in GPP ANNEXES (Annex 1) at greater than the individual or sum total concentration limits;
	
	
	

	3
	Durability standards:

	
	Does the Tenderer confirm that the final textile Goods conform with the relevant durability requirements identified in GPP ANNEXES (Annexes 2 and 3);
	
	
	


See Attached (GPP ANNEXES 1,2 &3 )
Tenderers shall confirm that all information provided is true and complete.  By signing this self-declaration, tenderers acknowledges that incomplete or untruthful information automatically leads to exclusion from this procurement procedure or will lead to the revocation of a contract award.
The Contracting Authority reserves the right to verify the above information at any time over the term of the contract.  The verification will be carried out either by requesting the submission of documents confirming the information provided, or by answering further questionnaires. 
Hereby it is confirmed that the requirements are met:

Signed: 									Witness:

Date:

GPP Annexes 1, 2 and 3:

Annex 1: Final product substance restrictions
	Substance group
	Restrictions that apply
	Concentration limits
	Test method

	1.1 Azo dyes 
Applicability: Clothing containing acrylic, cotton, polyamide and wool
	Azo dyes that may cleave to aromatic amines that are known to be carcinogenic must not be used (see the list in Appendix 2 of the EU Ecolabel criteria[footnoteRef:1]). A limit value for aryl amines will apply for the purpose of testing the final product. [1:  Commission Decision 2014/350/EU on the EU Ecolabel Criteria for Textile Products, as amended by Decision 2017/1392] 

	30 mg/kg for each amine
	EN 14362-1 and 3 or equivalent.

	1.2 Formaldehyde Applicability: All clothing and interior textiles containing natural fibres
	The following limit values apply to residual formaldehyde on the finished product:
- Products for babies and children under 3 years old
 - All other products 

Improved performance for skin contact garments could additionally be requested as an award criterion.[footnoteRef:2]  [2:  There may be a trade-off in terms of the quality and durability of stay-press garments, particularly where garments are to be subject to high temperature washing.] 

The following requirement can be applied as a comprehensive criterion for interior textiles only:
 - Emissions from the final product 
	


16 ppm

75 ppm







0.1 mg/m3
	


EN ISO 14184-1 or equivalent.






EN 16516 and EN ISO 14184-1 or equivalent

	1.3 Auxiliaries 
Applicability: All products
	The following substances must not be present on the final product: 
- Nonylphenol
 - Octylphenol
	100 mg/kg sum total
	Solvent extraction followed by HPLC/MS

	
	The following substances must not be present on the final product: 
- Nonylphenol ethoxylates
 - Octylphenol ethoxylates
	100 mg/kg sum total
	ISO 18254

	1.4 Coatings, laminates and membranes 
Applicability: Where incorporated into textile structure





	Coatings, plastisol printing, laminates, membranes and plastic accessories must not contain the following phthalates: 
- DEHP (Bis-(2-ethylhexyl)-phthalate) - BBP (Butylbenzylphthalate) 
- DBP (Dibutylphthalate) 
- DMEP (Bis2-methoxyethyl) phthalate
 - DIBP (Diisobutylphthalat) 
- DIHP (Di-C6- 8-branched alkyphthalates) 
- DHNUP (Di-C7- 11-branched alkylphthalates) 
- DHP (Di-n-hexylphthalate)
	Sum total 0.10 % w/w
	EN ISO 14389 or equivalent.



Annex 2: Production process substance restrictions
	Substance group
	Restrictions that apply
	Verification requirements

	1.1 Dyes and pigments 

	The following dyes and pigments must not be used in textile production: Acid Red 26, Direct Black 38, Disperse Blue 1, Basic Red 9, Direct Blue 6, Disperse Orange 11, Basic Violet 14, Direct Red 28, Disperse Yellow 3, Pigment Red 104, Pigment Yellow 34 
	Site audit at which the dyes used are to be identified. 

	2.2 Auxiliaries 
	The following substances must not be used in textile production: - bis(hydrogenated tallow alkyl) dimethyl ammonium chloride (DTDMAC) - distearyl dimethyl ammonium chloride (DSDMAC) - di(hardened tallow) dimethyl ammonium chloride (DHTDMAC) - ethylene diamine tetra acetate (EDTA) - diethylene triamine penta acetate (DTPA) - 4-(1,1,3,3-tetramethylbutyl)phenol - 1-Methyl-2-pyrrolidone - Nitrilotriacetic acid (NTA) 
	Site audit at which the chemical used as auxiliaries are to be identified. 

	2.3 Bleaching 
	Chlorine based bleaches must not be used for the bleaching of any yarns, fabrics or knitted panels. Site audit at which the bleaches used are to be identified.
	Site audit at which the bleaches used are to be identified.

	2.4 Water, stain and oil repellent treatments 
	Core requirement: Long chain (≥C5) perfluoroalkane sulfonic acids or sulfonates (PFSA) and (≥C7) perfluoroalkyl carboxylic acids or carboxylates (PFCA) substances must not be used. 
Comprehensive requirement: Fluorinated water, stain and oil repellent treatments must not be used, unless these functions are required in combination. 
In addition, for both core and comprehensive criteria the garment(s) must be tested for durability (see Criterion 3.1) 
	Site audit at which the repellents used for the finishes are to be identified.

	2.5 Waterproof membranes
	Fluoropolymer membranes and laminates used for outdoor clothing must not be manufactured using perfluorooctanoic acid (PFOA) or any longer chain fluorinated surfactants.
	Site audit of the membrane/laminate supplier or documentation from a government regulatory body.

	2.6 Flame retardants
	Core requirement: The following flame retardants must not be used: - HBCDD 
– Hexabromocyclododecane 
- DecaBDE 
– Decabromodiphenyl ether 
- TEPA – Tris(aziridinyl) phosphinoxide
- TRIS – Tris (2,3 dibromopropyl) phosphate 
- TCEP – Tris (2,chloroethyl)phosphate 
- Paraffin, C10-C13, chlorinated (SCCP) 
Comprehensive requirement: Where fire protection is required the fabric must be tested to ensure it provides a high level of durability (see Criterion 3.1)
	Site audit at which the flame retardants used are to be identified.





Annex 3: Durability tests 
1.1 Indicative applicability of the textile durability performance requirements 
[image: ]
1.2 Performance benchmarks and test methods
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