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Independent Technical Assessment for: 
Irish Defence Forces Motorcycle Suits, Motorcycle Protective Clothing, Motorcycle Footwear and Motorcycle Helmets


Part 1 - Anonymity – All Products

Pass = Tender samples submitted with Unique Anonymous Tenderer ID, sample / product packaging must be marked only with this information item reference / details and size. 

Fail = where Tenderers samples are marked with company references that restricts an independently / anonymously assessment. 

NOTE: if any submitted samples do not comply with the anonymity requirements, then the Tenderer’s samples may not be assessed and the Tenderer may automatically fail the technical assessment and be eliminated from the competition.



Part 2 - Compliance to Goods Specification Requirements

Each individual tender sample will be assessed and scored against each of the goods specification requirements as per the below:

1. Performance & Conformity Requirements. This requirement includes providing all of the detailed documentation listed in the specification.

a) Pass = compliance with all elements, and evidence of compliance (documents) is provided including product certificate
b) Conditional Pass = compliance with all elements, evidence of compliance (documents) is provided except for the product certificate with a confirmation statement that the manufacturer will provide this prior to contract signing.
c) Fail = does not comply with all elements, or evidence of compliance (documents) is not provided

2. Mandatory Product Requirements
a) Pass = compliance with all elements
b) Fail = does not comply with all elements

NOTE: where applicable and included within a product specification, compliance with desirable product requirements will be reviewed for reference only and will not be scored or assessed.

3. Detailed Product Requirements - Impact Protectors
Impact protectors must be provided and be compliant with all of the detailed requirements in the specifications:

a) Pass = compliance with all elements
b) Fail = does not comply with all elements

This assessment criteria applies to the following specifications ONLY:
(1) DF-1306-W-JKT Undersuit Motorcycle Jacket
(2) DF-1306-W-TRS Undersuit Motorcycle Trouser
(3) DF-1556-W-JKT Motorcycle Jacket (Black)
(4) DF-1556-W-TRS Motorcycle Trouser (Black)
(5) DF-1558-W-JKT Motorcycle Jacket (Alternative Colour)
(6) DF-1558-W-TRS Motorcycle Trouser (Alternative Colour)






4. Detailed Product Requirements
a) Pass = compliance with all elements
b) Conditional Pass = elements provided but may not exactly comply with the detailed requirements
c) Fail = does not comply with all elements

This assessment criteria applies to the following specifications ONLY:
(1) DF-1559-W-JKT Motorcycle High Viz Jacket 
(2) DF-1562-W-GL-EOH Escort of Honour Motorcycle Gloves
(3) DF-1564-W-BO DR Motorcycle Boots
(4) DF-1564-W-BO-EOH Escort of Honour Motorcycle Boots
(5) DF-1565-W-H-EOHDR Escort of Honour & DR Helmet
(6) DF-1565-W-H-EOHO Escort of Honour Officer Helmet

5. Size Range
a) Pass = confirmation of provision of mandatory minimum size range 
b) Fail = does not comply with mandatory minimum size range

NOTE: where applicable and included within a product specification, compliance with desirable size range will be reviewed for reference only and will not be scored or assessed.

6. Labelling & Traceability Requirements
a) Pass = compliance with all elements
b) Fail = does not comply with all elements

NOTE: Packaging Requirements are not assessed as part of the technical evaluation but will be a requirement for the successful Tenderer to comply with for the contract. 

Results: each sample must pass all Part 2 assessment criteria detailed above or will be deemed to have failed the technical evaluation under Part 2, and will not be progressed to Part 3 evaluation.  Therefore, the Tenderer may be eliminated from the competition. 


Part 3 – Sample Production / Manufacturing Quality

General sample manufacturing quality
Each individual tender sample will be assessed and scored for manufacturing quality as per the below:

a) Pass = not more than 0 major & 2 minor failures 
b) Conditional Pass = not more than 0 major and 3-4 minor failures. If successful, conditional pass subject to improvements in 2nd stage samples achieving pass under same criteria.
c) Fail = 5+ minor or 1 major failures 

NOTE: industry standard major/minor criteria will be applied, based on product types, as follows: 

A major failure is defined as something which would impact the wearability, overall look or safety of a product. For example, missed stitches or broken thread that would result in stitching/seams coming undone, damage or staining to the outside of the fabric, damaged/broken or non-working fastenings.

A minor failure would not impact the wearer ability, overall look or safety of a product but would need to be improved for production. For example, loose threads, mark or stains to fabric on the inside of the garment, marks to outside of an item (that easily rub off).

Results: each sample must pass the Part 3 assessment criteria detailed above or will be deemed to have failed the technical evaluation and the Tenderer may be eliminated from the competition.
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