RFQ Response
Supply, Delivery, Installation and Commissioning of an Automated Packing Machine for Fresh Herb and Salad Products
Insert details of company submitting tender response:
	Company Name 

	

	Address

	

	Contact Details 

	

	VAT Number Details
 
	

	Tax Clearance certificate Available (Yes/No)
	

	Insurance Available (Yes/No)
	



	
Signature 


	




Technical Specification
Tenderers must complete the technical response column and confirm whether each requirement is fully met, partially met or not met. Equivalent or superior solutions will be considered where they meet the functional requirement.

	Requirement

	Minimum specification
	Tenderer response guide
	Tenderer response

	Quantity
	One complete automated packing machine / packing line solution.

	Tenderer to confirm.
	

	Products
	Fresh culinary herbs, baby leaf greens and salad products in loose, bunched or tray/pack presentation as relevant to production requirements.
	Tenderer to confirm product suitability and list any exclusions.
	

	Pack style
	Horizontal flow-pack / pillow-pack style, or an equivalent sealed pack format suitable for fresh herbs and salad products.

	Tenderer to describe pack style.
	

	Pack size range
	Must be capable of handling product dimensions broadly covering approximately 250 x 120 x 90 mm, 320 x 120 x 50 mm, 320 x 180 x 50 mm and 280 x 140 x 20 mm, or equivalent product/pack sizes required by the purchaser.

	Tenderer to confirm minimum and maximum pack dimensions.
	

	Output speed
	Target output of approximately 50-60 packs per minute where product, film and operating conditions permit. Tenderer must state guaranteed and maximum operating speeds for the proposed products.

	Tenderer to state speed assumptions.
	

	Film / packaging compatibility
	Machine must be suitable for solderable food packaging films used for fresh produce, including BOPP or equivalent film in the approximate range of 20-30 microns, and should support lower-impact or recyclable packaging materials where technically feasible.

	Tenderer to confirm compatible materials.
	

	Sealing performance
	Reliable longitudinal and cross-seal performance suitable for fresh produce packs, with adjustable temperature, pressure and speed settings as appropriate.

	Tenderer to describe sealing system.
	

	Product detection
	Product detection in the sealing/cutting area suitable for light, leafy or irregular herb products to reduce product damage, mis-seals and downtime.

	Tenderer to describe detection method.
	

	Coding / traceability
	Integrated or compatible date/batch coding system, with bracket/mounting and interface where required.
	Tenderer to describe coder and consumables.
	

	Changeover
	Fast and repeatable changeover between relevant pack sizes and products, with stored recipes or equivalent settings where available.
	Tenderer to describe changeover process/time.
	

	Controls and reporting
	Clear operator interface; ability to store settings; preference for manuals, alarms, efficiency data or production metrics where available.

	Tenderer to describe controls.
	

	Construction and hygiene
	Food-production suitable construction, corrosion-resistant materials in relevant areas, cleanable design and accessible components for maintenance.

	Tenderer to confirm materials and hygiene features.
	

	Safety and compliance
	CE marked or equivalent compliant equipment, with declaration of conformity, guarding, emergency stops, risk assessment and operating manuals.

	Tenderer to provide evidence.
	

	Utilities
	Tenderer must state all electrical, compressed air, water, extraction, network, space, drainage and environmental requirements before contract award.

	Tenderer to list utility requirements.
	

	Layout and footprint
	Tenderer must provide a proposed layout drawing/footprint and confirm handedness/product flow suitable for the site.

	Tenderer to provide layout.
	

	Delivery and installation
	Tender price must include delivery, positioning, installation, commissioning and site acceptance testing unless clearly stated otherwise.

	Tenderer to confirm included items.
	

	Training
	Tender price must include operator and basic maintenance training for relevant staff, delivered on site at commissioning.

	Tenderer to confirm training scope.
	

	Warranty
	Minimum 12-month warranty from successful installation/commissioning, covering defects in materials and workmanship, excluding misuse or consumables.

	Tenderer to state warranty.
	

	Service and spares
	Tenderer must describe service response, remote/phone support, spare-parts availability, routine maintenance requirements and annual service options.

	Tenderer to describe support.
	

	Other 

	




	
	




FORM OF TENDER
This form of Tender must be completed with the total cost to match the detailed quotation you will provide, and returned by all. Failure to complete fully & sign this Form of Tender may invalidate the offer.

	To:
	Garden of Eden Fresh Herbs Ltd


	From: 
	


	Re: 
	Supply, Delivery, Installation and Commissioning of an Automated Packing Machine for Fresh Herb and Salad Products




I/We have examined the quotation documentation and thereby offer to provide the goods and service in accordance with the details and specification contained within this document. 
I/We undertake to supply all items in accordance with the terms and conditions of the quotation specification. 
I/We confirm this quote will remain valid for up to 6 months from date of submission and for the duration of the contract.


	Item(s)

	€

	Supply, Delivery, Installation and Commissioning of an Automated Packing Machine for Fresh Herb and Salad Products

	

	TOTAL COST EX VAT [FOR EVALUATION]

	

	VAT Rate % & Value €

	

	TOTAL COST INCL VAT

	

	

	Signed 

	

	Name (in Capital Letters):

	

	Address


	

	Email

	

	Telephone

	

	Date 

	


Please describe the product quoted for in order that the Contracting Authority can confirm it meets requirements. Any quotes not meeting the specification will not be considered.
