TRD - Tender Response Document Open Procedure – Supply and Delivery of Fire Service Vans and 4x4 Pick-up truck
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TENDER RESPONSE DOCUMENT

	Title of Procurement

	Supply and Delivery of 3no. Fire Service Vans and 1no. 4x4 Pick-up truck to Longford County Council

	Closing Date & Time for Receipt of Tenders
	12:00 on 28th August 2026

	Organisation Name
	Longford County Council – Longford Fire & Rescue Service

	Contact Name 
	

	Contact Email
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[bookmark: _Toc16597912][bookmark: _Toc61968791][bookmark: _Hlk535242154]Instructions for Completion
[bookmark: _Hlk13580347]This document MUST be used for the submission of tenders. Please read the following instructions carefully.
· Tenderers should ensure they have read the Request for Tender before they attempt to complete this Tender Response Document. 
 
· If you consider that the Tender Response Document is missing any sections which would prevent you from preparing a comprehensive response, please contact the Contracting Authority as soon as possible.   

· Where there is a discrepancy between the contents / instructions in this document and the Request for Tender, the Request for Tender will take precedence. 
  
· Tenderers must follow the instructions contained in this document in relation to attachments, format for submission, etc.  

· [bookmark: _Hlk495513867]Where tenderers are relying on other parties to meet the selection criteria, those parties must be available to deliver elements of the contract. 


[bookmark: _Toc16597913][bookmark: _Toc61968792][bookmark: _Hlk13580304]Response to the Selection Criteria
[bookmark: _Toc61968793]General Contact Information
	Organisation Name:
	

	Contact Person:
	

	Position: 
	

	Address: 
	

	Phone:
	

	Email: 
	

	Website: 
	

	Date of Establishment, if applicable:
	VAT Registration No:
	Legal Structure – partnership, limited company, etc.

	
	
	

	Details of any Sub-contractors or Consortium members:

	Name
	Proposed Role in Delivery of the Contract
	Confirmation relevant information is provided for each party (e.g. financial, experience, or other selection criterion where applicable)  

	
	
	

	
	
	

	
	
	



[bookmark: _Toc16597916][bookmark: _Toc61968794]SELECTION CRITERIA - Pass/Fail Criteria
Financial Information
	
Tax Clearance

	I confirm and declare being tax compliant.  The Contracting Authority can verify your tax clearance status through Revenue’s online facility at http://www.revenue.ie/en/online/tax-clearance.html To this end, please confirm:
	Yes
	

	(A) 
	No
	

	Tenderer Name:
	

	Tenderer PPSN/ Tax Reference Number:
	

	Access Number:
	

	OR, I confirm that I hold a current valid paper Tax Clearance Certificate (generally relates to Non-Residents)

	Registration Number:
	
	Certificate Number:
	

	OR, 
I confirm that I have applied for Tax Clearance status or a Tax Clearance Certificate which will be made available on request
	Yes
	

	
	No
	

	Turnover

	I confirm that we have the requisite qualification to be considered for the contract of a minimum annual financial turnover (ex VAT ) required of €540,000.


	Year
	2024
	2023
	2022

	Month End (e.g July)
	

	
	

	Turnover in €
	

	
	

	We Confirm that we have the financial capacity to pay our debts identified on the current statement of assets and liabilities as being the debts as they fall due. 
	Yes
	

	
	No
	

	I confirm that I will provide evidence of turnover and capacity to pay our debts promptly on request.
NOTE #1:  In the case of sole traders or partnerships this condition may be satisfied by a letter of confirmation from a senior partner.
	Yes
	

	
	No
	

	
Insurances 

	I confirm that we have the following insurances in place 

	Insurance Type
	Level required if successful
	Level in Place
	Details of Any Excess
	Renewal Date

	Employers Liability
	€13,000,000
	€
	
	

	Public Liability
	€6,500,000
	€
	
	

	Product Liability
	€6,500,000
	€
	
	

	Professional Indemnity
	€1,000,000
	€
	
	

	AND

	I confirm that if successful, where the levels required under the contract/framework are higher than those currently in our possession, I will be in a position to put the required forms and levels of insurances required in place. 
	

	AND

	I confirm that I will provide the following promptly on request:
· evidence of insurances in place
      or 
· letter from Insurance Broker confirming that the required levels can be put in place if successful 
	









[bookmark: _Toc16597917][bookmark: _Toc61968795]Declaration Re Personal Circumstances – Pass/Fail Criteria
	DECLARATION RE PERSONAL CIRCUMSTANCES AS PER ART. 57 OF DIRECTIVE 2014/24/EU
Economic Operators will be excluded from the procurement process if, within the past five (5) years, there is evidence of a conviction relating to a specific criminal offence listed below (see 1.1) or if they have been the subject of a binding legal decision which found a breach of legal obligations to pay tax or social security contributions (see 1.2) (except where this is disproportionate e.g. where only minor amounts are involved).

	1.1 	Has the Economic Operator or a member of their proposed 	consortium, (if applicable), Director, or Partner or any other 	person who has powers of representation, decision or 	control, been convicted of any of the following offences?
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box 

	1.1.a
	participation in a criminal organisation, as defined in Article 2 of Council Framework decision 2008/841/JHA;
	
	

	1.1.b
	corruption, as defined in Article 3 of the Convention on the fight against corruption involving officials of the European Communities or officials of Member States of the European Union and Article 2(1) of Council Framework Decision 2003/568/JHA as well as corruption as defined in Irish Law or the jurisdiction in which the Economic Operator is established;
	
	

	1.1.c
	fraud within the meaning of Article 1 of the Convention on the protection of the European Communities’ financial interests;
	
	

	1.1.d
	the subject of a conviction for terrorist offences or offences linked to terrorist activities or for inciting or aiding or abetting or attempting to commit an offence; 
	
	

	1.1.e
	the subject of a conviction for money laundering or terrorist financing; 
	
	

	1.1.f
	the subject of a conviction of child labour and other forms of trafficking in human beings;
	
	

	Non-payment of taxes or social security obligations
1.2 Has it been established by a judicial or administrative decision having final and binding effect in accordance with Irish law or the legal provisions of the country in which the Economic Operator is established (if outside Ireland), that the Economic Operator is in breach of obligations related to the payment of tax and social security contributions?
Note: If the response to 1.2 above is in the affirmative, please provide further information on the decision and the amounts involved
	
	



	2.1 	Please indicate if any of the following situations have applied, 	within the past three (3) years, or currently apply, to your 	organisation.
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box

	2.1.a
	has, in the performance of any public contract, failed to comply with applicable obligations in the field of environmental, social and labour law applying at the place where the works were carried out or the services provided, as established by EU law, national law, collective agreements or by international, environmental, social and labour law listed in Annex X of Directive 2014/24/EU;
	
	

	2.1.b
	is bankrupt or the subject of insolvency or winding-up proceedings, its assets are being administered by a liquidator or by the court, or has entered into an arrangement with creditors, suspended its business activities or is in any analogous situation arising from a similar procedure under national laws and regulations;  
	
	

	2.1.c
	is guilty of grave professional misconduct which renders its integrity questionable;
	
	

	2.1.d
	has entered into agreements with other economic operators aimed at distorting competition;
	
	

	2.1.e 
	has a conflict of interest within the meaning of Article 24 of 2014/24/EU that cannot be effectively remedied by other, less intrusive, measures; 
	
	

	2.1.f 
	confirms that it has had prior involvement in the preparation of the procurement procedure which has resulted in a distortion of competition, as referred to in Article 41 of 2014/24/EU, that cannot be remedied by other, less intrusive, measures;
	
	

	2.1.g
	has shown significant or persistent deficiencies in the performance of a substantive requirement under a prior public contract, a prior contract with a contracting entity, or a prior concession contract, which led to early termination of that prior contract, damages or other comparable sanctions. 
	
	

	2.1.h
	· is guilty of serious misrepresentation in supplying the information required for the verification of the absence of grounds for exclusion or the fulfilment of the selection criteria; or
	
	

	
	· has withheld such information or is not able to submit supporting documents required under Article 59 of Directive 2014/24/EU; or 
	
	

	2.1.i
	has undertaken to:
· unduly influence the decision-making process of the contracting entity, or
· obtain confidential information that may confer upon the Tenderer undue advantages in the procurement procedure; or
· negligently provide misleading information that may have a material influence on decisions concerning exclusion, selection or award.
	
	

	3.
	Comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same);
	
	

	4.
	The origin of goods connected to the Tender, if any, are subject to the prohibitions set out in Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same)
	
	

	5.
	Any subcontractor, supplier or other entity on whose capacity the organization relies as part of the Tender comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	


[bookmark: _Toc487559492]

[bookmark: _Toc16597918][bookmark: _Toc61968796]Declaration Re Statutory Obligations – Pass/Fail Criteria
	We confirm that we are fully compliant with the following legislation, or equivalent legislation in our country of establishment/operation:
	YES
	NO

	(a) 
	Safety, Health and Welfare at Work Act 2005 and Safety, Health and Welfare at Work (General Application) Regulations 2007
	
	

	(b) 
	Employment Equality Acts 1998-2011 
	
	

	(c) 
	Equal Status Acts 2000-2011
	
	

	(d) 
	National Minimum Wage Act 2000 as amended 
	
	

	(e) 
	Organisation of Working Time Act 1997 as amended
	
	

	(f) 
	Disability Act 2005
	
	

	(g) 
	Regulation (EU) 2016/679 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data, the Data Protection Act, 2018
	
	

	(h) 
	We further confirm that all Data Subjects whose Personal Data is provided in our Tender have consented to the processing of such Personal Data by us, the Contracting Authority, the Evaluation Team and the supplier of the etenders.gov.ie website, for the purposes of our participation in this Competition or that we otherwise have a legal basis for providing such Personal Data to the Contracting Authority for the purposes of our participation in this Competition and that we will provide evidence of such consent and / or legal basis to the Contracting Authority upon request.
	
	

	(i) 
	We have procedures in place to ensure that our subcontractors, if any are used for this contract, apply the same standards.
	
	

	This Declaration is made for the benefit of the Contracting Authority. 
I certify that the information provided in the Declaration re Personal Circumstances and the Declaration re Statutory Obligations is accurate and complete to the best of my knowledge and belief.  I understand that the provision of inaccurate or misleading information in these Declarations will lead to my organisation being excluded from participation in this and future tenders and I am signing on behalf of: 

	Name of Tenderer
	


	Name of Authorised Signatory
	


	Position
	


	Signature
	




Workshop Facility - Pass/Fail Criteria
Tenderers must operate, either directly or via an agent, at least one workshop facility with the capacity and capability to carry out repairs/servicing to the fire appliance and the ancillary equipment procured under this Contract. 
Please provide details of the workshop:
	







Call-out Service - Pass/Fail Criteria
Tenderers must have the capability to provide a call-out service within 24 hours on a nationwide basis in the Republic of Ireland. Any costs associated with collection and transport of fire appliances to the Tenderer’s workshop must be borne by the Tenderer.
Please provide details of your call-out service:
	






[bookmark: _Toc16597921][bookmark: _Toc61968797]Previous Contracts / Experience - Pass/Fail Criteria
	Reference Contract #1

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	







	Any other relevant information 

	

	Reference Contract #2

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	


	Reference Contract #3

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	



[bookmark: _Toc16597922][bookmark: _Toc61968798]Health & Safety - Pass/Fail Criteria
	Do you comply with the Safety Health & Welfare at Work Act 2005 
	Yes
	
	No
	

	Name of Manager responsible for Health and Safety 
	

	Is it 3rd party certified or managed in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	I confirm that evidence of compliance will be provided promptly on request.
	Yes
	

	
	No
	





[bookmark: _Toc16597923][bookmark: _Toc61968799]Quality Assurance – Pass/Fail Criteria 
	Do you operate a quality management system? 
	Yes
	
	No
	

	Name of Manager responsible for Quality 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	If in-house, please provide summary of system: 
	







[bookmark: _Toc16597924][bookmark: _Toc61968800]Environmental Management Systems – Pass/Fail Criteria 
[bookmark: _Toc488834423][bookmark: _Toc460518593][bookmark: _Toc474254483]
	Do you operate an Environmental Management System / Policy? 
	Yes
	
	No
	

	Name of Manager responsible for Environmental Management 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	  

	If in-house, please provide summary of system: 
	




















[bookmark: _Toc16597925][bookmark: _Toc61968802]Response to the Award Criteria
Award Criterion 1 – Compliance with Technical Specifications & Minimum Warranty Requirements 
	Criterion 1:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Compliance with Technical Specifications & Minimum Warranty Requirements 
	
	
	

	
	Pass/Fail
	N/A
	N/A

	Instructions
	The Tenderer must detail here the compliance of the tendered vehicle with the technical specifications and minimum warranty requirements set out in Appendix 1.
Longford County Council will review various proposed solutions along with variations and will determine if the solution proposed broadly meets their requirements as set out in the RFT.
Only Tenders that receive a “Pass” mark for this award criterion will proceed to be evaluated under the remaining award criteria.
As a minimum tenderers are requested to carry out the following;
· Complete requested technical detail in the areas provided below
· Ensure Comments/Variations are included in the column provided where applicable. Insert ‘N/A’ if not applicable
· Ensure boxes labelled ‘ Tenderers to fill in details Here ‘ are completed with the required information




1. [bookmark: _Toc61968804]General 

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	1.1
	The appliance must be constructed in accordance with all relevant parts of the Road Traffic (Construction, Equipment and Use of Vehicles) (Amendment) Regulations (http://www.irishstatutebook.ie) and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.2
	The appliance must be constructed in accordance with the most recent edition of the Council Directive 2003/20/EEC on the approximation of the laws of the Member States relating to safety belts and restraint systems of motor vehicles and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.3
	The design of an appliance and the stowage of equipment shall be in accordance with the Safety, Health and Welfare at Work Act 2005 and the Safety, Health and Welfare at Work General Application (Amendment) Regulations 2007 (and latest editions), with particular regard to Manual Handling of Loads, and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.4
	Man-made fibres used in the construction of the appliance shall have a fire-retardant additive so that, as a minimum, the material conforms to the latest relevant sections of standard EN 13501-1.
	
	

	1.5
	The appliance shall be delivered to the Brigade Headquarters (or alternate Fire Station nominated at the time of placing the official order).
	
	

	1.6
	1 No. set of Test Certificates shall be supplied in English with the appliance for the following:
a) Proof of pre-delivery inspection, including confirmation of appliance road worthiness, by the chassis manufacturer;
b) Test Certificates shall be provided as appropriate for any ancillary equipment supplied;

	
	

	1.7
	1 No. complete Operator Manual shall be supplied in English in both hard and soft copy 
1 No. Maintenance Manual shall be supplied in English in both hard and soft copy to include the following:
a) Finished vehicle including the chassis;
b) Detailed and complete Wiring Diagrams – all relays and fuses numbered and detailed on both the circuit diagram and on the appliance;
c) User and Installation Manual for each electrical component;
d) All ancillary systems and equipment supplied;
1 No. dossier must be supplied in English in both hard and soft copy containing all relevant certificates and documentation pertaining to the commissioning, inspection and customer acceptance and/or final sign-off of the vehicles.
The above may be provided in both hard and electronic format. A label showing the registration number of the vehicles shall be placed on the front of all manuals and soft data supplied.
	
	


[bookmark: _Toc471745508][bookmark: _Toc471814382][bookmark: _Toc471827365]


2. Vans

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	2.1 
	A panel van built around a chassis which is a model commonly sold in Ireland for which spare parts are readily available. The Tenderer must include any work needed to modify the chassis to suit the approved design. The chassis must have the following key characteristics:
· Right-hand drive,
· Twin Axle
· Minimum 180hp engine power,
· Euro 6 emission standards [or latest],
· Gearbox must be 6 speed manual,
· Power assisted steering must be provided,
· Air conditioning must be provided,
· Van must be diesel fuelled.
· Pay load capacity of greater than 2000kg
· Minimum Cubic capacity of 13.0m3 (Alternatives may be considered)
Make model & BHP of van proposed:,
Tenderers to fill in details Here:




	
	

	2.2 
	The overall dimensions of the van must be typically what is referred to as a “L3/H2” – overall length and overall height of the van to be confirmed in the tender submission.
	
	

	2.3 
	Reversing camera and RHINO Tow Step in Yellow to be fitted at the rear of the van.
	
	

	2.4 
	Tow bar to be fitted at the rear of the van which must include a socket for trailer lighting.
	
	

	2.5 
	Van must be Red in colour.
	
	

	2.6 
	Doors of the rear storage compartment must be “Barn Doors”.
	
	

	2.7 
	Door on the side of the rear compartment must be “Sliding Doors”.
	
	

	2.8 
	The bulkhead dividing the rear crew compartment from the rear storage compartment must be solid in nature and sealed all around. No viewing window is required.
	
	

	2.9 
	The van must be robust in nature and suitable for Fire Service Operations such as the transportation of up to three [3] persons and associated equipment.
	
	

	2.10 
	All materials used in the construction of the passenger compartment shall have such fire-retardant properties so that, as a minimum, they conform to standard ISO 3795 and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this document). The cab floor must be finished with a durable material that is easily washable and include a drain.
	
	

	2.11 
	The total weight of the vehicle with equipment, fittings and a crew of three must be within the permitted axle loading and permissible total laden mass – maximum weights to be provided by the Tenderer. The chassis must be strong enough to minimise any bending or torsional movement associated with rapid response vehicles.
	
	

	2.12 
	The factory fuel tank must have a minimum capacity of 50L. Adblue and Diesel Caps must be appropriately labelled and not protrude beyond the body line.
	
	

	2.13 
	A ceiling mounted LED Light must be provided within the cab compartment.
	
	

	2.14 
	Durable labelling must be provided in the cab and rear crew compartment in relation to the following:
· No smoking,
· Vehicle dimensions,
· Seatbelts must be worn,
· Parking brake application.
· Maximum towing capacity.
	
	

	2.15 
	An in-cab storage unit for documents and small items such as hand portable radios, torches, etc must be provided between the two front seats.
	
	

	2.16 
	Air conditioning and heating system shall be fitted within the cab.
	
	

	2.17 
	Heated wing mirrors to be narrow profile. These mirrors shall be electrically adjustable from the driver's position. The number of mirrors provided shall ensure that no blind spots exist.
	
	

	2.18 
	Each van will be provided with a nearside awning covering the length from the side door of van to the rear barn doors of the van. The awning should not affect the doors or the scene lights provided.
	
	

	2.19 
	The underside of the vehicle must be coated with a wax oil product to minimize corrosion.
	
	

	2.20 
	The rear axle shall have twin wheels. A label stating the appropriate Tyre pressure (in psi and in bar) shall be on each wheel arch. 
Inner Tyres shall be fitted with valve extenders to allow inflation / checking without removing the outer wheel. A Tyre pressure monitoring system shall be provided.
Wheel nut position indicators shall be fitted to all wheel nuts.
	
	

	2.21 
	Rear doors must be openable by 270° and lockable against the body. Internal surfaces of these doors to be fitted with a durable plastic liner.
Rear door windows not to be fitted. 
Dry wipe boards (x1) to be fitted to the top inside half of each rear door.
	
	

	2.22 
	A nominal role board holder shall be fitted.
	
	

	2.23 
	Textured yellow grab rails for mounting/dismounting at all doors
	
	

	2.24 
	2 rechargeable Streamlight Vulcan high quality LED hand torches (or approved other) and docking charger stations to be supplied and fitted.
	
	

	2.25 
	Walls and floors in the rear storage compartment shall be lined with marine plywood. Side walls will be finished a clean plastic lining sheeting. The floor will be coated with a robust sealant to make it completely waterproof. It shall be taken up the side walls by height of 250mm on all edges
	
	

	2.26 
	Two ceiling mounted LED Lights must be provided within the rear storage compartment.
	
	

	2.27 
	A high-level storage unit for beaters, brushes, shovels, etc must be provided in the rear storage compartment and must have a minimum depth of 400mm.
	
	

	2.28 
	Storage and Shelving must be provided to cater for the storage of Fire Service equipment including (but not limited to) Battery Operated Tools, Water Rescue Equipment, Traffic Cones, Hazmat Boxes etc
	
	

	2.29 
	A low external warning temperature device must be fitted with an audible alarm on the dash.
	
	

	2.30 
	The following applied reflective vinyl material must be Avery Dennison Visiflex V-8000 series or equivalent.
Yellow and red Battenburg pattern must be applied to both sides of the van from below the driver’s window to the very bottom. It must blend in with the vans contours whilst maintaining the overall profile of the Battenburg pattern along the full length of the vehicle. 
Pattern block dimensions shall be sized to fit with the dimensions and scale of the vehicle.
	
	

	2.31 
	The rear of the van must be striped in alternating yellow and red 150mm strips in the “A” Chevron style. The inside of the rear barn doors must match the striping profile of the rear of the van when they are opened.
	
	

	2.32 
	The front bumper and grill of the van must be striped in alternating yellow and red 150mm strips in the “A” Chevron style.
	
	

	2.33 
	Longford Fire & Rescue Service shall be applied in English and Irish on a side body panel nearside and offside, in white bold text writing (the wording in English and Irish shall be supplied at the time of placing the official order for the vehicle).

Longford Fire & Rescue Service crest transfers (x2) shall also be fitted.

FIRE signage shall be applied to the front and back of the vehicle.
	
	

	2.34 
	All high-visibility markings and letterings must be edge sealed where necessary to prevent the ingress of water. 
	
	

	2.35 
	A Variable Message Sign [VMS] must be provided on the roof and to the rear of each van. When activated via a handset, it should rise up proud of the van and display its message. At the end of the incident, the handset must be capable of shutting down the sign and returning it to the stowed position. The VMS must have or be capable of the following:
· The VMS face must measure a minimum of 900mm x 900mm,
· The VMS face must be capable of being raised vertically from the stowed position,
· The VMS must be capable of being operated by a handset utilising a bungee/wandering lead,
· The VMS handset must allow the operator to select pre-set text and image files to display on the VMS face in a simple and straight forward manner,
· The VMS handset must come pre-programmed with approved traffic sign graphics,
· The text and images on the VMS face must be visible at angles from -700 to +700,
· The VMS face must be a full matrix unit capable of displaying amber, red and white text & images,
· The VMS unit must be robust in nature and capable of withstanding inclement weather and the ingress of water, etc,
· The VMS unit must be powered by 1 12v DC power supply or other such means compatible with the van.
· IP65 rating as a minimum
	
	

	2.36 
	New heavy duty maintenance free batteries to be provided. They should be securely clamped to prevent them from coming loose in the event of an accident. The battery compartment must be ventilated.
A heavy-duty master switch shall be provided to isolate the battery supply when the vehicle is not in use. Accidental turning off, of the master switch when the vehicle is moving should not turn off the vehicle and should not affect the driving of the vehicle.
	
	

	2.37 
	All electrical wiring shall be of adequate gauge and insulation for the designed load, and where exposed shall be waterproof and corrosion free. 
All electrical wiring must be suitable protected from damage and from the elements. All electrical wires must run in conduits within the bodywork. The conduits must be fixed to the bodywork, easily accessible for maintenance and remain in place for the life span of the van.
	
	

	2.38 
	All electrical circuits must have separate circuit breakers, suitably indicated and grouped into a common box located in an accessible position within the van.
	
	

	2.39 
	All electrical components, where applicable must be CE marked and carry a minimum 5-year warranty.
	
	

	2.40 
	All LED’s, scene lights, strip lights, marker lights and cluster lights must be of the latest generation and be ECE R65 and ECE R10 approved.
	
	

	2.41 
	The alternator must be upgraded if considered necessary to cater for the electrical demands of the van.
	
	

	2.42 
	Light Bars, LED’s & Scene Lights must be provided for each van as follows:
· Two low profile blue light bars [roof mounted front & rear],
· Two blue LED’s alternate flashing lights on both sides of each van [high level],
· Two blue LED’s alternate flashing lights on the rear of each van [high level],
· Two blue LED’s alternate flashing lights on the front of each van [low level grill],
· Two blue LED’s alternate flashing intersector lights on the rear of each van [low level],
· Two blue LED’s alternate flashing intersector lights on the front corners of each van [low level],
· Two LED labcraft scene lights on both sides of each van [high level],
· Two LED labcraft scene lights on the rear of the h [high level],
· Two white LED’s alternate flashing lights on the front of each van [low level grill],
· LED lighting of the steps to aid access/egress and must illuminate automatically when the doors open.
· 3 yellow side marker lights either side.
· IP67 rated
	
	

	2.43 
	A remote electronic siren with wail, yelp and public address functions must be installed. 
The wail and yelp functions shall be turned on or off by a dash-mounted switch that is accessible to the Officer-in-Charge and the driver (this is to be agreed during fitout stage). Once armed it shall be possible to turn on/off and change sirens using the vehicle horn
	
	

	2.44 
	A TETRA vehicle kit and GPS antenna must be provided.
	
	

	2.45 
	An electric load management system shall be provided. It shall include an automatic shedding function to protect the road batteries from loss of voltage which would prevent the vehicle from starting.
	
	

	2.46 
	Switching controller shall be centrally located on the dash to perform pre-programmed audio / visual warning patterns such as 999 and In Attendance and to individually control all blue lights, scene lights, etc. The programming of various patterns shall be included.
A test walk facility will be included to allow the driver to walk the perimeter of the vehicle to inspect auxiliary lighting.
	
	

	2.47 
	LED labcraft scene lights shall be fitted as follows:
2 no. on either side of the vehicle;
1 no. on the rear of the vehicle (note, these rear scene lights should also automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected);
Scene lights shall be interlocked with the handbrake so that they automatically switch off when the handbrake is released. Manual operation of the scene light shall be possible from the control panel.
	
	

	2.48 
	An external audible warning alarm indicating that the vehicle is reversing shall be fitted.
	
	

	2.49 
	2 no. heavy duty twin 220V Sockets, switchable and fused fitted in the cab.
2 no. heavy duty twin 220V Sockets, switchable and fused fitted in the rear storage compartment.
The 220V sockets will be powered only through the shore cable. 4 no. USB charging points to be distributed around the crew cab.
	
	







3. 4x4 Pick-up truck

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	3.1 
	Double Crew Cab Auto  4x4 with a canopy for fire service use. The chassis must have the following key characteristics:
· Right-hand drive,
· All wheel drive function
· Minimum 230hp engine power,
· Euro 6 emission standards [or latest],
· Gearbox must be 6 speed automatic,
· Power assisted steering must be provided,
· Air conditioning must be provided,
· Pick-up truck must be diesel fuelled.
· Canopy for storage/cargo section
· Minimum ground clearance 230mm

	
	

	3.2 
	Double Crew Cab 4x4 pick-up truck
	
	

	3.3 
	Reversing camera and scene light to be fitted at the rear of the pick-up truck.
	
	

	3.4 
	Tow bar to be fitted at the rear of the pick-up truck which must include a socket for trailer lighting.
	
	

	3.5 
	Pick-up truck including canopy must be Red in colour.
	
	

	3.6 
	Doors of the rear storage compartment must be “Tailgate Doors”. An optional tailgate table should be proposed.
	
	

	3.7 
	Shall be capable of supporting the VMS sign on the canopy (if required)
	
	

	3.8 
	The bulkhead dividing the rear crew compartment from the rear storage compartment must be solid in nature and sealed all around. Viewing window is required.
	
	

	3.9 
	The pick-up truck must be robust in nature and suitable for Fire Service Operations such as the transportation of up to five [5] persons and associated equipment.
	
	

	3.10 
	All materials used in the construction of the passenger compartment shall have such fire-retardant properties so that, as a minimum, they conform to standard ISO 3795 and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this document). The cab floor must be finished with a durable material that is easily washable.
	
	

	3.11 
	The total weight of the vehicle with equipment, fittings and a crew of three must be within the permitted axle loading and permissible total laden mass – maximum weights to be provided by the Tenderer. The chassis must be strong enough to minimise any bending or torsional movement associated with rapid response vehicles.
	
	

	3.12 
	The rear storage floor must be finished with a durable material that is easily washable and will maintain its integrity throughout the lifetime of the vehicle (including if/when the canopy is removed)
	
	

	3.13 
	A ceiling mounted LED Light must be provided within the cab compartment. 2no. ceiling mounted LED lights must be provided within the storage compartment.
	
	

	3.14 
	Durable labelling must be provided in the cab and rear crew compartment in relation to the following:
· No smoking,
· Seatbelts must be worn,
· Parking brake application.
· Maximum towing capacity.
	
	

	3.15 
	An in-cab storage unit for documents and small items such as hand portable radios, torches, etc must be provided between the two front seats.  To be agreed at design stage.
	
	

	3.16 
	Air conditioning and heating system shall be fitted within the cab.
	
	

	3.17 
	Heated wing mirrors to be narrow profile. These mirrors shall be electrically adjustable from the driver's position. The number of mirrors provided shall ensure that no blind spots exist.	
	
	

	3.18 
	A Cradle to hold a Tetra handheld radio to be provided and a universal mobile phone cradle to be provided with universal charging capabilities.
	
	

	3.19 
	A Variable Message Sign [VMS] must be provided on the roof and to the rear of the pick-up truck. When activated via a handset, it should rise up proud of the Pick-up truck and display its message. At the end of the incident, the handset must be capable of shutting down the sign and returning it to the stowed position. The VMS must have or be capable of the following:
•	The VMS face must measure a minimum of 900mm x 900mm,
•	The VMS face must be capable of being raised vertically from the stowed position,
•	The VMS must be capable of being operated by a handset utilising a bungee/wandering lead,
•	The VMS handset must allow the operator to select pre-set text and image files to display on the VMS face in a simple and straight forward manner,
•	The VMS handset must come pre-programmed with approved traffic sign graphics,
•	The text and images on the VMS face must be visible at angles from -700 to +700,
•	The VMS face must be a full matrix unit capable of displaying amber, red and white text & images,
•	The VMS unit must be robust in nature and capable of withstanding inclement weather and the ingress of water, etc,
•	The VMS unit must be powered by 1 12v DC power supply or other such means compatible with the van.
•	IP65 rating as a minimum
	
	

	3.20 
	The underside of the vehicle must be coated with a wax oil product to minimize corrosion.
	
	

	3.21 
	Lightweight hardwearing and easily washable Storage box capable of accommodating 1no. Firefighter Kit, Helmet, Firefighter boots, Undergarments, Tabards etc to be provided, and capable of being stowed in a fixed position without the use of straps.
	
	

	3.22 
	Two ceiling mounted LED Lights must be provided within the rear storage compartment.
	
	

	3.23 
	The canopy shall be painted in the Colour Red identical to the colour of the pick-up truck.
	
	

	3.24 
	New heavy duty maintenance free batteries to be provided. They should be securely clamped to prevent them from coming loose in the event of an accident. The battery compartment must be ventilated. A heavy-duty master switch shall be provided to isolate the battery supply when the vehicle is not in use. Accidental turning off, of the master switch when the vehicle is moving should not turn off the vehicle and should not affect the driving of the vehicle.
	
	

	3.25 
	All electrical wiring shall be of adequate gauge and insulation for the designed load, and where exposed shall be waterproof and corrosion free. 
All electrical wiring must be suitable protected from damage and from the elements. 
	
	

	3.26 
	All electrical circuits must have separate circuit breakers, suitably indicated and grouped into a common box located in an accessible position within the pick-up truck.
	
	

	3.27 
	All electrical components, where applicable must be CE marked and carry a minimum 5-year warranty.
	
	

	3.28 
	All LED’s, scene lights, strip lights, marker lights and cluster lights must be of the latest generation and be ECE R65 and ECE R10 approved.
	
	

	3.29 
	The alternator must be upgraded if considered necessary to cater for the electrical demands of the pick-up truck.
	
	

	3.30 
	LED’s & Scene Lights must be provided for each van as follows:
· One (1no.) LED scene lights on both sides of each van [high level],
· One (1no.) LED scene lights on the rear of each van [high level],
· Four (4no.)  forward facing, two blue and two white flashing LED lamps to be fitted into the front grill. White Led Flashing light to act similar to flashing headlights.  
· Two (2no.) rear facing, combined blue, red, alternating flashing LED lamps fitted in the rear pillars.  The 2 red alternate flashing lamps are to be wired through the handbrake;
· One (1no.) number small alternating blue light on rear corner bumper each side 
· Licence Plate Flashing LED lamps to be fitted, front & side facing fitted to front of vehicle. 
Two number scene lights; one fitted on each side of the vehicle on the canopy.
	
	

	3.31 
	A remote electronic siren with wail, yelp and public address functions must be installed. 
The wail and yelp functions shall be turned on or off by a dash-mounted switch that is accessible to the driver (this is to be agreed during fitout stage). Once armed it shall be possible to turn on/off and change sirens using the vehicle horn.
	
	

	3.32 
	A TETRA vehicle kit and GPS antenna must be provided.
	
	

	3.33 
	2 no. on either side of the vehicle;
1 no. on the rear of the vehicle (note, these rear scene lights should also automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected);
Scene lights shall be interlocked with the handbrake so that they automatically switch off when the handbrake is released. Manual operation of the scene light shall be possible from the control panel.
	
	

	3.34 
	An external audible warning alarm indicating that the vehicle is reversing shall be fitted.
	
	






8. [bookmark: _Toc471745514][bookmark: _Toc471814388][bookmark: _Toc471827371]Spare Parts, Warranties and Delivery

	Item

	Description
	Complies
(Y/N)
	Comments/
Variations

	8.1 
	It is a requirement that the bodywork must have a minimum of 15 Years Warranty. 
	
	

	8.2 
	It is a requirement that all other parts of the appliance (including ancillary equipment) other than the chassis must have a minimum of 2 years warranty.
	
	

	8.3 
	
	It is a requirement that the chassis vehicle systems and driveline must have a minimum of 2 years warranty (other than standard serviceable items). 
	
	

	8.4 
	Spare Parts and Technical Assistance shall be available for a minimum of 15 years for the appliance and all ancillary equipment. Suppliers should have a network of support throughout the Republic of Ireland for both chassis and fire engineering support including trained technical personnel based in the Republic of Ireland and appropriate transport for these personnel and spare parts. A stock of all commonly used spare parts should be available at a store in the Republic of Ireland. Suppliers should have the ability to have a trained technical person present at any Fire Station throughout the Republic of Ireland within 12 hours from receipt of call-out.

	
	

	8.5 
	Tenderers must state their delivery lead time (in weeks) for a complete solution for each chassis option. 
The lead time shall be taken as the period from the date of the official order placement to the delivery on station of a fully approved appliance.
Delivery will be to Longford Fire Station, Templemichael, Longford Town, Co. Longford.
	
	


[bookmark: _Toc471827372]


Award Criteria 2 – Experience & Qualifications of Staff
	Criterion 2:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Experience & Qualifications of Staff
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must provide details and examples of the relevant qualifications and experience of its employees engaged in the fit out of Emergency Tender vehicles, Fire Service Utility vehicles and other Fire Service vehicles, and also of any subcontractors engaged in the process.
Include details of the number of
i. technicians/mechanics employed and their qualifications;
ii. their experience building fire appliances;
iii. ongoing training/upskilling; and any other information which demonstrates that its staff have the requisite skills and experience.

	Tenderers’ Response

















[bookmark: _Hlk217996479]Award Criterion 3 – Aftersales Support & Technical Assistance 
	Criterion 3:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Aftersales & Technical Assistance 
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must set out the quality of its proposal in relation to its capacity and capability for the provision of maintenance, repair and technical assistance from its workshop facilities, and its capacity and capability for repair/maintenance services on-site at Longford County Council. Tenderers must provide details of workshops, if any, they have in the Republic of Ireland to carry out both chassis and Fire Engineering repairs. The Tenderer should also provide details of the process by which clients’ repair issues are managed from the time a fault is reported through to   successful conclusion. If sub-contracting after sales support to another supplier, full details must be provided of that sub-contractor, including their workshop details (for both chassis and Fire Engineering repairs), network details, technical capabilities of their employees in relation to fire-engineering support and their qualifications for same, and details of stock they carry and where the stock is located.


	Tenderers’ Response











Award Criterion 4 – Availability of Spare Parts
	Criterion 4:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Availability of Spare Parts 
	
	
	

	
	10%
	100
	60

	Instructions
	
The Tenderer must set out the quality of its proposal for ensuring the availability of all spare parts for the appliance and ancillary equipment for the minimum expected lifespan of the vehicles (15 years). 
The Tenderer should include details of its process and lead times for obtaining spare parts; how it manages this supply chain to ensure parts are delivered on time; and how it manages instances of order delays and parts being out-of-stock.


	Tenderers’ Response
















Award Criterion 5 – Ordering & Delivery
	Criterion 5:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Ordering & Delivery  
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative demonstrating its high-level process and timescales for the successful delivery of the Fire Service vehicles listed in this tender - from the time of the official order through to full commissioning and handover of the appliance.
The Tenderer should Include details of the tenderer’s methodology for ensuring that all appliances are supplied and delivered in accordance with the requirements specified by the client.


	Tenderers’ Response

















Award Criterion 6 – Environmental & Sustainability Efficiencies
	Criterion 6:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Environmental & Sustainability Efficiencies 
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative to demonstrate how it incorporates environmental and sustainability efficiencies/measures during the build   process. For example:
· Energy optimisation initiatives in the              warehouse/premises including rain harvesting, use of PV Panels, fabric of the building including insulation, efficiency of lighting and heating, EV charging capabilities etc.
· Use of recycled and/or recyclable material
· Waste management/disposal/recycling
· Minimisation of waste
· Transport and logistics measures
· Corporate Social Responsibility policies
· Proposed Targets for Environmental Sustainability
· Sustainable purchasing


	Tenderers’ Response













Award Criterion 7 – Cost
	Criterion 7:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Cost  
	
	
	

	
	60%
	600
	N/A

	Instructions
	
The Tenderer must give the total cost, in Euros , of the vehicle as specified in Appendix 1
· Including delivery to Longford
· Including all expenses/ tariffs/ custom charges
· Excluding VAT 



	Total Cost  ( ex. VAT )
	€



I/We confirm that I/we: 

1. Will keep this offer for the contract open for acceptance by you for a period of 12 months from the date of deadline for submission of Tenders,
2. Agree that you are not bound to accept the most economically advantageous or any Tender you may receive,
3. Have read and thoroughly examined the Tender Document,
4. Fully understand the Tender Document and the Client’s requirements,
5. Undertake to treat the details of this Invitation to Tender, its Tender and any subsequent agreements as private and confidential,
6. Acknowledge that acceptance by the Contracting Authority of this tender will not constitute a binding and enforceable agreement and that a legally enforceable agreement will not exist until and unless the contract is awarded between the Contracting Authority and the Tenderer,
7. Have availed of all offers for additional information or have otherwise satisfied myself/ourselves as to conditions that may in any manner affect the performance of the contract,
8. Have included all elements necessary for the performance of the specified requirements, which are either expressly stated in the Tender Document or contained in any supplementary information or which could reasonably be inferred therefrom,
9. Have found no errors, omissions, conflicts or ambiguities in the Tender Document except those which I/We have brought to the attention of the Contracting Authority before the latest date for submitting queries,
10. Have included for compliance with all statutory requirements applicable in Ireland and those applicable in any country where parts of the contract may be performed that are in force 7 days prior to the deadline for receipt of Tenders, 
11. Will not, if awarded a contract employ labour in a manner that is discriminatory in relation to gender, civil/family status, sexual orientation, religion, age, disability, race, or membership of the traveller community.
12. [bookmark: _Hlk491592638]Agree that as a condition of award, it shall be our sole responsibility to fulfil the obligations under the Contract, notwithstanding any changes in circulars, laws, regulations, taxation, duties or other factors which might arise following the withdrawal of the United Kingdom from membership of the EU.
	Signed:
	

	Name (in Capital Letters):
	

	On behalf of:	
	

	Address:
	

	Telephone:
	
	Mobile:
	

	Email:
	
	Date:
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