SITE WORKS SPECIFICATION
Project: Greyhound Track Infrastructure Works Youghal
Date: 14/07/2026
1.0 Site Preparation & Groundworks
1.1 Site survey to be carried out prior to works commencing.
1.2 All services crossing or inside the excavation areas to be identified and marked clearly.
1.3 Hare rail to be adequately protected at plant crossings.
1.4 Removal of track layers.
1.5 Remove track layers 300 mm inside the inner running rail to 300 mm inside the grass verge at the hare rail.
1.6 On-site silica sand storage area to be agreed by GRI & Contractor.
1.7 Silica sand must not be contaminated.
1.8 Excavate silica sand above the fine pink silt onto the existing geotextile membrane.
1.9 Excavate 80 mm of pink silt and relocate to low-lying infield areas.
1.10 Remove and dispose of geotextile by Contractor.
2.0 Track Layer Process
2.1 The existing stone layer under the geotextile to be loosened.
2.2 Loosen the compacted stone.
2.3 Place 100 mm continuous depth of 50 mm clean stone.
2.4 Cover stone with woven geotextile membrane.
2.5 Place 100 mm coarse sand (type to be agreed by Contractor and GRI specialist).
2.6 Install silica sand to required depths, cambers and levels.
GRI Track Specialists to monitor construction throughout the works.
3.0 Commissioning & Handover
3.1 Site handed over to Contractor on agreed date.
3.2 Only Contractor-approved visitors permitted during works.
3.3 Handover back to GRI after full site testing and commissioning is complete.
4.0 Drainage Works
4.1 Clear infield drainage areas of vegetation and blockages.
4.2 Add additional drainage if required.
5.0 Additional Works
5.1 Retention board 225 × 22 treated timber fixed to inner running rail posts. 3 fixings per post.
5.2 Heights and levels of treated timber to be provided by GRI specialists.
