The table below refers to the second table in the Pricing Schedule (Appendix 2 of the RFT and the Cost section of the Tender Response Document) entitled Pricing Schedule – Costs per Signage Unit. 
Tenderers are asked to quote for each of the signage types as laid out in the specification documents and in the table below. 
Please note that all signs and graphic panels must have a corner radius of 10mm. However, this requirement does not apply to the lift up flaps and the floor plaques. 
[bookmark: _GoBack]Costs are to include installation.

COSTS PER SIGNAGE UNIT 

	Sign Type
	Sign Dimensions
	Cost including installation

	Sign Type A1 Welcome Sign
	Please see ‘General Signage Specification’, file 24033_G - Welcome Totem Type A1 
	

	Sign Type A2 
Entrance Information Sign
	Please see ‘General Signage Specification’, file 24075_C - Entrance Info - Type A2
	

	Sign Type B1 
Car Park Directional & Information Sign
	Please see ‘General Signage Specification’, file 24037_E - Carpark & Directional - Type B1
	

	Sign Type B2 
Car Park Directional & Information Sign
	Please see ‘General Signage Specification’, file 24440_B - CP Direction & Info Signs - Type B2
	

	Sign Type C 
Car Park Directional & Information Sign
	Please see ‘General Signage Specification’, file 24074_C - Carpark Info Totem - Type C
	

	Sign Type D Information and Direction Totem
	Please see ‘General Signage Specification’, file 24056_D - Info & Direction Totem - Type D
	

	Sign Type E Accessible Lectern
	Please see ‘General Signage Specification’, file 24221_C - Accessible Lecturn Type E
	

	Sign Type F 
Small Directional Totem
	Please see ‘General Signage Specification’, file 24029_D - Small Direction Totem - Type F
	

	Sign Type G2 Reduced Height (Medium) Directional Totem
	Please see ‘General Signage Specification’, file 24073_C - Reduced Height Large Totem - Type G2
	

	Sign Type G1 Large Directional Totem
	Please see ‘General Signage Specification’, file 24039_F - Large Direction Totem - Type G1
	

	Sign Type H1 
Large Sign Plate
	Please see p.6 of the Sign Artwork Layout V12
	

	Sign Type H2 Small Sign Plate
	Please see p.6 of the Sign Artwork Layout V12
	

	Metal road signage with rails and post collars
	Please see p.66 of the Sign Artwork Layout V12
	

	Metal road signage mounted directly to wall
	Please see p.69 of the Sign Artwork Layout V12
	

	Waterproof Outdoor Panoramic Binoculars. With step.
	Please see ‘Sensory Sign Specification’, file 1-N60-007 Binoculars with step specification
	

	Rotating Totem
	Please see ‘Sensory Sign Specification’, file 1-N60-010 Rotating Totem specification
	

	Flower talking tubes
	Please see ‘Sensory Sign Specification’, files 2-N60-002 Flower Talking Tubes Specifications and 3-N60-004 Flower Talking Tubes Specifications
	

	Upright sign with rotating discovery disc
	Please see ‘Sensory Sign Specification’, files 3-N60-003 Upright sign with rotating discovery disc Specifications and 5-N60-006 Upright sign with rotating discovery disc Specifications
	

	Guess the texture 
	Please see ‘Sensory Sign Specification’ file, 3-N60-005 Guess the texture Specifications
	

	Painted dotted lines 
	Please see ‘Sensory Sign Specification’, file 3-N60-008 Painted dotted lines Specifications
	

	Upright sign with tactile moving glacier
	Please see ‘Sensory Sign Specification’, file 4-N60-005 Upright sign with tactile moving glacier Specifications
	

	Upright freechimes
	Please see ‘Sensory Sign Specification’, file 4-N60-011 Upright freechimes Specifications
	

	Solar audio bench
	Please see ‘Sensory Sign Specification’, file 5-N60-005 Solar Audio bench Specifications
	

	Upright olfactory display
	Please see ‘Sensory Sign Specification’, file 6-N60-001 Upright olfactory display Specifications
	

	Upright frame inc 4x rotating tree sections
	Please see ‘Sensory Sign Specification’, file 6-N60-003 Upright frame inc 4x rotating tree sections Specifications
	




	Panel Type
	Panel Dimensions
	Cost including installation

	Small Square Panel 
	133mm x 133mm, 10mm corner radius
	

	Large Square Panel
	280mm x 280mm, 10mm corner radius
	

	Protect Nature Panel
	280mm x 574mm, 10mm corner radius
	

	Accessible Lectern Map Panel
	868mm x 574mm, 10mm corner radius
	

	
Accessible Lectern Map Panel
	
868mm x 427mm, 10mm corner radius

	

	Welcome Sign panel
	1190mm x 1350mm, 10mm corner radius
	

	Carpark Directional and Information Sign panel
	574mm x 574mm, 10mm corner radius
	

	Information and Direction totem panel
	1162mm x 574mm, 10mm corner radius
	

	Metal Road signage panel (Artwork, p.66)
	1250mm x 500mm, 10mm corner radius
	

	Metal road signage panel mounted directly to wall (Artwork, p.69)
	1000mm x 350mm, 10mm corner radius
	

	Panels for Upright sign with rotating discovery disc (Artwork, p.35)
	1040mm x 163mm, 800 diam, 600 diam, 10mm corner radius
	

	Panel for Guess the Texture sign (Artwork, p.37)
	830mm x 530mm, 10mm corner radius (corner radius not required for lift-up flaps)
	

	Panel for Guess the Texture sign (Artwork, p.37)
	130mm x 154mm, 10mm corner radius (corner radius not required for lift-up flaps)
	

	Floor plaques (Artwork, p.41)
	300mm x 200mm
	

	Panel for Upright sign with tactile moving glacier (Artwork, p.46)
	1050mm x 904mm, 10mm corner radius
	

	Panel for Upright sign with tactile moving glacier (Artwork, p.46)
	424mm x 215mm, 10mm corner radius
	

	Panel for Upright freechimes (Artwork, p.52)
	1050mm x 270mm, 10mm corner radius
	

	Panels for Upright sign with rotating discovery disc (Artwork, p.56)
	1050mm x 163mm, 800 diam, 600 diam, 10mm corner radius
	

	Panels for upright olfactory display (Artwork, p.59)
	1050mm x 747mm, 10mm corner radius (corner radius not required for lift-up flaps)
	

	Panels for upright olfactory display (Artwork, p.59)
	92mm x 142mm, 10mm corner radius (corner radius not required for lift-up flaps)
	

	Panel for Upright frame inc 4x rotating tree sections (Artwork, p.61)
	1050mm x 286mm, 10mm corner radius (corner radius not required for lift-up flaps)
	

	Panel for Upright frame inc 4x rotating tree sections (Artwork, p.61)
	92mm x 142mm, 10mm corner radius (corner radius not required for lift-up flaps)
	



