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[bookmark: _Toc16597912][bookmark: _Toc61968791][bookmark: _Hlk535242154]Instructions for Completion
[bookmark: _Hlk13580347]This document MUST be used for the submission of tenders. Please read the following instructions carefully.
· Tenderers should ensure they have read the Request for Tender before they attempt to complete this Tender Response Document. 
 
· If you consider that the Tender Response Document is missing any sections which would prevent you from preparing a comprehensive response, please contact the Contracting Authority as soon as possible.   

· Where there is a discrepancy between the contents / instructions in this document and the Request for Tender, the Request for Tender will take precedence. 
  
· Tenderers must follow the instructions contained in this document in relation to attachments, format for submission, etc.  

· [bookmark: _Hlk495513867]Where tenderers are relying on other parties to meet the selection criteria, those parties must be available to deliver elements of the contract. 


[bookmark: _Toc16597913][bookmark: _Toc61968792][bookmark: _Hlk13580304]Response to the Selection Criteria
[bookmark: _Toc61968793]General Contact Information
	Organisation Name:
	

	Contact Person:
	

	Position: 
	

	Address: 
	

	Phone:
	

	Email: 
	

	Website: 
	

	Date of Establishment, if applicable:
	VAT Registration No:
	Legal Structure – partnership, limited company, etc.

	
	
	

	Details of any Sub-contractors or Consortium members:

	Name
	Proposed Role in Delivery of the Contract
	Confirmation relevant information is provided for each party (e.g. financial, experience, or other selection criterion where applicable)  

	
	
	

	
	
	

	
	
	



[bookmark: _Toc16597916][bookmark: _Toc61968794]SELECTION CRITERIA - Pass/Fail Criteria
Financial Information
	
Tax Clearance

	I confirm and declare being tax compliant.  The Contracting Authority can verify your tax clearance status through Revenue’s online facility at http://www.revenue.ie/en/online/tax-clearance.html To this end, please confirm:
	Yes
	

	(A) 
	No
	

	Tenderer Name:
	

	Tenderer PPSN/ Tax Reference Number:
	

	Access Number:
	

	OR, I confirm that I hold a current valid paper Tax Clearance Certificate (generally relates to Non-Residents)

	Registration Number:
	
	Certificate Number:
	

	OR, 
I confirm that I have applied for Tax Clearance status or a Tax Clearance Certificate which will be made available on request
	Yes
	

	
	No
	

	Turnover

	I confirm that we have the requisite qualification to be considered for the contract of a minimum annual financial turnover (ex VAT ) required of €2,000,000.


	Year
	2025
	2024
	2023

	Month End (e.g July)
	

	
	

	Turnover in €
	

	
	

	We Confirm that we have the financial capacity to pay our debts identified on the current statement of assets and liabilities as being the debts as they fall due. 
	Yes
	

	
	No
	

	I confirm that I will provide evidence of turnover and capacity to pay our debts promptly on request.
NOTE #1:  In the case of sole traders or partnerships this condition may be satisfied by a letter of confirmation from a senior partner.
	Yes
	

	
	No
	

	
Insurances 

	I confirm that we have the following insurances in place 

	Insurance Type
	Level required if successful
	Level in Place
	Details of Any Excess
	Renewal Date

	Employers Liability
	€13,000,000
	€
	
	

	Public Liability
	€6,500,000
	€
	
	

	Product Liability
	€6,500,000
	€
	
	

	Professional Indemnity
	€1,000,000
	€
	
	

	AND

	I confirm that if successful, where the levels required under the contract/framework are higher than those currently in our possession, I will be in a position to put the required forms and levels of insurances required in place. 
	

	AND

	I confirm that I will provide the following promptly on request:
· evidence of insurances in place
      or 
· letter from Insurance Broker confirming that the required levels can be put in place if successful 
	









[bookmark: _Toc16597917][bookmark: _Toc61968795]Declaration Re Personal Circumstances – Pass/Fail Criteria
	DECLARATION RE PERSONAL CIRCUMSTANCES AS PER ART. 57 OF DIRECTIVE 2014/24/EU
Economic Operators will be excluded from the procurement process if, within the past five (5) years, there is evidence of a conviction relating to a specific criminal offence listed below (see 1.1) or if they have been the subject of a binding legal decision which found a breach of legal obligations to pay tax or social security contributions (see 1.2) (except where this is disproportionate e.g. where only minor amounts are involved).

	1.1 	Has the Economic Operator or a member of their proposed 	consortium, (if applicable), Director, or Partner or any other 	person who has powers of representation, decision or 	control, been convicted of any of the following offences?
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box 

	1.1.a
	participation in a criminal organisation, as defined in Article 2 of Council Framework decision 2008/841/JHA;
	
	

	1.1.b
	corruption, as defined in Article 3 of the Convention on the fight against corruption involving officials of the European Communities or officials of Member States of the European Union and Article 2(1) of Council Framework Decision 2003/568/JHA as well as corruption as defined in Irish Law or the jurisdiction in which the Economic Operator is established;
	
	

	1.1.c
	fraud within the meaning of Article 1 of the Convention on the protection of the European Communities’ financial interests;
	
	

	1.1.d
	the subject of a conviction for terrorist offences or offences linked to terrorist activities or for inciting or aiding or abetting or attempting to commit an offence; 
	
	

	1.1.e
	the subject of a conviction for money laundering or terrorist financing; 
	
	

	1.1.f
	the subject of a conviction of child labour and other forms of trafficking in human beings;
	
	

	Non-payment of taxes or social security obligations
1.2 Has it been established by a judicial or administrative decision having final and binding effect in accordance with Irish law or the legal provisions of the country in which the Economic Operator is established (if outside Ireland), that the Economic Operator is in breach of obligations related to the payment of tax and social security contributions?
Note: If the response to 1.2 above is in the affirmative, please provide further information on the decision and the amounts involved
	
	



	2.1 	Please indicate if any of the following situations have applied, 	within the past three (3) years, or currently apply, to your 	organisation.
	YES
	NO

	
	Please indicate your answer by marking ‘X’ in the relevant box

	2.1.a
	has, in the performance of any public contract, failed to comply with applicable obligations in the field of environmental, social and labour law applying at the place where the works were carried out or the services provided, as established by EU law, national law, collective agreements or by international, environmental, social and labour law listed in Annex X of Directive 2014/24/EU;
	
	

	2.1.b
	is bankrupt or the subject of insolvency or winding-up proceedings, its assets are being administered by a liquidator or by the court, or has entered into an arrangement with creditors, suspended its business activities or is in any analogous situation arising from a similar procedure under national laws and regulations;  
	
	

	2.1.c
	is guilty of grave professional misconduct which renders its integrity questionable;
	
	

	2.1.d
	has entered into agreements with other economic operators aimed at distorting competition;
	
	

	2.1.e 
	has a conflict of interest within the meaning of Article 24 of 2014/24/EU that cannot be effectively remedied by other, less intrusive, measures; 
	
	

	2.1.f 
	confirms that it has had prior involvement in the preparation of the procurement procedure which has resulted in a distortion of competition, as referred to in Article 41 of 2014/24/EU, that cannot be remedied by other, less intrusive, measures;
	
	

	2.1.g
	has shown significant or persistent deficiencies in the performance of a substantive requirement under a prior public contract, a prior contract with a contracting entity, or a prior concession contract, which led to early termination of that prior contract, damages or other comparable sanctions. 
	
	

	2.1.h
	· is guilty of serious misrepresentation in supplying the information required for the verification of the absence of grounds for exclusion or the fulfilment of the selection criteria; or
	
	

	
	· has withheld such information or is not able to submit supporting documents required under Article 59 of Directive 2014/24/EU; or 
	
	

	2.1.i
	has undertaken to:
· unduly influence the decision-making process of the contracting entity, or
· obtain confidential information that may confer upon the Tenderer undue advantages in the procurement procedure; or
· negligently provide misleading information that may have a material influence on decisions concerning exclusion, selection or award.
	
	

	3.
	Comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same);
	
	

	4.
	The origin of goods connected to the Tender, if any, are subject to the prohibitions set out in Regulation (EU) No 833/2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same)
	
	

	5.
	Any subcontractor, supplier or other entity on whose capacity the organization relies as part of the Tender comes within the category of prohibited economic operators identified in Regulation (EU) No 833/2014 of 31 July 2014 (as amended by EU Regulation 2022/576 or any subsequent amendments to same).
	
	


[bookmark: _Toc487559492]

[bookmark: _Toc16597918][bookmark: _Toc61968796]Declaration Re Statutory Obligations – Pass/Fail Criteria
	We confirm that we are fully compliant with the following legislation, or equivalent legislation in our country of establishment/operation:
	YES
	NO

	(a) 
	Safety, Health and Welfare at Work Act 2005 and Safety, Health and Welfare at Work (General Application) Regulations 2007
	
	

	(b) 
	Employment Equality Acts 1998-2011 
	
	

	(c) 
	Equal Status Acts 2000-2011
	
	

	(d) 
	National Minimum Wage Act 2000 as amended 
	
	

	(e) 
	Organisation of Working Time Act 1997 as amended
	
	

	(f) 
	Disability Act 2005
	
	

	(g) 
	Regulation (EU) 2016/679 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data, the Data Protection Act, 2018
	
	

	(h) 
	We further confirm that all Data Subjects whose Personal Data is provided in our Tender have consented to the processing of such Personal Data by us, the Contracting Authority, the Evaluation Team and the supplier of the etenders.gov.ie website, for the purposes of our participation in this Competition or that we otherwise have a legal basis for providing such Personal Data to the Contracting Authority for the purposes of our participation in this Competition and that we will provide evidence of such consent and / or legal basis to the Contracting Authority upon request.
	
	

	(i) 
	We have procedures in place to ensure that our subcontractors, if any are used for this contract, apply the same standards.
	
	

	This Declaration is made for the benefit of the Contracting Authority. 
I certify that the information provided in the Declaration re Personal Circumstances and the Declaration re Statutory Obligations is accurate and complete to the best of my knowledge and belief.  I understand that the provision of inaccurate or misleading information in these Declarations will lead to my organisation being excluded from participation in this and future tenders and I am signing on behalf of: 

	Name of Tenderer
	


	Name of Authorised Signatory
	


	Position
	


	Signature
	





Workshop Facility - Pass/Fail Criteria
Tenderers must operate, either directly or via an agent, at least one workshop facility with the capacity and capability to carry out repairs/servicing to the fire appliance and the ancillary equipment procured under this Contract. 
	Do you operate Workshop facility with the capacity and capability to carry out repairs/servicing to the fire appliance and the ancillary equipment procured under this Contract 
	Yes
	
	No
	

	Location of Workshop 
	

	Please provide details of the workshop
	












Call-out Service - Pass/Fail Criteria
Tenderers must have the capability to provide a call-out service within 24 hours on a nationwide basis in the Republic of Ireland. Any costs associated with collection and transport of the water tender fire appliances to the Tenderer’s workshop must be borne by the Tenderer.
	Do you have the capability to provide a call-out service within 24 hours on a nationwide basis in the Republic of Ireland
	Yes
	
	No
	

	Location of Call-out facility 
	

	Please provide details of the call-out service 
	












[bookmark: _Toc16597921][bookmark: _Toc61968797]Previous Contracts / Experience - Pass/Fail Criteria
Tenderers must have successfully supplied and delivered, or be in the process of supplying and delivering, a minimum of 2 No. fire appliances of a similar type to the Water Tanker appliance specified in this RFT, in the past seven years (similar appliance means: Class B Water Tender, Water Tanker, Emergency Tender or Aerial Appliance). It is at the Contracting Authority’s sole discretion to decide on whether these examples are deemed of a similar type to those sought in this RFT.
	Reference Contract #1

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	







	Any other relevant information 

	


	Reference Contract #2

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	

	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	


	Reference Contract #3

	Customer Name
	

	Contact Name
	

	Contact Number
	

	Delivery Date(s)
	From
	
	To 
	

	Contract Value
	
	Period value refers to
	

	Detailed description
	



	Taking account of the features of the contract please provide information in relation to the following, demonstrating comparability with the contract / framework being awarded under this procurement:  

	

	Any other relevant information 

	



[bookmark: _Toc16597922][bookmark: _Toc61968798]Health & Safety - Pass/Fail Criteria
	Do you comply with the Safety Health & Welfare at Work Act 2005 
	Yes
	
	No
	

	Name of Manager responsible for Health and Safety 
	

	Is it 3rd party certified or managed in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	I confirm that evidence of compliance will be provided promptly on request.
	Yes
	

	
	No
	





[bookmark: _Toc16597923][bookmark: _Toc61968799]Quality Assurance – Pass/Fail Criteria 
	Do you operate a quality management system? 
	Yes
	
	No
	

	Name of Manager responsible for Quality 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	

	
	Evidence will be provided on request
	Yes
	

	
	
	No
	

	If in-house, please provide summary of system: 
	







[bookmark: _Toc16597924][bookmark: _Toc61968800]Environmental Management Systems – Pass/Fail Criteria 
[bookmark: _Toc488834423][bookmark: _Toc460518593][bookmark: _Toc474254483]
	Do you operate an Environmental Management System / Policy? 
	Yes
	
	No
	

	Name of Manager responsible for Environmental Management 
	

	Is it 3rd party certified or in-house? 
	3rd Party Certified
	

	
	In-House
	

	If 3rd party certified, please provide the following information: 
	Date of most recent certification 
	

	
	Scope of Certification
	

	
	Name of Certification Body
	  

	If in-house, please provide summary of system: 
	




















[bookmark: _Toc16597925][bookmark: _Toc61968802]Response to the Award Criteria
Award Criterion 1 – Compliance with Technical Specifications & Minimum Warranty Requirements 
	Criterion 1:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Compliance with Technical Specifications & Minimum Warranty Requirements 
	
	
	

	
	Pass/Fail
	N/A
	N/A

	Instructions
	The Tenderer must detail here the compliance of the tendered vehicle with the technical specifications and minimum warranty requirements set out in Appendix 1.
Waterford City & County Council will review various proposed solutions along with variations and will determine if the solution proposed broadly meets their requirements as set out in the RFT.
Only Tenders that receive a “Pass” mark for this award criterion will proceed to be evaluated under the remaining award criteria.
As a minimum tenderers are requested to carry out the following;
· Complete requested technical detail in the areas provided below
· Ensure Comments/Variations are included in the column provided where applicable. Insert ‘N/A’ if not applicable
· Ensure boxes labelled ‘ Tenderers to fill in details Here ‘ are completed with the required information




1. [bookmark: _Toc61968804]General 

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	1.1
	The appliance must be constructed in accordance with the most recent edition of all parts of EN 1846, with a motor class of super (S), urban category (1), for water tanker appliance with a seating capacity of 2 persons, a tank capacity for firefighting water of minimum contents 8,000 litres, an installed pump performance of 10bar delivering 2,000 l/min and appropriate locker arrangement, and any subsequent amendments of same on the date this tender was advertised (unless specifically stated otherwise within this RFT).
	
	

	1.2
	The appliance must be constructed in accordance with all relevant parts of the Road Traffic (Construction, Equipment and Use of Vehicles) (Amendment) Regulations (http://www.irishstatutebook.ie) and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.3
	The appliance must be constructed in accordance with the most recent edition of the Council Directive 2003/20/EEC on the approximation of the laws of the Member States relating to safety belts and restraint systems of motor vehicles and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.4
	The design of an appliance and the stowage of equipment shall be in accordance with the Safety, Health and Welfare at Work Act 2005 and the Safety, Health and Welfare at Work General Application (Amendment) Regulations 2007 (and latest editions), with particular regard to Manual Handling of Loads, and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.5
	The cab construction must conform to ECE R29 (or equivalent) Standards and any subsequent amendments of same on the closing date of tender (unless specifically stated otherwise within this RFT).
	
	

	1.6
	Man-made fibres used in the construction of the appliance shall have a fire-retardant additive so that, as a minimum, the material conforms to the latest relevant sections of standard EN 13501-1.
	
	

	1.7
	The appliance shall be delivered to the Brigade Headquarters (or alternate Fire Station nominated at the time of placing the official order).
	
	

	1.8
	1 No. set of Test Certificates shall be supplied in English with the appliance for the following:
a) Proof of pre-delivery inspection, including confirmation of appliance road worthiness, by the chassis manufacturer;
b) Test Certificates shall be provided as appropriate for any ancillary equipment supplied;

	
	

	1.9
	1 No. complete Operator Manual shall be supplied in English in both hard and soft copy 
1 No. Maintenance Manual shall be supplied in English in both hard and soft copy to include the following:
a) Finished vehicle including the chassis;
b) Detailed and complete Wiring Diagrams – all relays and fuses numbered and detailed on both the circuit diagram and on the appliance;
c) Engineering Drawings of the appliance;
d) User and Installation Manual for each electrical component;
e) All ancillary systems and equipment supplied;
1 No. dossier must be supplied in English in both hard and soft copy containing all relevant certificates and documentation pertaining to the commissioning, inspection and customer acceptance and/or final sign-off of the vehicle.
The above may be provided in both hard and electronic format. A label showing the registration number of the appliance shall be placed on the front of all manuals and soft data supplied.
	
	


[bookmark: _Toc471745508][bookmark: _Toc471814382][bookmark: _Toc471827365]


2. Chassis

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	2.1 
	An 18 tonnes (18,000 Kg) Gross Vehicle Weight Rating chassis must be proposed such that will fully comply with all items contained in this Section 2.

Make model & BHP of truck chassis proposed:,
Tenderers to fill in details Here:




	
	

	2.2 
	The total weight of the appliance with equipment, water and crew must be within the permitted axle loading and permissible total laden mass. The front axle shall have minimum 9,000Kgs capacity. Details of typical equipment stowed are detailed in 4.7.2 below.
	
	

	2.3 
	Right Hand Drive 4 X 2 Rear Wheel Drive
	
	

	2.4 
	The appliance must be minimum Euro 6 compliant.
	
	

	2.5 
	The appliance shall have an engine power output of not less than 320 BHP.

	
	

	2.6 
	The appliance speed limiter shall be set at 90kph such that the appliance cannot exceed this speed. 

	
	

	2.7 
	The appliance must either:
Have no Tachograph installed, which results in no warning lights on the dash; or
The Appliance shall be fitted with a Tachograph simulator: A tachograph 1391 Siemens VDO interface (or equivalent).  Please note that the 1391 Siemens VDO tachograph is not a standard type tachograph and for example does not accept driver cards.

	
	

	2.8 
	The appliance shall be fitted with a clutch-less fully automatic Allison Automatic Transmission (or equivalent) with Fully Automatic Integral Retarder.
It shall only be possible to start the appliance in neutral with the handbrake on.

Make,model of transmission proposed:
Tenderers to fill in details Here:



	
	

	2.9 
	A visual and audible alarm shall activate on the dash if the driver’s door is opened and the handbrake is released.
	
	

	2.10 
	[bookmark: _Hlk203121959]The appliance shall be fitted with lightweight alloy wheels. The rear axle must have twin wheels. The appliance must be supplied with new Michelin XZE 2 (or equivalent) tyres that are approved by the chassis manufacturer. The tyres must be rated for the maximum speed of the appliance. 
Yellow Wheel Nut position indicators shall be fitted to all external wheels. A label stating the appropriate tyre pressure must be located on each wheel arch. It must be possible to easily check the tyre pressures of the inside tyres without removing the outside tyres. A new spare front wheel and tyre must be supplied with the appliance (Note: the spare wheel and tyre must not be carried on the appliance).
Make,model of tyres proposed:
Tenderers to fill in details Here:



	
	

	2.11 
	The appliance shall have a rear air suspension including a stabiliser (anti-roll) bar. It shall be possible to dump the air in the cab and pump bay – with a default to ride height on release of the handbrake. 
	
	

	2.12 
	Electronic ABS must be fitted to the appliance.
	
	

	2.13 
	ASR Traction control must be fitted to the appliance.
	
	

	2.14 
	Advanced Emergency Braking shall be fitted.
	
	

	2.15 
	Lane Departure Warning shall be fitted.
	
	

	2.16 
	An electronic stability control system / programme shall be fitted to the appliance.
	
	

	2.17 
	The fuel tank, and any alterations, must be manufactured from a corrosion resistant material and must not encroach into the locker areas. An anti-spill device is to be located between the filler cap and the fuel tank. The fuel tank must have a minimum capacity of 130 litres.
	
	

	2.18 
	The air intake must be located at least 1.3m above ground level. 
	
	

	2.19 
	The exhaust system must be manufactured from a corrosion resistant material. A low-level offside exhaust must be high enough to not get caught on traffic calming measures when fully laden. Details shall be provided of the required location of the end of the exhaust system at the time of placing the official order. 
	
	

	2.20 
	A transponder may be supplied by the Contracting Authority for fitting to the appliance to automatically activate the exhaust extraction system on return to station.
	
	

	2.21 
	Electric heated and electrically adjustable side mirrors must be provided on both sides of the vehicle.
A nearside Kerb Mirror and a Wide Angled Mirror located above the centre of the windscreen showing the ground area immediately in front of the full cab width must be fitted.
[bookmark: _Hlk203122461]Camera mirrors will be acceptable as an alternative to the above mirrors. 
	
	

	2.22 
	The chassis shall be fitted with LED chassis lights. The chassis shall also have front cornering lights. 
	
	

	2.23 
	A low external warning temperature device must be fitted with an audible alarm on the dash.
	
	

	2.24 
	The chassis cab shall be fitted with driver, passenger and side curtain airbags.
	
	

	2.25 
	Inspection checks shall be easily carried out by lifting the bonnet. The bonnet must be supported by two gas struts when it is open.
	
	

	2.26 
	Each door shall be fitted with a suitable strap to prevent the hinges being damaged in the event of wind or other suddenly forcing the door to a fully open position.
	
	

	2.27 
	The appliance must be equipped with two towing devices at both the front and rear, which will provide anchorage for winches and facilitate vehicle recovery. These devices shall be of sufficient strength to allow the vehicle to be towed on road at its permitted Total Laden Mass and no undue pressure shall be exerted on the chassis by these devices. A label shall be attached adjacent to each towing eye stating the capacity of each eye.
	
	

	2.28 
	Anti-Bandit windscreen glazing to be provided for both windscreen and side glazing.
The appliance shall be fitted with electric windows for the driver and passenger position.
	
	

	2.29 
	A full set of snow socks suitable for the appliance tyre size shall be supplied with the truck.
	
	

	2.30 
	The chassis shall be fitted with a tyre pressure monitoring system that will alert the driver in the event of the tyre pressure being low in any tyre.
	
	

	2.31 
	All chassis rails, crossmembers, air tanks, axles and suspension systems shall be protected by either painting it with Sigmashield 880 (or equivalent) or by waxing it with DINITROLL 4010 wax. All chassis preparation works (e.g. re-sighting air reservoirs etc.) shall be included. This coating shall provide corrosive protection from water contact and road salt. 
	
	

	2.32 
	The chassis manufacturer shall approve any modifications made to the chassis.
	
	

	2.33 
	A Breakdown Triangle, a Dry Powder Fire Extinguisher and a First-Aid Kit shall be fitted in the drivers’ cab. A Hydraulic Jack Kit and a complete chassis toolkit shall be supplied with the appliance.
	
	

	2.34 
	1 Day Driver Familiarisation Training shall be delivered by the chassis supplier (separate to pump operation training) for up to 40 personnel at the station that the appliance will be based.
1 Day Mechanical and Electrical Maintenance training (separate to pump and driver familiarisation training) for up to 3 maintenance personnel at each Brigade Headquarters or other nominated location.
1 Day Pump operator to be provided by a suitably qualified pump instructor nominated by the main agent for the pump provided. The cost of the provision of the above training shall be borne by the supplier.
	
	









3. Cab

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	3.1 
	The cab shall be a new single-construction cab. 
	
	

	3.2 
	An Electro/Hydraulic Cab Tilt mechanism must be fitted to the cab. Full access must be provided to the engine and gearbox for maintenance.
	
	

	3.3 
	The drivers and officer’s seat shall be fully adjustable both fore and aft, for height and rake. The seats shall have a leatherette finish.
	
	

	3.4 
	Grab Handles shall be provided in yellow to assist with access / egress from all cab doors.
	
	

	3.5 
	Seat positions shall be fitted with three point high-conspicuity seat belts. The seat belts shall be positioned such that a Firefighter wearing fire-kit can fasten the seat belt.
	
	

	3.6 
	A seat belt warning device shall indicate which personnel are not wearing seat belts.
	
	

	3.7 
	Height adjustable head restraints shall be provided where full length back seats are not provided. Care shall be taken concerning the position and suitability of head restraints considering helmets have to be worn.
	
	

	3.8 
	If a storage unit is not provided for documents and small equipment between the driver and the officer seat by the chassis supplier, a storage unit 400mm wide by 500mm deep by 250mm high with a lockable lid shall be provided. It shall be constructed of material and furnishings to blend in with the manufacturer’s cab.
In addition, suitable storage for 1 No. Fire-fighter helmet shall be provided in the front of the cab.
	
	

	3.9 
	A Flexi Map Reading Light shall be fitted in the offside front side of the cab.
	
	

	3.10 
	An hour meter for engine running time shall be installed in the cab.
	
	

	3.11 
	A 24 hour vehicle powered digital clock visible to the driver in daylight and darkness. It shall operate independently of the master switch.
	
	

	3.12 
	A notice shall be fixed in the cab visible to the driver giving details of the height (highest point of appliance), width, length and gross laden mass of the appliance.
	
	

	3.13 
	All internal finishings shall be to a factory finish and any amendments to the interior of the cab shall be made good.
	
	

	3.14 
	All Cab Stepwells shall be fitted with Tread Kicker Plats to prevent paint damage from kicking. All Cab steps shall be painted in yellow high conspicuity non-slip paint.
	
	

	3.15 
	The appliance shall be registered by the tenderer. 
1 No. reflective registration number plate shall be fixed to the front of each appliance and 1 No. reflective registration number plate shall be fixed to the rear of each appliance. A light shall be placed to illuminate each rear registration number plate.
	
	




[bookmark: _Toc471745510][bookmark: _Toc471814384][bookmark: _Toc471827367]

4. Body Construction and Design

	Item
	Description
	Complies
(Y/N)
	Comments/
Variations

	4.1 
	The body layout provided in this Section 4 is a suggested layout but variations may be accepted if deemed suitable. The exact layout will be agreed with the successful tenderer at pre-build meeting stage.
	
	

	4.2 
	The required body construction type, including the water storage tank is a composite material. 
	
	

	4.3 
	The body design shall be profiled to match the cab profile, including the provision of chassis side air deflectors to completely close the gap between the cab and the body.
	
	

	4.4 
	The body shall be mounted onto the chassis strictly in accordance with the chassis manufacturer’s guidelines.
	
	

	4.5 
	The main body of the appliance shall be designed to accommodate a minimum water capacity of 8,000 litres. The final volume will be confirmed during the build stage to ensure the maximum possible water stowage is achieved while remaining within legal weight limits for the fully equipped appliance, including crew and equipment. Lockers on the side of the appliance shall incorporate stowage for ancillary equipment including a dam and a portable pump. A locker at the rear of the appliance shall house the main fire-fighting pump. 
	
	

	4.6 
	The overall length of the body should not exceed 6,000mm. The overall height of the appliance shall not exceed 3,500mm when fully laden.
The minimum width of the pump bay shall be 1,000mm. 
	
	

	4.7 
	The following section outlines the dimensions and requirements for the lockers.
	
	

	4.7.1
	The lockers shall be enclosed by either weather proofed alloy shutters with a lift bar easy opening latch assembly or with hinged doors to match the bodywork with a minimum of 2 No. quick release locks on each door.  The shutters / doors shall be designed to prevent accidental opening. Shutters, once opened, shall remain in the open position and shall have a strap fitted to the bottom of them hanging down to assist closing of the shutters when fully opened. Shutter lift bars shall be recessed inside the body profile. Doors once opened shall remain in the open position. Central locking shall be provided to all lockers, including the pump bay, operated from a button on the dash.
Make,model of Locker Shutter proposed:
Tenderers to fill in details Here:


	
	

	4.7.2
	Locker(s) shall be provided on both sides of the rear of the appliance to allow for stowage of the following typical ancillary equipment. The equipment layout will be agreed between the successful tenderer at pre-build meeting stage:
a) 1 No. Water Dam contained in a durable storage bag. The dam stowage should take into consideration manual handling issues that may arise with stowing and removing the dam into and out the locker and should include appropriate mechanical aids to safely load and unload the dam from the locker, i.e. no manual handling issues should be encountered when stowing or removing the dam from a locker;
b) 1 No. lightweight portable pump stored on a Sliding Cradle on the nearside of the appliance with a facility to charge the LPP; 
c) 4 No. 100mm x 2440mm suction hoses ;
d) 1 No. Round Thread 100mm Combined Suction and Strainer Basket;
e) 1 No. Standpipe key and bar;
f) 2 No. 20 litre drums of road washing detergent – note these should be stored such that the detergent pick up tube for induction can be dropped into the drums where stored;
g) 2 No. 20 litre drums of fire-fighting foam – note these should be stored such that the detergent pick up tube for induction can be dropped into the drums where stored;
h) 8 No. 23m length of 70mm hoses;
i) 2 No. 5m length of 70mm hoses;
j) 6 No. 750mm traffic cones;
k) 1 No. Directional arrow that will mount on top of a 750mm cone
l) 1 No. Ground Monitor;
m) 1 No. Dividing Breach;
n) 1 No. Collecting Head;
o) 1 No. Low level strainer;
p) 1 No. Slurry Tanker Adaptor;
q) 1 No. Milk Tanker Adaptor; and
r) 1 No. Incident Warning Sign 
One full width locker at the rear of the appliance, accessible by a roller shutter door on either side of the appliance, complete with appropriate shelving, stowage tunnels, bollarding and strapping is a suggested way to store all equipment. Other alternatives may be considered and agreed at pre-build meeting stage.
Note: Only the Dam is required to be supplied with the appliance
	
	

	4.7.3
	Any sliding trays and cradles shall have automatic locking in the ‘IN’ and ‘OUT’ position.
	
	

	4.7.4
	All bottom shelves shall have a minimum capacity of 150Kgs. All shelves shall be of peg board construction. High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) yellow reflective tape shall be placed on the front of all shelves. High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) yellow reflective tape shall be placed on the front side of all cradles, sliding and tilt and slide shelves that protrude more than 25mm outside the vehicle bodyline. High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) red reflective tape shall be placed on the front side of all cradles, sliding and tilt and slide shelves that protrude more than 25mm outside the vehicle bodyline.
	
	

	4.7.5
	The Rear Pump Bay locker shall be provided with robust construction barn doors which can be secured in the open position. 
Stowage shall be provided in the pump bay for the following:
a) 2 No. Suction Keys (in suitable storage tubing); and
b) A Blank Cap;
Note, items a) and b) above must be supplied with the appliance.
	
	

	4.8 
	‘Cat’s Whiskers’ shall be fitted to the wheel arches for spray suppression. Mud Flaps shall be fitted behind the rear wheels for spray suppression. 
	
	

	4.9.1
	Roof access ladder support brackets to be fitted to the nearside of the appliance.
	
	

	4.9.2
	Anti-slip adhesive tape / paint shall be placed on the roof of the body of the appliance in any areas where an operator could potentially walk.

	
	

	4.9.3
	1 No. rated Safety Harness anchor point on the roof
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5 Paint & Conspicuity Markings

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	
	All conspicuity markings must conform to ECE 104 (or equivalent) Standard. 

	
	

	5.1
	The appliance, including the bodywork header panels, front grille closure, front bumper, the step well areas, all wheel arches, the Ad Blue tank (where visible) and the diesel tank (where visible) shall be painted in Red to BS 381C-538 (or equivalent) applied in a wet effect finish.

	
	

	5.2
	All locker roller shutters and exposed patterned aluminium shall be left unpainted.
Hinged locker doors where provided shall be so designed to prevent the ingress of water/ road spray.	
	
	

	5.3
	All metal fabrications must be thoroughly degreased.
	
	

	5.4
	The front bumper of the appliance shall be painted red and have High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) White (to be agreed at the pre-build meeting) 100mm Reflective Strips to match the bumper contours in inverted V style.
The area between the windscreen and the grill shall have a High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow Reflective Strip with the wording FIRE (forward and reverse) on top of the 150mm Reflective Yellow Strip in red Writing. The Chassis badge name shall be painted in red to match the appliance colour. 25mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow Reflective Strips shall be placed on the grill bars on the front of the appliance.
Note, variations may be required to the above markings depending on the chassis tendered.

	
	

	5.5
	High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Yellow and Red Day-Glo Reflective Battenburg Pattern shall be applied to both sides of the appliance. The Battenburg pattern shall be applied to the crew cab to blend in with the cab contours whilst maintaining the overall profile of the Battenburg pattern along the full length of the appliance. Individual squares in the Battenburg pattern shall measure between 700mm and 900mm square (note, other variations will also be considered).
150mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Reflective Yellow strips to be positioned along the length of the Header Panel overhead the lockers on either side of the appliance. The name of the Brigade shall be applied in English on the nearside header panel and in Irish on the offside header panel in red writing – the wording for the name of the Brigade in English and Irish shall be supplied at the time of placing the official order for the appliance.

	
	

	5.6
	The rear of the appliance shall be striped in alternating yellow and red 100mm High Visibility Avery Dennison Omnidirectional for homogenous night-time visibility (or equivalent) Reflective strips in inverted V style. The inside of the barn doors shall match the striping profile on the rear of the appliance when they are opened.
	
	

	5.7
	[bookmark: _Hlk206685043]Brigade Crest Transfers shall be placed on either side of the appliance. In addition, the Local Authority Crest and name shall be applied to the Battenburg on the driver and passenger doors. The detail shall be agreed at the pre-build meeting. The supplier shall be responsible for printing the crests in colour on clear vinyl transfers. The electronic files shall be supplied by the Brigade when placing the official order.
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6 Electrical Systems

	Item
	Description
	Complies
(Y/N)
	Comments/ 
Variations

	6.1 
	All electrical wiring shall be of adequate gauge and insulation for the designed load, and where exposed shall be waterproof and corrosion free. 
All electrical wiring shall be suitably protected from damage and from the elements. All electrical wires and small air pipes shall be run in conduit within the bodywork. The conduit shall be fixed to the bodywork, easily accessible for maintenance and remain in place for the life span of the appliance. 
All important electrical circuits shall have separate circuit breakers, suitably indicated and grouped into a common box located in an accessible position within the cab.

	
	

	6.2 
	The electrical system shall be 24V negative earth with 2 No. 180 amp hour heavy-duty maintenance free batteries in series fitted in an accessible position. 

	
	

	6.3 
	LED lighting of the cab doors and steps to aid access/egress shall illuminate automatically when the corresponding door is opened. 
There shall be a means of switching on the cabin lighting when the doors are closed – the cabin lights shall be red to minimise distraction for the driver if turned on when the appliance is being driven.
Red LED strip lighting shall be provided on the edge of the doors to increase the conspicuity of the doors when they are opened at night-time. The LED strip shall illuminate automatically on a particular door if that door is opened when the sidelights are turned on.

	
	

	6.4 
	A Low Profile full width Blue Light bar shall be fitted on the roof of the cab that is visible to oncoming traffic containing the following:
a) LED in a rotation pattern at either end of the light bar;
b) 4 No. Independent forward and rear facing LED alternating flashing lights, two either side of the centre of the Light bar;
Make & model of Light Bar proposed:
Tenderers to fill in details Here:


	
	

	6.5 
	A remote electronic 200-watt siren system shall be fitted, incorporating ‘wail’, ‘yelp’, and public address functions. Activation of the ‘wail’ and ‘yelp’ tones shall be possible via a dash-mounted switch accessible to the Officer, a floor-mounted switch at the driver’s position, or by depressing the vehicle horn. The system shall include a low-frequency pulsing howler module, with dedicated speaker(s) if required, designed to enhance audible warning effectiveness in high-noise and high-traffic environments. The howler shall operate in conjunction with the primary siren amplifier, generating synchronized low-frequency tones that are both heard and physically felt.
Make & model of Electronic Siren proposed:
Tenderers to fill in details Here:


	
	

	6.6 
	An independent set of air operated two tone horns shall be fitted and they shall be driver operated through a momentary switch. The horns shall be fitted in a location behind the front grille in an area that does not affect their effectiveness.
	
	

	6.7 
	4 No. Dual blue/white alternating LED’s shall be fitted to the front of the appliance. The lights shall flash alternating white when:
a) the handbrake is off;
b) the blue lights are on; and
c) the vehicle lights are off.
The lights shall flash alternating blue at all other times when powered on. 

	
	

	6.8 
	LED Blue alternate flashing lights shall be fitted as follows:
a) 2 No. on both sides of the appliance;
b) 2 No. on the rear of the appliance;
c) 2 No. on the rear corners (1 per side) of a locally recessed chamfered portion of the bodywork to allow the lights to flash at an angle of 45° to the rear of the appliance;
d) 2 No. Blue RSG (or equivalent) alternate flashing intersector lights on each side of the number plate mount
Make & model of LED Blue Lights proposed:
Tenderers to fill in details Here:


	
	

	6.9 
	A light mast shall be fitted as follows:
a) Minimum 5m (to the bottom of the lamps) above ground level when erected;
b) Vertical, telescopic, non-turning tube style light mast with the vertical tubes fitted in the space between the bodywork and the crew cab. The final location will be agreed at Pre-Build meeting stage;
c) A decal advising the operator to check for overhead cables before raising the mast shall be located beside the controller;
d) An adjustable air regulator, mast controller complete with an air pressure gauge to be positioned in the pump bay locker;
e)  4 No. 1,100 Lumen, rated 24V LED Lamps on each light mast;
f) Light mast to be IP68, RoHS and EMC rated;
g) Blue Beacon on top of light mast;
h) Protective Guard / Deflector plate shall be fitted to the roof of the appliance to protect mast from damage from trees in the housed position;
i) Handbrake Interlock shall be fitted with an audible alarm and supplemented with a flashing red LED light in the cab 
j) Wanderlead controller shall be provided to operate the unit. From this unit it shall be possible to raise, park and rotate the light mast. Auto-park and auto-park cancellation must be provided available on the controller.
Where possible the light mast should be a non-folding light mast and the vertical tubes should be fitted in the space between the bodywork and the crew cab. The final location will be agreed at Pre-Build meeting stage.
Make & model of Light mast proposed:
Tenderers to fill in details Here:


	
	

	6.10 
	LED Scene Lights shall be fitted as follows:
a) 2 No. on both sides of the appliance bodywork;
b) 2 No. on the rear of the appliance (note, these 2 No. rear scene lights should also automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected);
Scene lights shall be interlocked with the handbrake so that they automatically switch off when the handbrake is released. Manual operation of the scene light shall be possible at speeds less than 20kph. There shall be a facility to switch on the LED Scene lights from the pump bay.
Make & model of LED Scene Lights proposed:
Tenderers to fill in details Here:


	
	

	6.11 
	A VMS Sign shall be supplied and fitted to the roof of the appliance at the rear. The VMS sign shall be of approximate dimensions 1,200mm wide x 600mm high and shall be no higher than 300mm in the closed position. The VMS sign shall be deployable to 90° or folded to the closed position through a switch in the crew cab. The frame shall be constructed from heavy gauge aluminium and shall be powder coated in red.. The VMS frame shall have a high strength polycarbonate screen. The display screen shall have a minimum of 32 x 64 matrix graphics/led modules with a minimum visible angle of 25°. A controller, with a minimum of a 50mm wide display screen, shall be mounted in the crew cab to display to display what is on the sign. A minimum of 50 pre-programmed messages shall be stored such that they can be easily selected for display. It shall be possible to free programme messages at any time. 
Make & model of VMS proposed:
Tenderers to fill in details Here:


	
	

	6.12 
	A Reversing Camera shall be mounted above the pump bay locker fitted with a flat screen colour display located on top of the dash. The display shall be at the same eye-line height as the appliance mirrors and shall not interfere with the drivers view and the camera shall automatically come on when a reverse gear is selected and should automatically go off again when the reverse gear is de-selected. There shall be a manual override facility to leave the camera switched on permanently also.
	
	

	6.13 
	A Reversing Proximity Sensor with an audible alert shall be fitted in the dash.
An Audible Alarm warning that the vehicle is reversing shall be fitted. A Facility to turn off this alarm shall be fitted on the dash. The switch shall be reset once the appliance is switched off.
Low Level Rear light clusters shall be LED and repeated at roof level and all rear lights shall be flush mounted.

	
	

	6.14 
	White LED strip lighting shall be provided in both frames on either side of all stowage lockers the full height of the frames. Locker lights shall automatically switch on in a particular locker when that locker is opened if the sidelights are turned on.

	
	

	6.15 
	An LED strip light shall be installed overhead the pump compartment to illuminate the area for maintenance activities. The light shall be switchable on/off within the pump bay.

	
	

	6.16 
	An Electronic Management Control System shall be fitted with the following characteristics:
a) [bookmark: _Hlk206594316]The System shall have sufficient input and output ports to deliver all functionality with spare redundancy for future expansion;
b) A touchscreen with the following characteristics shall be located on the dash that will enable the operator to activate warning systems, lighting and other functions;
c) The touchscreen shall be capable of providing information using both visual and audio alerts;
d) The touchscreen shall allow the operator to activate pre-programmed audio / visual warning patterns such as ‘999’ and ‘In Attendance’ and to individually control all blue lights;
e) The system shall have J1939 and Generic CAN Bus Integration;
f) [bookmark: _Hlk206594437]The system shall incorporate a run-lock capability;
g) The system shall integrate with the siren solution;
h) The system shall have an on-board interface for programming;
i) An accessory load management system shall be included to isolate circuits should the vehicle not be generating sufficient power to run the accessories, without using battery power. The system shall reintroduce the accessories, automatically, when power is available. The system shall not interfere with the standard vehicle equipment required for road driving. The system shall also offer thermal protection;
j) The Hardware must be CE marked 
k) The hardware must comply with Regulation 661/2009 and any subsequent amendments under the EU Whole Vehicle Type-Approval System
Make & model of Electronics Management System proposed:
Tenderers to fill in details Here:


	
	

	6.17 
	A 110 / 220 Volt input socket with an Auto-Eject System shall be fitted to the appliance to keep the batteries automatically charged in situ or alternatively a 24 Volt input socket with an Auto-Eject System shall be fitted to the appliance to keep the batteries automatically charged in situ The supply voltage shall be specified at the time of placing the official order. 
Make & model of Auto-Eject System proposed:
Tenderers to fill in details Here:


	
	

	6.18 
	A 110 / 220V Top-Up compressor complete with wiring and socket shall be fitted with a minimum capacity of 0.45 m3/min. 
Make & model of Top-Up Compressor proposed:
Tenderers to fill in details Here:


	
	

	6.19 
	A Run lock and Keyless running facility shall be fitted where available from the chassis supplier. Where not provided by the chassis supplier, the supplier shall retrofit an electronic solution to provide a keyless running solution.

	
	

	6.20 
	Accidental turning off of the master switch when the appliance is moving should not turn off the appliance and should not affect the driving of the appliance. A time-delay mechanism shall be integrated into the master switch system. The delay duration shall be recommended by the chassis supplier and shall account for the operational requirements of electronic systems and the AdBlue pump.

	
	

	6.21 
	· 1 No. Twin Metal 110 V / 220V Sockets with USB charging ports, switchable, fused and with a red light on each switch indicating whether powered up or not, shall be fitted to the bulkhead between the driver and the Officer for the charging of fire service radios, tablets etc. – the exact voltage shall be confirmed in the Pre-Build Meeting.
· 4 No. combined USB and USB-C charging points shall be fitted to the bulkhead between the driver and the Officer.
· 2 No. 12V Sockets shall be fitted in the cab – the exact location shall be confirmed in the Pre-Build Meeting.

	
	

	6.22 
	Warning lights with an audible device shall be mounted on the dash to indicate the following:
a) Locker open;
b) Cab or Crew cab door open;
c) PTO Engaged;
d) What seat belts are not in use
e) When snow chains are deployed
	
	

	6.23 
	The supplier shall arrange for a third party approved supplier to supply and fit all necessary Tetra Hardware to the appliance other than the radio base (the radio base will be provided Free Issue by the Fire Authority). This shall include the supply and fitting of all Control Heads, Microphone Heads, Speakers, Antennas, all necessary cabling, brackets, clips and pump bay kits. The current C Trí approved third parties are Tetra Ireland and Sigma Wireless. In addition
a) The supplier shall run a free issue wiring loom from the agreed location of the radio to the agreed location of the control head
b) The supplier shall run a free issue wiring loom from the agreed location of the radio to the agreed location of the Pump Bay Voice Terminal in the pump Bay
c) The supplier shall run a free issue wiring loom from the agreed location of the radio to the agreed location of the aerials (Tetra and GPS)
d) The supplier shall provide a 12/24V DC supply at the agreed location of the radio
e) The supplier shall provide a 12/24V DC supply at the agreed location of the Pump Bay Voice Terminal in the pump Bay
Note, the supplier shall be responsible for all costs associated with the above items in this Section, including payment to the Third Party Supplier.
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7. Fire Engineering 

	Item
	Description
	Complies
(Y/N)
	Comments/
Variations

	7.1 
	A Chelsea PTO (or equivalent) shall be supplied (if not supplied with chassis). Any moving part of the PTO shall be guarded against contact by the operator during use.
The pump shall be capable of being engaged / disengaged from both the cab and the pump bay in a single operation (i.e. depress one switch only). A light shall illuminate on the pump bay panel when the PTO is engaged.
Make & model of PTO proposed:
Tenderers to fill in details Here:


	
	

	7.2 
	A low-pressure alloy single stage pump with the following criteria shall be fitted:
a) Nominal low-pressure delivery of 2,000l/min at a nominal delivery pressure of 10bar and a maximum operating pressure of 17bar at 3m suction lift;
b) Automatic Primer;
c) An induction system , commonly known as a round the pump proportioner, for inducting road cleaning detergent or firefighting foam into the discharge stream of the pump. The solution shall be picked up using a pickup tube, inserted into either the road cleaning detergent or firefighting foam 20 litre drums which will be stored in a suitable locker. The pickup tube should be sufficiently long to enable it to be dropped into an external storage intermediate bulk container (IBC) of either road cleaning detergent or firefighting foam. The induction rate shall be controllable between 0 and 6% through a calibrated valve. The solution shall be delivered to either the delivery valves or the spray bar ( see 7.6 below ).
d) Two crank handle continental style dual flow delivery valves fitted with female instantaneous couplings, each with a blank rubber cap;
e) An integrated twin inlet collecting head
f) The pump suction eye shall be provided with a blank metal cap;
g) The suction inlet shall be fitted with a conical strainer;
h) Any cooling loop shall not return inducted solution to the main tank;
i) A drain valve shall be fitted;
j) Thermal and pressure relief valves shall be fitted;
Note, the cost of any consumables including road cleaning detergent and foam incurred in testing and commissioning the pump shall be borne by the supplier. 
Make & model of Pump proposed:
Tenderers to fill in details Here:


	
	

	7.3 
	A vented on-board tank with a minimum capacity of 8,000 Litres shall be incorporated into the body work. The tank shall be fitted with an appropriate pressure relief valve to prevent the structural integrity of the body. The final volume will be confirmed during the build stage to ensure the maximum possible water stowage is achieved while remaining within legal weight limits for the fully equipped appliance, including crew and equipment. An overflow pipe capable of discharging at 4,000l/min shall be provided. The tank shall be equipped with internal longitudinal and lateral baffles to minimise water surge during transit when the tank is partially filled.

	
	

	7.4 
	1 No. Sight Tube Gauge for Water Tank contents with illumination shall be fitted in the pump bay. Valves to isolate the gauge to allow for removal and cleaning shall be installed. 
	
	

	7.5 
	All associated pipe work and valves shall be fitted. The pipework shall be designed to withstand maximum operating pressures. Anti-surge valves shall be fitted to prevent damage to the pump or pipe work. Access panels shall be provided in lockers for maintenance of the main pump. No fixed panelling / shelving shall impede the removal of the volute from the pump for maintenance purposes.
	
	

	7.6 
	1 No. stainless steel Spray Bar shall be fitted:
a) At low level underneath the front bumper but with sufficient ground clearance to avoid damage. Note, the Fire Authority may wish to agree an alternative location at the rear of the appliance at the pre-build meeting.
b) The spray bar shall be used to wash oil spills from roadways using a water and detergent mix solution.
c) The spray bar shall be the full width of the appliance with 7 evenly distributed nozzles fitted to the spray bar.
d) The outer nozzles shall be located as close as possible to the extremities of the spray bar to maximise the coverage of detergent solution.
e) An electronic valve, switched in the cab, will turn on / off the spray bar.
f) It shall be possible when the spray bar is turned on to deliver either water or water with an inducted road detergent to the spray bar - there shall be independent switches for both in the cab, i.e. the operator will have the option of delivering either water directly from the tank or water with inducted road detergent solution to the spray bar regulated at 3 to 4 Bar pressure.
g) It shall be possible to drive the appliance at a maximum speed of 20kph, or in first gear only, in pump on the run mode when the PTO is engaged.
h) The spray bar, nozzles and pipework shall be designed to withstand the maximum pump pressure, and the supply shall be filtered to prevent grit entering the nozzles.
i) It shall be possible to dump the water solution to the spray bar / underneath the appliance when the water temperature reaches 38°C (this is an additional safety feature to the thermal relief valve on the main pump in 7.2 above).
	
	

	7.7 
	2 No. taps, suitable for dispensing drinking water into containers, shall be provided in a suitable easy accessible location to allow for simultaneous ease of filling. 
	
	

	7.8 
	A water feed pipe of minimum 100mm diameter shall be fitted between the tank and the main pump. A manual ball valve to open or close the tank to pump valve shall be fitted.
	
	

	7.9 
	A hydrant to tank fill system, with twin male instantaneous couplings shall be fitted incorporating strainers or filters and shall be connected to a 100mm tank fill pipe. The couplings shall be located in the pump bay at a position that is easy to connect and disconnect a delivery hose. A manual ball valve to open or close the tank fill valve shall be fitted.

	
	

	7.10 
	The appliance shall be supplied with 4 No. Lengths of 100mm x 2440mm clear hard suction hose, 4 No. Suction Keys and 1 No. Round Thread 100mm Combined Suction and Strainer Basket. 

	
	

	7.11 
	The appliance shall be supplied with 1 No. self-supporting Water Dam capable of containing 110% of the water stored in the appliance. The dam shall be made from durable heavy-duty material. The dam sides shall automatically lift with the water level when filled and shall have a flotation collar around the dam rim, filled using a hand-pump connected to a non-return valve. Crease removing straps shall be fitted to the dam. The dam shall have a low-level 100mm female suction hose coupling with a shut off valve. 2 No. low level instantaneous non-return couplings shall also be fitted to the dam for pressure feeding the dam. The dam should have a durable storage bag, with suitable carrying handles, capable of storing the dam after multiple uses (i.e. allowance should be made for the dam not being folded into its’ original size after multiple uses). All valves should be removable (to avoid damage to the dam in storage) and provision should be made for storing them in a locker, secured with appropriate bracket(s) – see 4.7.2 above for equipment stowage requirements.

	
	

	7.12 
	An IP66 rated (or equivalent) Emergency Engine Stop Button shall be provided in the pump bay.
	
	

	7.13 
	An IP66 rated throttle control lever (or equivalent) shall be fitted in the pump bay to increase or lower engine revs. A control device shall be provided to immediately drop the engine revs to the engine idling speed.

	
	

	7.14 
	The following gauges and controls shall be fitted in the pump bay:
a) PTO Engaged Warning Light
b) Dampened Low Pressure Gauge;
c) Dampened Compound Pressure Gauge;
d) Engine RPM Meter;
e) Pump Hour Meter;
f) Engine warning indicator – audible and visual;

	
	





8. [bookmark: _Toc471745514][bookmark: _Toc471814388][bookmark: _Toc471827371]Spare Parts, Warranties and Delivery

	Item

	Description
	Complies
(Y/N)
	Comments/
Variations

	8.1 
	It is a requirement that the bodywork must have a minimum of 15 Years Warranty. 
	
	

	8.2 
	It is a requirement that all other parts of the appliance (including ancillary equipment) other than the chassis must have a minimum of 2 years warranty.
	
	

	8.3 
	
	It is a requirement that the chassis vehicle systems and driveline must have a minimum of 2 years warranty (other than standard serviceable items). 
	
	

	8.4 
	Spare Parts and Technical Assistance shall be available for a minimum of 15 years for the appliance and all ancillary equipment. Suppliers should have a network of support throughout the Republic of Ireland for both chassis and fire engineering support including trained technical personnel based in the Republic of Ireland and appropriate transport for these personnel and spare parts. A stock of all commonly used spare parts should be available at a store in the Republic of Ireland. Suppliers should have the ability to have a trained technical person present at any Fire Station throughout the Republic of Ireland within 12 hours from receipt of call-out.

	
	

	8.5 
	Tenderers must state their delivery lead time (in weeks) for a complete solution for each chassis option. 
The lead time shall be taken as the period from the date of the official order placement to the delivery on station of a fully approved appliance.
Delivery will be to Waterford City Fire Station, Kilbarry Road, Waterford.
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Award Criteria 2 – Experience & Qualifications of Staff
	Criterion 2:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Experience & Qualifications of Staff
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must provide details and examples of the relevant qualifications and experience of its employees engaged in the build/assembly of Class B Water Tender, Emergency Tender, Aerial Appliance, Water Tanker or Incident Command Unit, and also of any subcontractors engaged in the process.
Include details of the number of
i. technicians/mechanics employed and their qualifications; 
ii. their experience building fire appliances;
iii. ongoing training/upskilling; and any other information which demonstrates that its staff have the requisite skills and experience. 

	Tenderers’ Response















[bookmark: _Hlk217996479]
Award Criterion 3 – Aftersales Support & Technical Assistance 
	Criterion 3:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Aftersales & Technical Assistance 
	
	
	

	
	10%
	100
	60

	Instructions
	The Tenderer must set out the quality of its proposal in relation to its capacity and capability for the provision of maintenance, repair and technical assistance from its workshop facilities, and its capacity and capability for      repair/maintenance services on-site at Waterford City & County Council. Tenderers must provide details of workshops, if any, they have in the Republic of Ireland to carry out both chassis and Fire Engineering repairs. The Tenderer should also provide details of the process by which clients’ repair issues are managed from the time a fault is reported through to   successful conclusion. If sub-contracting after sales support to another supplier, full details must be provided of that sub-contractor, including their workshop details (for both chassis and Fire Engineering repairs), network details, technical capabilities of their employees in relation to fire-engineering support and their qualifications for same, and details of stock they carry and where the stock is located.


	Tenderers’ Response











Award Criterion 4 – Availability of Spare Parts
	Criterion 4:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Availability of Spare Parts 
	
	
	

	
	10%
	100
	60

	Instructions
	
The Tenderer must set out the quality of its proposal for ensuring the availability of all spare parts for the appliance and ancillary equipment for the minimum expected lifespan of the vehicle (15 years). 
The Tenderer should include details of its process and lead times for obtaining spare parts; how it manages this supply chain to ensure parts are delivered on time; and how it manages instances of order delays and parts being out-of-stock.


	Tenderers’ Response
















Award Criterion 5 – Ordering & Delivery
	Criterion 5:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Ordering & Delivery  
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative demonstrating its high-level process and timescales for the successful delivery of a Water Tanker - from the time of the official order through to full commissioning and handover of the appliance.
The Tenderer should Include details of the tenderer’s methodology for ensuring that all appliances are supplied and delivered in accordance with the requirements specified by the client.


	Tenderers’ Response

















Award Criterion 6 – Environmental & Sustainability Efficiencies
	Criterion 6:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Environmental & Sustainability Efficiencies 
	
	
	

	
	5%
	50
	30

	Instructions
	
The Tenderer must provide a detailed narrative to demonstrate how it incorporates environmental and sustainability efficiencies/measures during the build   process. For example:
· Energy optimisation initiatives in the              warehouse/premises including rain harvesting, use of PV Panels, fabric of the building including insulation, efficiency of lighting and heating, EV charging capabilities etc.
· Use of recycled and/or recyclable material
· Waste management/disposal/recycling
· Minimisation of waste
· Transport and logistics measures
· Corporate Social Responsibility policies
· Proposed Targets for Environmental Sustainability
· Sustainable purchasing


	Tenderers’ Response












Award Criterion 7  – Cost
	Criterion 7:  
	Weighting
	Maximum Marks
	Minimum Marks Required

	Cost  
	
	
	

	
	60%
	600
	N/A

	Instructions
	
The Tenderer must give the total cost, in Euros , of the vehicle as specified in Appendix 1
· Including delivery to Waterford
· Including firefighting equipment & ancillary equipment  specified in Section 4 of Appendix 1 
· Including all expenses/ tariffs/ custom charges
· Excluding VAT 



	Total Cost  ( ex. VAT )
	€



I/We confirm that I/we: 

1. Will keep this offer for the contract open for acceptance by you for a period of 12 months from the date of deadline for submission of Tenders,
2. Agree that you are not bound to accept the most economically advantageous or any Tender you may receive,
3. Have read and thoroughly examined the Tender Document,
4. Fully understand the Tender Document and the Client’s requirements,
5. Undertake to treat the details of this Invitation to Tender, its Tender and any subsequent agreements as private and confidential,
6. Acknowledge that acceptance by the Contracting Authority of this tender will not constitute a binding and enforceable agreement and that a legally enforceable agreement will not exist until and unless the contract is awarded between the Contracting Authority and the Tenderer,
7. Have availed of all offers for additional information or have otherwise satisfied myself/ourselves as to conditions that may in any manner affect the performance of the contract,
8. Have included all elements necessary for the performance of the specified requirements, which are either expressly stated in the Tender Document or contained in any supplementary information or which could reasonably be inferred therefrom,
9. Have found no errors, omissions, conflicts or ambiguities in the Tender Document except those which I/We have brought to the attention of the Contracting Authority before the latest date for submitting queries,
10. Have included for compliance with all statutory requirements applicable in Ireland and those applicable in any country where parts of the contract may be performed that are in force 7 days prior to the deadline for receipt of Tenders, 
11. Will not, if awarded a contract employ labour in a manner that is discriminatory in relation to gender, civil/family status, sexual orientation, religion, age, disability, race, or membership of the traveller community.
12. [bookmark: _Hlk491592638]Agree that as a condition of award, it shall be our sole responsibility to fulfil the obligations under the Contract, notwithstanding any changes in circulars, laws, regulations, taxation, duties or other factors which might arise following the withdrawal of the United Kingdom from membership of the EU.
	Signed:
	

	Name (in Capital Letters):
	

	On behalf of:	
	

	Address:
	

	Telephone:
	
	Mobile:
	

	Email:
	
	Date:
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