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JAMES STEPHENS  PARK

Supply and Installation of Third Generation G Synthetic Playing Surface Pitch 
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Name- Ballina Stephenites GAA
Contact Mr. Vincent Lang 086-3086047 

Nature- Work Scope for the Anthony Golden Park Phase 1 – Construction of Site Access, a Multi-Use Natural Grass Pitch and an Exercise Circuit

Location- James Stephen’s Park, Ballina, Co. Mayo. F26EW22
Ballina Stephenites GAA Club proposes to construct a new third-generation (4G) synthetic playing pitch within the Club grounds at Ballina, County Mayo.

The overall project will be delivered in separate work packages. The formation, drainage, granular sub-base, porous base and shock pad will be constructed under separate contracts and do not form part of these Works.

This Contract comprises the supply, delivery and installation of approximately 3,705 m² of third-generation (4G) synthetic grass carpet together with kiln-dried silica sand infill, performance infill, permanent inlaid line markings, jointing materials and all ancillary works necessary to provide a complete finished synthetic playing surface.

The successful Contractor shall install the synthetic playing surface onto the prepared shock pad and porous base to be provided by the Employer prior to commencement of these Works.
The completed playing surface shall be suitable for Gaelic Games and Association Football and shall be complete in every respect in accordance with the Contract Documents.

[bookmark: _Toc237184786]SCOPE OF WORK

The Contractor shall supply, deliver and install a complete third generation (4G) synthetic grass playing surface to a prepared shock pad and porous base which will be provided by others.

The work shall include all labour, materials, plant, transport, supervision, equipment and incidental work necessary to complete the installation.

The playing area measures approximately 47.5 meters × 78.0 meters (3,705 m²).
The Contractor shall inspect the prepared shock pad and base before commencing installation. Commencement of installation shall constitute acceptance that the prepared surface is suitable for the Works. Any defects observed shall be reported to the Employer in writing before installation commences.
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The Contractor shall supply and install a complete synthetic turf system comprising:
•	60 mm monofilament synthetic grass carpet. 
•	proprietary jointing tapes and adhesives. 
•	kiln-dried silica sand infill. 
•	performance infill. 
•	permanent inlaid line markings. 

All components shall be compatible with each other and recommended by the system manufacturer.

The proposed synthetic turf system shall be an established proprietary sports surface manufactured by a recognised manufacturer with a proven record of successful installations within Ireland or the United Kingdom.
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The synthetic carpet shall:
•	be a third generation (4G) sports surface. 
•	comprise monofilament polyethylene fibers. 
•	have a nominal pile height of 60 mm. 
•	be UV stabilised. 
•	be fully permeable. 
•	be suitable for year-round outdoor sports use under Irish climatic conditions. 
•	be suitable for Gaelic Games and Association Football. 

The complete playing surface shall be suitable for the playing of Gaelic Games and Association Football and shall be installed in accordance with the manufacturer's published recommendations for the proposed system.
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The Contractor shall install kiln-dried silica sand together with an approved performance infill in accordance with the manufacturer's recommendations.
The Contractor shall identify the proposed performance infill material in the Tender.
All infill materials shall comply with applicable Irish and European environmental and product safety requirements.
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Permanent tufted and inlaid line markings shall be provided as per the drawings.
All line colours shall be agreed with the Employer before manufacture.
Painted lines shall not be accepted.
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Installation shall be carried out by suitably experienced personnel in strict accordance with the manufacturer's written installation procedures.

All joints shall be securely formed using proprietary jointing tape and adhesive recommended by the system manufacturer.

The completed surface shall be:
•	uniform in appearance. 
•	free from wrinkles. 
•	free from ridges. 
•	free from depressions. 
•	free from loose joints. 

Contractors should keep the site clean and remove all surplus materials and waste upon completion.

The Contractor shall inspect the completed shock pad before commencing installation. Commencement of installation shall constitute acceptance by the Contractor that the shock pad is suitable for the installation of the synthetic turf system. Any defects identified shall be notified to the Employer in writing before work commences.
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The completed synthetic surface shall:
•	provide a safe, even and durable sports surface. 
•	provide effective drainage. 
•	be suitable for year-round outdoor use. 
•	be capable of accommodating Gaelic Games and Association Football. 
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The Contractor shall provide:
•	a minimum 10-year manufacturer's warranty on the synthetic carpet. 
•	all manufacturer's warranties relating to the proposed synthetic turf system. 
•	a minimum 2-year workmanship warranty. 
Warranty documentation shall be provided prior to Practical Completion.
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Upon completion the Contractor shall provide:
•	manufacturer's product data sheets. 
•	warranty certificates. 
•	maintenance recommendations. 
•	maintenance schedule. 
•	layout drawing showing all line markings. 
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The Contract Sum shall include full compensation for:
•	supply of all materials. 
•	transport. 
•	labour. 
•	plant. 
•	installation. 
•	jointing. 
•	infill installation. 
•	line markings. 
•	testing by the Contractor. 
•	cleaning. 
•	completion documentation. 
•	warranties. 
•	all incidental works necessary for the satisfactory completion of the Contract.
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The following items do not form part of this Contract:
· Site clearance and enabling works.
· Demolition works.
· Earthworks and excavation.
· Formation preparation.
· Drainage works.
· Underground drainage connections.
· Ducting and underground services.
· Granular sub-base.
· Porous macadam or equivalent porous base.
· Shock pad.
· Kerbing and edgings.
· Concrete works.
· Fencing and gates.
· Ball stop netting.
· Floodlighting.
· Electrical installations.
· Irrigation systems.
· Goalposts and sports equipment.
· Landscaping and reinstatement.
· Footpaths and external paved areas.
· Car parking works.
· Utility diversions.
· Statutory approvals.
· Maintenance of the completed playing surface following Practical Completion (other than the provision of maintenance recommendations and warranty obligations).

The Employer shall provide a completed porous base and installed shock pad prior to commencement of this Contract.

The Contractor shall inspect the prepared surface before commencing installation and shall notify the Employer immediately of any defects or deficiencies considered likely to affect the satisfactory installation or long-term performance of the synthetic playing surface. Commencement of installation shall constitute acceptance by the Contractor that the prepared surface is suitable for the execution of the Works.
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