                                              Volume A – Technical Specifications
Project: Installation of A New 800m x 2.4m walking track with associated lighting and fencing.
Contracting Authority:  Eire Og Corra Choill Hurling & Camogie Club, 
Location:  Eire Og Corra Choill Hurling & Camogie Club, Donore, Caragh, Naas, Co Kildare.

Contract Type: Short Public Works Contract (PW-CF6)
Contract Duration:  3 months from date of site possession

A1 – Scope of Works
The Contractor shall provide all labour, materials, plant, and supervision necessary for the construction and installation of New 800m x 2.4m walking track with associated lighting and fencing including:
· All preliminaries including transportation, site set up & H & S 
· Excavate topsoil from trackway and stockpile on site 
· Supply and install 100mm x 25mm treated timber kerb 1600m approx. 
· Supply and install theram weed clothe
· Supply and install hardcore aggregate and compact 
· Supply and install dusting and compact 
· Ducting, Foundation Bases and standing of poles for lighting
· 6m poles with 3 wattage changeable LED street lighting
· Supply and Install 1200mm high Irfen® Specterail Standard Mesh System (or equivalent) with 200 x 50mm mesh
· with three reinforcement crimps. Posts & Top rail 60 X 60mm SHS at 3030mm post centres. Finish: Galvanised & Powdercoated (Plasgalv®), Colour: Green RAL
· Single Leaf 90º Left gate of width required 1.2m high x 1.2m wide infilled with Kinsale Mesh Gate (or equivalent).
· Frame 60 X 60mm SHS Mitred corners with fully welded joints Infill to be affixed to frame by full welds or by clips specified by Irfen®, to be supplied with Irfen®(or equivalent) drop bolts and receivers, adjustable Irfen® hangers, and Sliding Bolt+Drop Bolts locking system. Installed to Gate Posts of 80 x 80 +Hangers. Finish: Galvanised & Powdercoated (Plasgalv®), Colour: Green RAL
· Double Leaf 90º gate of width required 1.2m high x 4.0m wide infilled with Kinsale Mesh Gate. Frame 60 X 60mm SHS Mitred corners with fully welded joints Infill to be affixed to frame by full welds or by clips specified by Irfen®, to be supplied with Irfen® drop bolts and receivers, adjustable Irfen® (or equivalent) hangers, and Sliding Bolt+Drop Bolts locking system. Installed to Gate Posts of 100 x 100 + Hangers. Finish: Galvanised & Powdercoated (Plasgalv®), Colour: Green RAL


A2 – Performance and Quality Standards
The completed installation shall:
· Meet all relevant Irish Building Regulations, Health & Safety, and local Planning Authority provisions.
· Use only CE-marked and REACH-compliant materials. 
· Include a 5-year workmanship warranty on installation.

A3 – Contractor Requirements
The Contractor must demonstrate:
· Successful delivery of at least two (2) similar projects within the last five (5) years.
· Appointment of a Site Supervisor with CIF Safe Pass and PSCS training.
· Valid Public Liability Insurance (€6,500,000) and Employer’s Liability Insurance (€13,000,000).
· Compliance with the Safety, Health and Welfare at Work (Construction) Regulations 2013.
· Submission of a Construction Programme and Quality Plan for Client approval prior to commencement. 
· Compliance with the Safety, Health and Welfare at Work (Construction) Regulations 2013.
· Submission of a Construction Programme and Quality Plan for Client approval prior to commencement.

A4 – Drawings and Supporting Information
Draft drawings are attached, the Contractor shall refine these drawings detailing the installation and submit same for Client approval prior to commencement of works.

A5 – Testing and Handover
Prior to Practical Completion, the Contractor shall;
· Arrange independent testing
· Provide as-built drawings, drainage test results, and a maintenance manual.
· Deliver training to Club representatives in correct walking track maintenance procedures.
· Submit all warranties, certificates, and completion sign-off documentation.

A6 – Environmental and Community Requirements
The Contractor shall:
· Minimise waste generation and transport movements.
· Prevent contamination of adjacent land, watercourses, or drains.
· Ensure safe working practices around live club facilities and neighbouring properties.
· Reinstate all disturbed areas to equal or better condition than prior to works commencement.

A7 – Completion and Defects Period
· Practical Completion shall be deemed achieved once the work has been completed certified compliant.
· Defects Liability Period: Twelve (12) months from the date of Practical Completion.
· The final inspection shall be carried out jointly by the Client and the Contractor’s independent testing body.

