We have a question regarding Appendix 1 A16
XXXX The system MUST be capable of positive and negative ion detection, with the capability of within-run switching between either mode and MUST have a polarity switching time of 10 ms.XXXX
Is there a particular method that requires polarity switching of 10ms ? Is this a mandatory requirement that excludes a vendor without this specification from the evaluation? Would a polarity switching time of 25ms be acceptable, if it can be clearly demonstrated that all the necessary data points are collected to give reproducible peak shape and quantitation at a switching speed of 5ms?
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“With respect to the query raised, it will be the decision of the evaluation team once appointed, to appraise the entire offering from all tenderers and consider all pertinent information provided in response to the technical requirements listed in Appendix 1.”

