
Tender Response Document (TRD)


Section A

Table 1
	
Turnover Requirements; (> €500,000 Annually)
	Annual Turnover (€)
	

	State Annual turnover here and provide a copy when requested of most recent annual accounts or a statement from your Accountant that the most recent annual turnover threshold for this tender can be met. By entering your annual turnover on this form you commit to providing evidence prior to award of contract.
	
	Pass/Fail











Table 2
	Tax Clearance 
	Tenderers must provide evidence with their tender of having Irish Tax Clearance in the form of a copy of their Certificate/Compliance (TCC Form) or other proof acceptable to the DAFM. 
	Provided 

Yes/No

	Pass/Fail 

	Insurance 
	Tenderers must provide evidence with their tender of having appropriate levels of insurance as detailed in section 2.21.1 or a letter from Insurance Provider confirming that the requested level of insurance can be provided upon award of this contract.
	Provided

Yes/No
	Pass/Fail




Table 3

	Tenderers to detail their current capacity and recent experience (within the last 5 years) in delivering similar goods and providing similar after sales service as required by this contract. Give details of recipient, contact details, details of goods and guarantee/maintenance services delivered. Only provide examples if client approval for DAFM to contact them has been granted. 

	






Section B
COMPLIANCE TO SPECIFICATION FORM

0. Specification for (180 H.P.) 4 WD LWB Tractor with Five-Year Warranty and Five-Year Service/Maintenance Package
0. 
Company tendering: 
	Description
	Please complete in respect of your offer
	Confirm your level of compliance with any additional remarks/notes necessary and to illustrate exceeding the minimum requirements specified.
	For DAFM use only

	0. The Tenderer shall comply fully with the requirements set out in this document. Not complying with the minimum requirements as outlined in the specification below shall be deemed a failure to comply and the tender may be rejected. The requirements below shall be treated as pass/fail criteria. Refer to RFT for further requirements.



	 Note: Product Information:
The specification, technical data information and after sales terms and conditions in the catalogues and brochures provided for DAFM reference purposes, will be considered as being representative of the tractor offered.
	
	

	1) General:

A 180HP  4Wheel Drive Long Wheel Base Tractor 



The Tenderer shall supply the quantity actually ordered during the currency of this contract to meet the requirements of the DAFM at the prices stated in the tender, whether they be more or less in any degree than the quantity stated in the schedule.

Minor variances to the specifications may be taken into account and considered at competition assessment stage. 
This shall be solely at the discretion of the DAFM.

	

State Specification & Confirm: 
Make: 
Model: 





Confirm acceptance: 



Confirm agreement: 
	
	

	2) Weight:

The tractor must have an un-laden weight not less than 7,700Kg  

In addition, the vehicle must be capable of being fitted with front or rear ballast (wheel mounted) or a combination to achieve a max permissible weight of not less than 13,000kg to manufacturers specification.  Water in tyres shall not be permitted as a means of achieving this weight.
	


State Specification & Confirm: 





Confirm: 
	
	

	3) Engine:

4 stroke Common Rail Diesel 6 Cylinder

The engine must develop a minimum of 132 kW (180 HP-ISO TR14396) at a rated speed of 2100 - 2300 RPM and a corresponding minimum torque of 840 Nm at an engine speed of 1500 RPM.  

The engine must comply with Stage V emission regulations. The engine must be fitted with a “power boost” function with a minimum additional 25HP available for road transport and PTO applications. 

Incl Emergency Stop on both mudguards.

	

State Specification & Confirm: 




State Specification & Confirm: 




State Specification & Confirm: 
 


State Specification & Confirm
	
	

	4) Fuel Tank:

The fuel tank must have a capacity not less than 300 litres.

	

State Specification & Confirm: 

	



	



	5) Transmission:

The tractor must be fitted with a full power-shift transmission with hydraulic forward / reverse shuttle (with aggressiveness setting) and be capable of providing a speed of ≥ 50 km/hr.

Transmission functionality must be controlled from one multi-function lever, which also includes the ability to operate the three-point linkage / forward reserve shuttle operation.


Electro hydraulically operated front and rear axle differential lock must be fitted.

Minimum 18 x forward and 6 x reverse gears. 

Creeper Gears are required capable of achieving a low speed of 0.33kph.
	




State Specification & Confirm: 



Confirm: 



Confirm: 

State Specification & Confirm: 


State Specification & Confirm: 



	

	

	

	
	
	

	6) P.T.O.:

The tractor shall have 3 speed PTO capable of being engaged / switched from the driver’s cab with 540/540economy and 1000 rpm settings.

Fender/remote mounted PTO controls to aid the attachment of rear-mounted implements. Incl Emergency Engine Stop on both mudguards.

	



Confirm: 



Confirm: 

	
	

	7) Rear Linkage:

The tractor must be fitted with electro hydraulically operated Cat 2/3 3-point linkage with position / draft / mix and float functionality.

Fender / remote mounted lift controls to aid the attachment of rear mounted implements.

A rear lift capacity of ≥ 5,000kg is required (measured at ball ends). Min drawbar pull of 5,000kg at 10kph is required. 

	



State Specification & Confirm: 


Confirm: 


State Specification & Confirm: 

	
	

	8) Steering / Turning & Wheelbase/Wheel Track:

Power assisted steering is required. The tractor should also have a maximum turning circle / radius of 6.1m.

Wheelbase must measure ≥ 2.800 metres 

The wheel track width as measured from centreline of tyres must be supplied to measure 2.0m.
	


State Specification & Confirm: 

State Specification & Confirm: 


Confirm:
	

	

	
	
	
	

	9) Hydraulics: 

The tractor must be fitted with a “load-sensing” hydraulic system with a minimum displacement of 120 litres per minute @ 190 bar.

As standard, the tractor must be fitted with 4 mechanically operated, flow adjustable double acting remote hydraulic valves / connections for operating rear mounted equipment.

Provision for hydraulically operated trailer brakes. 

“Free Flow” low pressure return circuit.
	



State Specification & Confirm: 



Confirm: 

Confirm: 

Confirm: 

	

	

	10) Brakes:

As standard, the tractor must be fitted with wet disc brakes with separate front axle braking or a similar robust braking system suitable for the model of tractor.

Two-line pneumatic (air hydraulics) braking system with connections for trailed implements must also be fitted.

	



State Specification & Confirm: 


Confirm: 

	
	

	11) Wheels & Tyres:

The vehicle must be fitted with a minimum wheel size of R38 rear and R28 front (600/65 R38 rear and 540/65 R28 front or similar). The tyres fitted will be low-profile tyres capable of enabling the tractor to operate safely and efficiently both “on” and “off” road at both the required maximum speed and also when carrying the maximum requested trailer payload.

Rear wheels must be fitted with ballast weights to wheel centres of ≥200Kgs per side (≥400Kgs in total).

	








State Specification & Confirm: 


State Specification & Confirm: 

	
	

	12) Cab:

An ergonomic high visibility factory fitted glazed cab complete with high visibility roof window, heater & air conditioning, wipers (front and rear) and sunblind must be fitted.

Internal rear-view mirror, electrically adjustable and heated shatterproof external rear-view mirrors with integrated wide-angle functionality will attract additional marks.

Fitted with a rear mounted reverse / safety camera will attract additional marks.

Radio with mp3 and Bluetooth connectivity. 

The Cab must also have a four point Pneumatic or Mechanical suspension system. 

The maximum noise level in the cab will be no greater than 70dB(A). 

The Cab will have ROPS (rollover protection system) and FOPS (falling object protection) to OECD Code 10 Level 1 for roof window. 

An air-sprung driver’s seat must be fitted complete with seatbelt.

A passenger seat complete with seatbelt must also be fitted.

Twin rotating LED beacons must be fitted to the exterior of the cab.

Fire extinguisher with fitted bracket.

Front mounted camera for viewing linkage will attract additional marks.

Connection at rear of cab for ISObus and implement mounted camera will attract additional marks.

	




State Cabs Specification & Confirm: 



Confirm: 


Confirm:

Confirm: 


Confirm: 


Confirm: 



Confirm: 


Confirm: 

Confirm: 

Confirm: 


Confirm: 


Confirm: 



Confirm: 

	
	

	13) Reversing Aids:

The Tractor must be fitted with a reversing beeper, which will sound when reverse gear is engaged will attract additional marks.

The tractor must be fitted with a reverse/safety camera to aid with the attaching of rear-mounted implements will attract additional marks. 





	


State Specification & Confirm: 





State Specification & Confirm: 


	
	

	14) Lighting:

Full road lighting must be fitted, to comply with current regulations.

The tractor will have at least four forward facing and four rear facing LED work lights mounted the Cab.



Auxiliary high mounted headlights for use with front loader. 

	


State Specification & Confirm: 


State Specification & Confirm: 



State Specification & Confirm: 



	
	

	15) Hitch:

An automatic telescopic pick-up hitch must be fitted as standard.

Standard “clevis” and “hook” type hitch coupling must be supplied separately.

Hydraulic Top-Link.

	

Confirm: 



Confirm: 

Confirm:
	

	

	
	
	
	

	
	
	
	

	16) Delivery:

Delivery to Killybegs Fishery Harbour Centre Workshop.
Tenderers must confirm the 30 Calander day delivery time on the Pricing Schedule. Extra marks allocated for a speedier delivery.
	

Confirm: 


Confirm: 
State delivery in days after award:
	







	

	
	
	
	

	17) Finish:

The tractor must have a durable painted finish.
	

Confirm:
	




	

	18) Compliance:

The tractor must comply with all National and EU Regulations and Legislation pertaining to its Construction and its use both on and off Public roads.

	



Confirm: 
	


	

	19) Vehicle Registration:

The tractor must be registered for use on the public road and fitted with normal equipment to comply with the Irish Road Traffic Legislation.

	



Confirm: 
	
	

	20) Mudguards:

The Tractor will have mudguards fitted to front (pivoting) and rear wheels.

Mudguards must cover the entire width of front and rear wheels.

Fender mounted emergency stop buttons for tractor engine if fitted to both mudguards will attract additional marks.

	

Confirm: 



Confirm:


Confirm:
	

	

	21) Rear Axle:
Adjustable track width bar type.



	
Confirm:
	
	

	22) Front Axle:

The front axle must be fitted with a hydro-pneumatic / pneumatic suspension system.

	


Confirm:
	
	

	23) Fuel:

The tractor must be capable of running on low sulphur diesel.

The tractor must be capable of running on B7 biodiesel.




	

State Specification & Confirm: 


State Specification & Confirm: 
 

	
	

	24) Literature:

The following literature must be supplied in both manual and electronic (printable) form:-
• Operators Manual
• Spare Parts List
• Workshop/Repair Manual.
	



Confirm: 
Confirm: 
Confirm: 

	

	

	25) Training:

Comprehensive operator training must be provided by a dedicated operator trainer and must be provided on the Tractor at Killybegs Harbour or an agreed location. 

The session should cover in-depth training focusing on fuel efficient driving and safety related vehicle systems – the session content to be recorded in writing and signed by the person giving the session and passed on to the DAFM with the signed attendance sheet. At least 2 no training sessions shall be provided.

	



Confirm: 






Confirm: 
	
	

	26)   Supplier After Sales Service with Warranty and Service/Maintenance Package:
Ref Section 2, Appendix 1 Requirements and Specifications. A fully inclusive five (5) year warranty together with a five (5) year Service/Maintenance Package (or 6000 hours - whichever occurs first), will be required with this vehicle commencing on the day of delivery of the vehicle to Killybegs Fishery Harbour Centre. The vehicle supplied under this contract must be reliable in use and have reasonable servicing, maintenance and inspection requirements for their period in the client fleet.
Where an individual vehicle requires additional time out of service due to a high incidence of mechanical or body defects, this will be brought to the attention of the Supplier who will arrange an appropriate detailed inspection and full rectification of all faults with the vehicle.
In the event of persistent failures within the first 24 months from delivery of that vehicle, the client reserves the right to reject it and receive in its place a suitable replacement vehicle of similar type and specification, and of similar age and distance travelled.
The Supplier will be responsible to the client for ensuring that all appointed dealers work to the highest standards of technical expertise for all maintenance and repair work carried out to the vehicle delivered under this contract.
All work undertaken at an appointed dealer will not be charged under the Warranty and Maintenance Package. 
Similarly, the Supplier will be responsible for the suitability, availability, quality and warranty of all service items and replacement parts fitted to the vehicle by an appointed dealer.
The fully inclusive Annual Warranty and Maintenance Package will be paid annually at the rates in the tender at the end of each annual period and invoiced by the supplier. 

This shall be a fixed sum and shall not be altered for inflation or other price or cost increases. The Warranty and Maintenance Package will be transferable only to Successor Government Departments to the Department of Agriculture, Food and the Marine should this arise during the lifetime of the Warranty and Maintenance Packages. 
(Note Marks for exceeding minimum stated in Section 2 and here.)
	Give details.






Confirm:



Confirm:


Confirm:


Confirm:

Confirm:

Confirm:


Confirm:




Confirm:
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