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Appendix 1.4   Contractor Competency Matrix and Tender Returns
Tenderers shall complete this matrix and return it with the tender. Evidence of competency held, in-house or through a named subcontractor, is required at tender stage. Where a platform is to be obtained after award, the tender shall include the training booking or plan, and the certificates shall be provided within 8 weeks of award.
For every platform listed in Part 2, competency shall be held in-house, held through a named subcontractor, or committed to be obtained within 8 weeks of award. A platform marked ‘Not held’ makes the tender non-compliant for that platform.
1.4.1   Part 1: Company registrations
	Requirement
	Held (Yes / No)
	Evidence reference

	Safe Electric Registered Electrical Contractor (mandatory for the Contractor or a named subcontractor carrying out electrical work in Parts A and B)
	
	

	Health and safety management certification: ISO 45001, Safe-T-Cert or equivalent
	
	

	Quality management certification: ISO 9001 or equivalent
	
	

	Current safety statement
	
	

	Third-party certification for fire detection and alarm maintenance. Not required at tender. To be held within 12 months of award of contract, or 6 months from accreditation becoming available, whichever is later
	
	


1.4.2   Part 2: Engineer competency by platform
For each platform, enter the names of the engineers and attach their training certificates, showing the issuing body, date and expiry date. Manufacturer training shall be issued by the manufacturer or its approved training body.
	System / platform
	In-house (engineer names)
	Named subcontractor
	Obtain within 8 weeks
	Not held

	Fire detection and alarm (competent person to I.S. 3218)

	Advanced
	
	
	
	

	Morley
	
	
	
	

	C-Tec
	
	
	
	

	Johnson Controls FireClass
	
	
	
	

	Protec
	
	
	
	

	Automatic opening vents

	Colt
	
	
	
	

	WindowMaster
	
	
	
	

	Crossflow
	
	
	
	

	Disabled refuge / EVC

	Sigtel
	
	
	
	

	Baldwin Boxall
	
	
	
	

	Lexicom
	
	
	
	

	Discipline competency

	Emergency lighting (I.S. 3217)
	
	
	
	

	Portable extinguishers (I.S. 291)
	
	
	
	

	Sprinkler systems (I.S. EN 12845, BS 9251)
	
	
	
	

	Fire pumps, diesel and electric
	
	
	
	

	Dry risers and fire hydrants (I.S. 391)
	
	
	
	

	Standby generators
	
	
	
	

	Gas detection (manufacturer calibration)
	
	
	
	

	Alarms within dwellings, including CO
	
	
	
	

	Electrical installation (Safe Electric REC)
	
	
	
	



Where asset verification identifies a platform not listed above, the Contractor shall provide evidence of competency on that platform within 8 weeks, or propose a named subcontractor for Tuath’s approval.
1.4.3   Part 3: Tender returns
Tenderers shall return the following with the tender, in addition to the returns required by the RFT.
	Item
	Included (Yes / No)
	Reference

	Proof of current Safe Electric registration
	
	

	Manufacturer training certificates for every platform claimed in Part 2, showing the issuing body, the date and the expiry date where one applies
	
	

	Sample service report, sample inspection report and sample certificate, for all systems
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