Specification Planer Thicknesser

Ready Electronic Control
Simultaneous lifting and locking of surface tables with a mechanical safety device
Speedy setting up for changeover from surfacing to thicknessing.

Rubber-coated outfeed roller
Interchangeable feed rollers
Infeed sectional pressers

Capacity 520 x 250mm
Min working thickness 3mm
Total Length of Surfacing tables 2310mm

Xylent Spiral cutterblock
4 Feed Speeds 5/8/12/18 m/min
Auto star-delta start of 9kw motor
[bookmark: _GoBack]
Thicknessing table with 2 idle rollers
1st Roller sectional steel

Additional overturning fence for processing thin pieces
Working width -520mm

Cutterblock diameter/standard knives 120/4 mm/n
Total length of surface work tables -2310mm

Min. ÷ max. working height on thicknesser - 3,5 ÷ 250 mm

Three-phase motors starting from kW/Hz 9 (11) / 50 (60)

Planer table dimensions mm / inches 300 x 585 / 12 x 22
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