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Safety, Health, and Welfare at Work (Construction) 
Regulations 2013 
 
Preliminary Safety and Health Plan 
 
1 INTRODUCTION 
 
The Preliminary Safety and Health Plan has been prepared in accordance with the Safety Health, and Welfare at Work (Construction) Regulations 2013 by the Project Supervisor Design Process (PS-DP). It is being made available to the Project Supervisor for the Construction Stage (PS-CS) who will incorporate it and develop it as required into the final Health and Safety Plan.  
 
2 PROJECT SUPERVISOR FOR DESIGN STAGE 
 
2.1 Appointment 
 
The Client has appointed Tom O’Loughlin as Project Supervisor for the Design Stage of the Project to carry out the duties set out in the Regulations. 
 
2.2 Preliminary Health and Safety Plan 
 
In accordance with the Regulations, a Safety and Health Plan in a preliminary form as defined in the regulations, has been prepared for the purpose of providing information to the Project Supervisor for Construction Stage.  A copy of the said Plan is attached. 
 
3 APPOINTMENT OF PROJECT SUPERVISOR FOR CONSTRUCTION STAGE 
 
It is the intention of the Client that the Contractor appointed to carry out the works will undertake the duties of Project Supervisor for Construction Stage of the project as set out in the Regulations.  
 
4 CONTRACTOR TO CHECK ALL MATTERS 
 
The Contractor is to examine the site and the information supplied regarding the nature and extent of the proposed work so as to be satisfied as to what is required to be done to fulfil the duties of Project Supervisor for Construction stage and also what measures are required to be taken to meet the requirements of the Regulations in the execution of works including compliance with the Safety and Health Plan. All costs arising in respect of these matters are to be separately identified. The Client will not be liable for any such costs which are reasonably foreseeable and which are not so included. 
 
5 DESIGN BY CONTRACTORS 
 
It should be noted that where the Contractor or any Sub-Contractor carries out any design (as defined in the Regulations) the duties set out in Article 5 apply. 
 
 
6 GENERAL PROJECT DETAILS 
 
The Irish Cattle Breeding Federation (ICBF) intend to modify an existing cattle housing unit by raising the roof and ridge height of a central section, installing two new slatted tanks, and construct a lean-to shed over the cattle handling unit.  
 
The ICBF use the research farm at Tully (R51HN92) to capture expensive and hard to record features of interest on cattle that are progeny of artificial insemination sires of interest to the national breeding programme. 
 
The Contractor shall hold a copy of this document on site during the course of the contract. The content of this Preliminary Health and Safety Plan is as follows: 
 
· Description of the Project 
· Timescale for the Project 
· A list of those works which would involve the particular risks referred to in the Second Schedule of the Regulations 
· A list of specific measures for reducing particular risks 
· Additional information 
· Requirements for continuing liaison 
· Documents to be read in conjunction with the Preliminary Health and Safety Plan 
 
6.1 Contract Title 
 
The scheme shall be known as: Modifications to Existing Building and New Cattle Crush Lean-To at ICBF Beef and Dairy Research Centre 
 
6.2 Client  
Irish Cattle Breeding Federation Society Ltd

6.3 Project Supervisor for the Design Process 
 
The Project Supervisor for the Design Process is: 
 
Tom O’Loughlin 
 
6.4 Scope of Works 
 
The works consist of the following: 
 
The works will include: 
 
All construction works associated with the modification of existed cattle housing unit, construction of slatted tanks, and construction of cattle handling unit lean-to. The building will be a steel portal framed structure and all building elements shall be in accordance with Dept of Agricultural specifications. There will also be a requirement for existing drainage and structural tie ins.
 
6.5 Time for Completion 
 
It is the intention of the Project Supervisor for the Design Stage to allow adequate time for the Contractor to mobilise and carry out the work in a safe manner. The PS-DP has also allowed adequate time for the development of the Health and Safety Plan for the construction stage. 
 
· The timescale for construction of the works shall allow for the following: - 
i. Mobilisation / Site Storage. 
ii. Site Establishment 
iii. Location and protection of existing services. 
iv. Construction works. 
v. Undertaking all liaisons. 
vi. Complying with current Safety, Health and Welfare legislation.  
vii. Temporary Works 
 
· Commence Works 	September 2026 
· Complete all Works  	December 2026
 
· The Project Supervisor Construction Stage is required to assess whether the intended programme and initial dates stated are achievable in view of the safety and health issues. 
 
· If the scope of the works is changed then the adequacy or otherwise of the time for completing the works should be reviewed by the Client, and Project Supervisor Design Process in consultation with the Project Supervisor Construction Stage.   
 
6.6 Site Restrictions 
 
The site is located at ICBF Beef and Dairy Research Centre, Tully, Kildare, Co. Kildare R51HN92   
 
Access for the fire service and client activities shall be available at all times. The Contractor is responsible or securing the site and all works and storage should be with the enclosure. The Contractor must give advance notice to ICBF farm staff of all delivers to site. 

6.7 Other Activities on Site 
 	 
The Contractor shall plan and execute the work in a manner that will not cause any disruption to the Employers activities.  
 
6.8 Relevant Adjacent Land Uses 
 
All adjoining land is used for farming. 
 
6.9 Restrictions on Access 
 
Access is from the adjacent public road. Signage for deliveries to be provided by the Contractor. 
 
6.10 Restriction on Working Hours 
 
The works shall be confined to the hours 08.00 – 18.00 Monday to Saturday. 
 
6.11 Requirements for Notification by Client and PSCS 
 
The size and timescale for construction of the project is such that notification in writing must be sent to the Health & Safety Authority before work begins on site on prescribe form AF2 by the Project Supervisor Construction Stage in accordance with the Regulations.  
 
The size and timescale for construction of the project is such that notification in writing must be sent to the Health & Safety Authority before work begins on site on prescribe form AF1 by the client in accordance with the Regulations.  
 
7 WORK INVOLVING PARTICULAR RISKS 
 
This section of the Preliminary Safety & Health Plan is prepared to highlight work involving particular risks to the Safety and Health of persons at work. This list has been prepared in accordance with the Safety, Health & Welfare at Work (Construction) Regulations and represents a non-exhaustive list of particular risks. It should be noted that many of the risks on the project may arise out of working methods, which are at the discretion of the Contractor and as such cannot be determined by the Project Supervisor for the design Stage. 
 
The schedule of particular risks outlined below includes items of work involving particular risk to the Safety and Health of persons at work. 
 
7.1 Works which put persons at work at risk of – burial under earthfalls, engulfment in swampland or falling from a height, where the risk is particularly aggravated by the nature of the work or processes used or by the environment at the place of work on site: 
 
· Working at height during demolition of steel fame, cladding and electrical fittings and fixtures. 

· Working at height during erection of steel fame, cladding and electrical fittings and fixtures. 
 
· Deep excavations for building foundations, slatted tanks,  and laying of ducting for services. 
 
Affects 
 
· Site workers 
 
Principles of Prevention at design stage 
· Requirements for the contractor to provide adequate fall protection  
 
Potential Alleviation Measures 
· Adequate fall protection to be installed by the contractor 
· Experienced personnel to be used for all works. 
· Toolbox talks to highlight risks. 
· Excavations to have a safe angle of repose. 
· Method Statement and Risk Assessments to be developed for all works at a height.  
· Suitable working platforms to be employed and Safety harnesses to be used. 
 
7.2 Work which puts persons at risk from chemical or biological substances constituting a particular danger to the safety and health of such persons or involving a legal requirement for health monitoring.  
· Working on existing drains for tie into existing services.  
 
Affects: 
· Site workers. 
 
Principles of Prevention at design stage:  
 	N/A 
 
Potential Alleviation Measures: 
· Experienced personnel to be used.
·  Adequate PPE to be worn at all times.  
· Method Statement to be developed for all work on services.
· Toolbox talks to highlight risks. 
 
 
7.3 Work with ionizing radiation requiring the designation of controlled or supervised areas as defined in Directive 96/29/Euratom. 
No particular risks envisaged.  
 
 
7.4 Work near live electrical cables 
· Live services within the farm 
 
Affects 
· Site Workers 
 
Principal of Prevention at Design Stage 
· Details of know existing services identified prior to site mobilisation 

Potential Alleviation Measures 
· Provision of warning signs. 
· CAT scan to be carried out before works commence. 
· Method Statement and Risk Assessment to be prepared 
· Use of appropriate PPE. 
· Toolbox talks to highlight risk. 
· Contractor to comply with ESB procedures.  
· Contractor to locate all existing services. 
· Live Services to be isolated where possible.  
· Goal posts where construction vehicles/machinery passing under over-head cables. 
  
 
 
7.5 Work Exposing Persons to Risk of Drowning 
No significant risk identified.  
 
7.6 Work on wells, underground earthworks and tunnels.  
No risks identified.  
 
7.7 Work carried out by divers at work 
No risk identified.  
 
7.8 Work carried out in a caisson with a compressed air atmosphere 
No particular risks envisaged.  
 
7.9 Work involving the use of explosives 
Explosives will not be used in the works. No risks are identified.  
 
7.10 Work involving the assembly or disassembly of heavy prefabricated components 
· Disassembly of existing roof structure
· Erection of steelwork, building services etc. 
 
Affects 
· Site Workers 
· ICBF Farm Personnel 
 
Principles of Prevention at Design Stage 
· Details of all items to be dissembled provided in the tender documents 
· Details of all items to be erected provided in the tender documents 
 
Potential Alleviation Measures 
· Suitable equipment e.g. MEWP’s and cranes to be used.  
· Experienced personnel to be used.  
· Toolbox talks to be held to highlight the risks 
· Method Statements and Risk Assessments to be developed.  
· Safety nets to be used where possible.  
· Safety harnesses and other PPE to be used.  
· Temporary bracing to be used if necessary to maintain building stability. 
 
 
 
8 SITE SPECIFIC RISKS 
 
8.1 Working Within ICBF Beef and Dairy Research Centre, Tully
· The works will involve working adjacent to ICBF Tully Farm activities. There are also risks due to vehicular movements associated with deliveries, farming activities and vehicular movements through the main entrance and throughout the campus.  
 
Affects: 
· Site workers  
· ICBF Tully Farm personnel 
 
Principles of Prevention at design stage: 
· Details of required works provided in the tender documents.  
· Temporary hoarding or fencing required to separate the site from ICBF Tully Farm activities. Access to the construction site by ICBF Tully Farm staff not required during period of works.
 
Potential Alleviation Measures 
· Control access to the site.  
· Toolbox talks to highlight risk.  
· Method Statement and Risk Assessments to be developed.  
· PPE to be worn.  
· Provision of warning signs.  
 
 
8.2 Working on or Adjacent to Electrical Services 
 
The works will be constructed adjacent to existing high, medium and low voltage electrical cables. 
 
Affects 
· Site workers 
 
Principles of Prevention at Design Stage 
· Details of required works included in Tender Pack 
 
Potential Alleviation Measures 
 
· Locate the cables by CAT scan and hand excavation 
· Use of PPE 
· Selection of appropriate plant and equipment for the construction works. 
· Experienced personnel to be employed.  
· Method Statement and Risk Assessments to be developed.  
· Toolbox talks to be held to highlight the risks.  
· Warning signs to be erected.  
 
 
 
9 SPECIFIC MEASURES FOR REDUCING PARTICULAR RISKS 
 
It is envisaged at the Design Stage that most of the particular risks will be reduced by careful planning by the Contractor prior to work commencing. In particular the need to programme the works carefully so that work activities are not being carried out close to potential hazards and prepare and work in accordance with method statements for the major risk items. 
 
In addition, the following non-exhaustive list of specific measures for reducing particular risks will need to be addressed in the Construction Stage Safety and Health Plan: 
 
· All personnel will be required to have a safe pass.  
· All personnel of whatever function must wear an approved yellow high visibility vest / jacket. 
· Appropriate personal protective equipment shall be worn at all times to mitigate risks of personal injury. 
· Measures will be required for the safe operations of plant and other construction activities where these are in the vicinity of any utilities, boundaries, access routes etc.  
· The use of machinery shall be planned by the Contractor so that sufficient clearance both laterally and vertically shall be ensured for vehicles and machinery, so as not to trap or crush persons or cause damage. 
· Measures will be put in place to reduce risk from scaffolding, working adjacent to traffic routes and working adjacent to live areas.   
· Suitable firefighting and first aid equipment shall be provided and maintained on the site. All possible precautions shall be taken to provide for the safe storage if necessary, of petroleum, gas bottles and other potentially dangerous goods.  
· Measures will be required for the safe operation of lifting appliances  
· Measures will be required for the safe use of skips 
· Measures shall be taken to minimise risks arising from dust and noise that occur as a result of the works. 
· Provision of adequate ear protection when working with or near machinery   
· Provide protective clothing for working with hazardous materials e.g., when pouring concrete, working on drains etc.   
· Securing of the site against unauthorised access. Site fencing shall be erected around the main site/work areas. Heras fencing or similar will generally be acceptable  
· Labelling of dangerous chemical substances and other substances and provision of appropriate protective masks and clothing. Providing secure storage facilities for hazardous materials 
· Measures must be taken to prevent the discharge of pollutants, oils, fuels, chemical and uncured cementitious products into drains. 
 
Procedures will be implemented to ensure that all specialist construction activities are planned and executed by suitably qualified and experienced personnel. 

10 	ADDITIONAL INFORMATION 
 
The PS-CS is to be aware of the following: 
· Safe access to the site shall be provided for personnel, plant and equipment. 
· Safe access shall be provided for emergency vehicles, and the emergency services informed of restrictions at all times. 
· Safe storage of materials to be provided by the Contractor. 
· Safe access to all parts of the site shall be provided and maintained.  
· The Contractor should give careful consideration to suitable construction methods to suit the site environment. 
· The works need to be carefully programmed to meet the requirements to maintain safe traffic flow at all times throughout the contract and to minimise risks to safety and health.  
 
 
11 	REQUIREMENTS FOR CONTINUING LIAISON 
 
Procedures will be required for liaison between the PSCS, the Contractor, the Designer and ICBF to consider the following: 
 
1) Safety and Health implications of the design of the works 
2) Unforeseen events during the works resulting in substantial design changes that might affect particular risks, contract timescale and have safety and health implications. 
 
12 	DOCUMENTS TO BE READ AND OBSERVED IN CONJUNCTION WITH THE PRELIMINARY HEALTH AND SAFETY PLAN 
 
· 2013 Safety, Health & Welfare at Work (Construction) Regulations 
· Requirements provided by ICBF when tendering the works 

13 	SAFETY FILE 
 
Pursuant to 'Duties of Project Supervisor for the Design Process, Safety File’ of the Safety and Health at Work Regulations, the Project Supervisor Design Process is required to; 
· Prepare a safety file appropriate to the characteristics of the project, containing relevant safety and health information, including any information provided under the Regulations, to be considered during any subsequent construction work following completion of the project, and 
· Promptly deliver the safety file to the client on completion of the project. 
  
The following is a non-exhaustive list of contents which the Project Supervisor Construction Stage (PSCS) may be required to supply to the PSDP for inclusion in the safety file. It is not intended to be a complete list and in no way relieves the PSCS of his obligations under the regulations. 
· Health and Safety Plan prepared by PSCS; 
· Details of Subcontractors and other Contractors on Site; 
· Insurance Details of all Contractors on Site; 
· Main Contractors Safety Statement / Policy; 
· As Built Drawings; 
· Copy of Method Statements; 
· Statements of General Design Criteria; 
· Details of Equipment and Maintenance Facilities; 
· Maintenance Procedures and Manuals; 
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Appendix 1 
 
Risk Assessments 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 





 
INTRODUCTION 
In the following design risk assessments, the risks are assessed on the basis of likelihood and severity in order to generate a risk rating as follows. 
 
	Likelihood 
	0 
	No Risk 

	 
	1 
	Highly Unlikely 

	 
	2 
	Remote 
	

	 
	3 
	Possible 
	

	 
	4 
	Probable 
	

	 
	5 
	Highly likely 
	

	Severity 
	1 
	Negligible 
	

	 
	2 
	Minor Injury 
	

	 
	3 
	Major Injury 
	

	 
	4 
	Severe Injury 
	

	 
	5 
	Fatalities 
	

	Risk Rating 
	1-4 
	Low Risk  
	- Communicate 

	 
	5-14 
	Medium Risk 
	- Reduce 

	 
	 
	 
	 - Communicate 

	 
	15-25 
	High Risk  
	 - Eliminate from design and / or construction 

	 
	 
	 
	- Reduce 

	 
	 
	 
	- Communicate 



Persons Exposed 
	Contractor: 
 
	Includes employees of the contractor and any sub-contractor engaged by the Client for the construction or maintenance of the Project 

	End-User: 
	Includes the Client, their employees and the facilities operator 

	Maintenance: 
	Includes persons undertaking maintenance activities during the operation of the facility 

	Public: 
	Includes any member of the public or visitor who could be exposed to hazards during the construction use or maintenance of the facility.

	Client 
	Irish Cattle Breeding Federation Society Ltd. 

	PSDP 
	Tom O’Loughlin 
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	No Control Measures 
	
	Control Measures Applied 

	Item No. 
	Identified Hazards 
	Associated Risks 
	Population 
 Exposed 
	Risk 
	
	Control Measures 
	Person 
Responsible for Action 
	Residual  
Risk 

	 
	 
	 
	 
	Contractor 
	Likelihood of 
Occurrence
 

	Consequence of 
Occurrence
 

	Risk Rating 

	 
	 

	  
Risk 
 Rating 

	
	
	
	 
	End User 
	
	
	
	
	
	

	
	
	
	 
	Maintenance  
	
	
	
	
	
	

	
	
	
	 
	Public  
	
	
	
	
	
	

	1. 
	Earthworks 
	Excavation 	collapse, 	fall from heights 
	 
	Contractor 
	4 
	5 
	20 
	Details of structures provided in the tender documents 
	 
	10 

	
	
	
	
	
	
	
	
	Safe angle of repose on excavations  
 
Excavations to be railed off 
 
	Contractor 
 
Contractor 
	

	
	
	
	
	
	
	
	
	Tender documents require the Contractor to submit Method Statements and Risk Assessments 
	Contractor 
	

	2. 
	Working close to electrical cables 
	Exposure 	to 	electrical cables. 
	 
	Contractor 
	4 
	5 
	20 
	Tender documents require the Contractor to submit Method Statements and Risk Assessments 
	Contractor 
	10 

	3. 
	Erection of scaffolding, structural steel, roofing, walls, services, including, 
doors, finishes
	Risk of falling from a height 
	 
	Contractor 
	4 
	5 
	20 
	Contractor to submit method statement and Risk Assessment to the PSDP for approval.  
 
 
 
 

	Contractor 
	10 


 
 
	 
	 
	No Control Measures 
	
	Control Measures Applied 
	
	

	Item No. 
	Identified Hazards 
	Associated Risks 
	Population 
 Exposed 
	Risk 
	Control Measures 
	Person 
Responsible for Action 
	Residual  
Risk 

	4. 
	Building Works Generally 
	Risk of objects falling, risk of scaffolding collapse, risk of shutter collapse 
	 
	Contractor 
	3 
	15 
	15 
	Experienced personnel to carry out the Work. Suitable equipment to be used.  
Method Statements 	and Risk Assessments to be developed.  
Risk to be highlighted at toolbox talks, by erecting warning signs etc.  
PPE to be worn.  
	Contractor 
	10 

	5. 
	Existing and proposed services 
	Risk of injury from contact with existing electrical services 
	 
	Contractor 
	3 
	5 
	15 
	Experienced personnel to carry out the Work. Suitable equipment to be used.  
Method Statements 	and Risk 
Assessments to be developed.  
Risk to be highlighted at toolbox talks, by erecting warning signs etc.  
PPE to be worn.  
	Contractor 
	10 

	6. 
	Traffic  
	Risk of injury or death due to collision 
	 
	Contractor 
ICBF
Farm 
Personnel  
	4 
	5 
	20 
	Traffic 	Management Plan to be developed. 
Method Statements 	and Risk 
Assessments to be prepared.  
PPE to be worn 
Diversions to be provided 
Signs to be erected 
	Contractor 
	12 

	7
	Removal of existing structures
	Risk of structural collapse during demolition
Falling materials / debris

	 
	Contractor 
	3
	5
	20
	Use of experienced personnel only
Demolition to be carried out in a controlled sequence
Exclusion zones around demolition area
Signs to be erected
Certified lifting equipment and competent operators used
Method Statements 	and Risk Assessments to be developed.  
Risk to be highlighted at toolbox talks, by erecting warning signs etc.  
PPE to be worn.  
	Contractor
	10



	 
	 
	No Control Measures 
	Control Measures Applied 

	Item No. 
	Identified Hazards 
	Associated Risks 
	Population 
 Exposed 
	Risk 
	Control Measures 
	Person 
Responsible for Action 
	Residual  
Risk 

	8. 
	Concrete walls 
	Risk of collapse due to lack of support 
	 
	Contractor 
	4 
	5 
	20 
	Method Statement and Risk Assessment to be developed. Temporary props to be provided until permanent works are completed.  
	Contractor 
	12 

	9. 
	Working Close to other Activities 
	Risk of accidents 
	 
	Contractor 
ICBF
Farm 
Personnel  
	3 
	5 
	15 
	Toolbox talks to be held.  
Safety Meetings to plan daily activities.  
Experienced personnel  
Safety barriers to be provided.  
	Contractor 
	10 

	10. 
	Working at a height 
	Risk of Falling  
	 
	Contractor 
	3 
	5 
	15 
	Method Statement and Risk Assessment to be prepared.  
Safety Harness to be used.  Handrailing to be provided PPE to be worn. 
	Contractor 
	10 

	11. 
	Maintenance  
	Falling from a height 
	 
	ICBF
Staff, 
Maintenance crews 
	3 
	5 
	15 
	Method Statement and Risk Assessments to be developed.  
Experienced personnel to carry out the Works appropriate equipment.  
	Contractor 
	8 

	12. 
	Use of 
Construction 
Equipment 
	Accidents, crushing, falls, electrocution  
	 
	Contractor 
	4 
	5 
	20 
	Appropriate equipment to be used. All equipment to have valid certificates.  
Experienced personnel to be used.  
PPE to be worn 
Method Statements and Risk Assessments to be prepared.  
	Contractor  
	8 


 
	 
	 
	No Control Measures 
	Control Measures Applied 

	Item No. 
	Identified Hazards 
	Associated Risks 
	Population 
 Exposed 
	Risk 
	Control Measures 
	Person 
Responsible for Action 
	Residual  
Risk 

	13. 
	Electrical Work  
	Electrocution 
	 
 
	Contractor 
	3 
	5 
	15 
	Experienced personnel to be used with training as necessary.  
Use of chemicals to be controlled.  
PPE to be worn.  
Method Statements and Risk Assessments to be developed 
	Contractor 
	9 

	14 
	Temporary Works 
	Structural collapse during temporary works 
	 
	Contractor 
	4 
	5 
	20 
	Tender documents require the Contractor to submit Temporary Works Design, Method Statements and Risk Assessments 
PPE to be worn 
Experienced personnel to be used 
	Contractor 
	10 

	15. 
	Working adjacent to existing structures 
	Electrocution, burns etc Undermining, collapses 
	 
	Contractor 
	4 
	5 
	20 
	Tender documents require the Contractor to submit Temporary Works Design, Method Statements and Risk 
Assessments 
PPE to be worn 
Experienced personnel to be used 
	Contractor 
	10 

	16. 
	Loading, unloading, use of cranes, etc 
	Risk of collapse and materials falling 
	 
	Contractor 
	4 
	5 
	20 
	Tender documents require the Contractor to submit Temporary Works Design, Method Statements and Risk Assessments 
PPE to be worn 
	Contractor 
	10 
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& Safety, Health and Welfare at Work (Construction) Regulations 2013
Hi-'u\[LHI;\I?;]:;RH-u Approved Form (AF 2) Regulation 22

Particulars to be notified by Project Supervisor for the Construction Stage to
NG the Health and Safety Authority before the construction work begins

This form is to be used to notify the Health & Safety Authority of any project covered by the Safety, Health and Welfare at Work (Construction) Regulations
2013, which will last longer than 30 days or 500 person days. It can also be used to provide changes to initial notification of projects.

Any day on which construction work is carried out (including holidays and weekends) should be counted, even if the work on that day is of short duration. A
person day is one individual, including supervisors and specialists, carrying out construction work for one normal working shift.

This Notification is to be made by Registered Post to HSA, Metropolitan Building, James Joyce Street, Dublin 1; or as may be directed by the Authority.

The project supervisor for the construction stage shall clearly display on the construction site a copy of this form.

Client(s): Provide name, full address, telephone number and e-mail address for the Client. If more than one Client,
please attach details of all Clients on a separate sheet.

Name I

Address

Telephone I Email I

Project Supervisor Design Process and Health & Safety Coordinator: Provide name, full address, telephone
number and e-mail address for the PSDP and Health & Safety Coordinator for the PSDP, if appointed.

PSDP name I H&SC name I
Address Address

Telephone I Telephone |

Email I Email I

Project Supervisor Construction Stage and Health & Safety Coordinator: Provide name, full address,
telephone number and e-mail address for the PSCS and Health & Safety Coordinator for the PSCS, if appointed.

PSCS name | H&SC name |
Address Address

Telephone I Telephone I

Email I Email I

° Information on Construction Work: Please provide your details / estimates for the following.

Description of
project

Exact address
of site

The planned date for the commencement of the construction work |

How long the construction work is expected to take (in weeks) |

Estimated maximum number of workers on site at any one time |

Planned number of contractors and self-employed persons expected to work on site |

Details of Contractors Chosen: Provide name, full address & telephone number of those selected to work on this
project (if required continue on a separate sheet).

Name Address Telephone and email

Signed | by or on behalf of the PSCS

Position | Date
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Particulars to be notified by Project Supervisor for the Construction Stage to
NG the Health and Safety Authority before the construction work begins

This form is to be used to notify the Health & Safety Authority of any project covered by the Safety, Health and Welfare at Work (Construction) Regulations
2013, which will last longer than 30 days or 500 person days. It can also be used to provide changes to initial notification of projects.

Any day on which construction work is carried out (including holidays and weekends) should be counted, even if the work on that day is of short duration. A
person day is one individual, including supervisors and specialists, carrying out construction work for one normal working shift.

This Notification is to be made by Registered Post to HSA, Metropolitan Building, James Joyce Street, Dublin 1; or as may be directed by the Authority.

The project supervisor for the construction stage shall clearly display on the construction site a copy of this form.

Client(s): Provide name, full address, telephone number and e-mail address for the Client. If more than one Client,
please attach details of all Clients on a separate sheet.

Name I

Address

Telephone I Email I

Project Supervisor Design Process and Health & Safety Coordinator: Provide name, full address, telephone
number and e-mail address for the PSDP and Health & Safety Coordinator for the PSDP, if appointed.

PSDP name I H&SC name I
Address Address

Telephone I Telephone |

Email I Email I

Project Supervisor Construction Stage and Health & Safety Coordinator: Provide name, full address,
telephone number and e-mail address for the PSCS and Health & Safety Coordinator for the PSCS, if appointed.

PSCS name | H&SC name |
Address Address

Telephone I Telephone I

Email I Email I

° Information on Construction Work: Please provide your details / estimates for the following.

Description of
project

Exact address
of site

The planned date for the commencement of the construction work |

How long the construction work is expected to take (in weeks) |

Estimated maximum number of workers on site at any one time |

Planned number of contractors and self-employed persons expected to work on site |

Details of Contractors Chosen: Provide name, full address & telephone number of those selected to work on this
project (if required continue on a separate sheet).

Name Address Telephone and email

Signed | by or on behalf of the PSCS

Position | Date
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