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	Number
	Query/ Clarification
	Response

	1
	Can the contract authority confirm if it is willing to review the annual turnover of the procurement given the market contract value which is set. As it stands, we feel the values set will preclude the market response and the objective of most economically advantageous cannot be achieved as this requirement will eliminate SMEs from responding.
	The Contracting Authority requires - Evidence of a minimum turnover over of €300,000 per annum by way of Accountants/Auditors letter. 


The Contracting Authority will not review the annual turnover of the procurement as this is 1.5 times the value of the contract.

	2
	Core Switch
Downlink Ports, it’s stated that "Downlink Port Requirement - at least 24 ports supporting 40Gb/s SFP/SFP+/SFP28 ports (Matching the Edge Switch Uplinks)"
Will the Authority accept "QSFP28" ports operating at 40GbE for the required 24 × 40Gb/s core downlink interfaces?

	The Contracting Authority requires Core Switch
Downlink Port Requirement - at least 24 ports supporting 40Gb/s SFP/SFP+/SFP28 ports (Matching the Edge Switch Uplinks).

The Contracting Authority will not accept any configuration outside of this mandatory requirement. 

	3
	Edge Switches
Standard Port Requirement - Minimum 48 x 1/2.5/5/10Gb/s RJ45 ports
Is it mandatory to have 10G ethernet ports? or will you accept an edge switch with the following ports:
48 multigigabit RJ45 ports supporting 10M/100M/1G/2.5G/5G, 95W IEEE 802.3bt PoE, 256-bit MACsec, approximately 1.88 Tb/s aggregated switching capacity, virtual chassis capability up to eight members, redundant hot-swappable PSUs, redundant fans, 1U form factor, front-to-back airflow, out-of-band management, console and USB ports,

	The Contracting Authority requires Edge Switches
Standard Port Requirement - Minimum 48 x 1/2.5/5/10Gb/s RJ45 ports.

The Contracting Authority will not accept any configuration outside of this mandatory requirement. 
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