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AirNav Ireland was established as a commercial state-sponsored body on 1 May 2023 with the responsibility for the provision of Air Traffic services in Irish controlled airspace. 
AirNav Ireland provides air traffic control services for aircraft travelling through Irish airspace and those landing and taking off from Dublin, Cork and Shannon airports. AirNav Ireland’s Air Traffic Controllers at the North Atlantic Enroute Centre in Shannon safely handle over 90% of all aircraft that operate between North America and Europe. The AirNav Ireland North Atlantic Communications Centre in Ballygirreen, Co. Clare provides a long-range High Frequency Radio (HF) communications service for Oceanic Air Traffic Control in the eastern half of the north Atlantic. AirNav Ireland is regulated by the Irish Aviation Authority 
AirNav Ireland’s primary responsibility is promoting and maintaining safety in all matters relating to aviation activities under its remit. In this respect, AirNav Ireland complies with and is responsible for implementing and supervising the highest standards and procedures in aviation. These standards are agreed at an international level by legally established bodies, charged with the responsibility for regulating all aspects of commercial aviation. 
The Air Traffic Management (ATM) function is discharged by highly skilled professional personnel operating from modern purpose designed buildings utilising the most up to date technology available. References to “Irish Aviation Authority” on documentation issued before 1st May 2023 shall be deemed to reference “AirNav Ireland” accordingly. 
Further Information available at www.airnav.ie
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AirNav Ireland requires the supply of ergonomic Air Traffic Controller (ATC) chairs for use within operational control room across its sites. These chairs will be used by Air Traffic Controller in safety-critical environments that operate on a contains 24 hours a day, 7 days a week basis. 
The successful supplier is required to provide controller chairs that are specifically designed for intensive 24/7 operational use and that deliver a high standard of ergonomic support, durability, safety and use comfort. The chairs must be suitable for prolonged periods of seated operations while supporting the health, wellbeing and operational performance of Air Traffic Controllers.
Depended on the chair proposed, . Candidates will not be expected to deliver sample unit at the same time as their written responses to this Tender document, but should confirm their willingness to do so, as a potential follow-up evaluation step, if requested to do so by AirNAV.

(a) Candidates should confirm their willingness to deliver such evaluation equipment as may be requested by AirNAV within one week of receiving the request, to be delivered to the AirNAV HQ building in Dublin.


(b) Candidates should confirm that they agree that neither AirNAV nor its advisors will be liable in respect of any costs incurred by the Candidate in the preparation and submission of a proposal repsponding to this Tender, or any associated work effort, and specifically not in the provision, delivery, or recovery of any sample units requested by AirNAV.

(c) Candidates should confirm that they fully understand that a request for the supply of sample units is not an indication of intent to do business with that Candidate.

(d) Candidates should note that AirNAV commits to perform evaluation and testing of any supplied sample units in a fully impartial and genuinely unbiased manner. 

a. AirNAV would propose to use its Bid Evaluation team to evaluate the equipment, but also reserves the right to invite nominated members of the AirNAV management and user communities to present their comments and opinions.

b. No marks will be given in the scoring of this section of the Tender response to any Candidate’s bid until after any requested sample units have been delivered, and configured (where necessary) by the Candidate, and tested by AirNAV.

(e) Notwithstanding AirNAV’s commitment to Candidates of total impartiality (as per point (e) above), Candidates should confirm that they fully accept that the assessment that AirNAV proposes undertaking will, by its very nature, be somewhat subjective in nature ... and that they agree to abide by the scoring evaluation of the AirNAV team. If Candidates cannot accept this condition, they should:



Order Details
	Year
	Number of the Chairs
	Price
	Delivery

	1
	Up to 50 units
	
	

	2
	Up to 50 units
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


· The Tendered Price must include delivery to all AirNav locations, as required.
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The supplier shall supply controller chairs that meet the technical specifications and minimum standards set out below:

Standards
The controller chairs are required to comply with Irish, European and British standards applicable to ergonomic seating and fire safety.
As a minimum, the upholstery materials shall comply with the following standards:
•BS 7176: 2007 – Specification for resistance to ignition of upholstered furniture for non-domestic seating by testing composites.
•BS EN 1021: 2006 parts 1 & 2 – Assessment of the ignitability of upholstered furniture.
•BS 5852: 2006 – Fire resistance testing of upholstered seating.
The supplier shall provide documentary evidence demonstrating compliance with the above standards upon request.

Minimum Functional Requirements
Each controller chair shall include, as a minimum:
•Air lumbar adjustment or equivalent ergonomic pressure relief system
•Inflatable lumbar support pump 
•Ergonomic multi-adjustable 6-way headrest
•30° tilt Adjustable armrest
•27° tilt Adjustable backrest recline
•Adjustable backrest angle
•16° Adjustable seat tilt/ rocking mechanism
•Adjustable seat cushion height
•Adjustable seat cushion length
•Height (100mm height riser) and weight adjustment mechanism 
•Minimum user weight capacity of 200kg

Minimum Product Requirements
The controller chair shall, as a minimum:
•Be designed and certified for continuous 24/7 operational use.
•Be suitable for use within Air Traffic Control and other operational control room environments.
•Be fitted with castors suitable for control room flooring.
•Have a black fabric seat and backrest.
•Have a black leather upholstered armrests and headrest.
•Be manufactured using robust, high-quality materials suitable for continuous operational use.
•Be supplied fully assembled (or installed by the supplier if required).
Replacement parts and key components, including armrests, wheels and air pumps, must remain readily available for a minimum 4 years following delivery of the chairs to facilitate ongoing maintenance and replacement as required.
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