Appendix A	Compliance to Specification 
Inland Fisheries Ireland
LOT1 Thermal Imaging Equipment – Compliance to Specification

	Tenderer Organisation Name

	

	Equipment Proposed (Make/Model/Variant)

	



	[bookmark: _Hlk211249652][bookmark: _Hlk171599575]Tender Ref
	Specification/Requirement
	Compliant
Yes/No
	Notes (please provide any additional information in support of the equipment offered)
	IFI Use

	1

	Device should be robust and rubber armoured and it should be ergonomically designed
	
	
	

	2

	Thermal Sensor 640 x 480 or above
	
	
	

	3

	Warranty of three years or greater
	
	
	

	4

	Design Type must be monocular
	
	
	

	5
	NETD of <15mk 
	
	

	

	6

	Base magnification 2.5x
	
	
	

	7

	Detection range 1800m
	
	
	

	8

	Unit must not have a range finder
	
	
	

	9

	Wi-Fi with supporting App is required with the ability to connect to an Android device
	
	
	

	10

	Weight must be 800g or less
	
	
	

	11

	Multiple colour palettes
	
	
	

	12

	Device must a minimum of IPX7 rated
	
	
	

	13

	Detection range 1800m
	
	
	

	14

	Display is 1024 x 768 or above
	
	
	

	15

	Battery to last for a minimum of 6 hours or above
	
	
	

	16

	Frame rate of 50Hz
	
	
	




	Please state the maximum delivery lead time in days from award of contract.

	



	Signed:
	


	Position in company:
	

	Print Name:
	


	Date: 
	



