Appendix A	Compliance to Specification 
Inland Fisheries Ireland
LOT2 Spotting Scopes – Compliance to Specification

	Tenderer Organisation Name

	

	Equipment Proposed (Make/Model/Variant)

	



	[bookmark: _Hlk211249652][bookmark: _Hlk171599575]Tender Ref
	Specification/Requirement
	Compliant
Yes/No
	Notes (please provide any additional information in support of the equipment offered)
	IFI Use

	Key Elements

	1

	A minimum zoom range of 20x with a maximum range of 70x
	
	
	

	2

	Straight eyepiece
	
	
	

	3

	Effective lens diameter of at least 95mm – 115mm
	
	
	

	4

	The optics must be capable of long-range visibility and sharp image rendition across the entire field of view; bright high contrast images are essential especially in difficult weather and light conditions 
	
	
	

	5
	Light transmission of at least 86% - 88% is required 
	
	

	

	6

	A scratchproof/treated lens and protective eyepiece coating is required
	
	
	

	7

	There should be no difference in field of view between spectacle wearers and other users
	
	
	

	8

	Exterior body of scope must be of non-slip design for use in adverse weather conditions
	
	
	

	9

	A submersion capability of 4m is required as the scopes will be used in and around water. In addition, be waterproof to 400mbar of pressure and resistant to internal fogging
	
	
	

	10

	A ten year warranty is required.
	
	
	

	11

	The unit must be light weight and of rugged design. Size and transport dimensions are important factors.
	
	
	

	12

	The unit must be user friendly with quick and precise focus adjustment for positive target identification and monitoring.
	
	
	

	Accessories

	13

	Carrying, protective case must be practical for field operations and offer a degree of protection for the unit.
	
	
	

	14

	The legs of the tripod must be made of carbon and be capable of rapid adjustment and compact for ease of transport. The tripod head should allow for panning and tilting with ease.
	
	
	

	15

	Camera adaptor to enable attachment of cameras
	
	
	

	16

	Smart phone adaptor to enable photographs to be taken
	
	
	

	17
	Car window mount/clamp to enable scope to be used from a vehicle
	
	
	

	18
	Repair and maintenance of equipment and goods purchased through this framework agreement
	
	
	




	Please state the maximum delivery lead time in days from award of contract.

	



	Signed:
	


	Position in company:
	

	Print Name:
	


	Date: 
	



