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[bookmark: _Toc492028203]NOTES 
1. Supply prices to include delivery and offloading to site Ballydavid Co.Kerry. (Ireland).
2. All prices shall be in euro (€) and exclusive of any Value Added Tax (which may be added to invoices at the appropriate rate)
3. Any applicable import duty or taxes must be clearly shown in the tender.
4. The Tender Price shall be delivered duty paid (DDP) to site in Ireland and shall include payments necessary to comply with all acts, laws, rules, work permits, national insurance contributions, government stamp tax, taxes and regulations current at the time of tendering including, but not limited to those applicable in the Republic of Ireland and in the country of origin;
5. Tender prices are to be submitted as per the tables shown below.  Prices shall also be submitted to 2RN in electronic (Microsoft Excel spreadsheet soft copy) form.
6. The tenderer shall state all assumptions with the prices.
7. Any formula bids as to price shall be excluded from consideration.
8. Unit prices are requested for certain items, but all costs associated with the works should be included in the total price.



Prices shall be in accordance with the following breakdown.



1
BALLYDAVID CIVILS WORK & SUPPLY OF TOWER
	[bookmark: _Hlk509582933]
	Design, supply, construction of new Tower
	
	
	
	
	

	[bookmark: _Hlk498698322]No.
	Description
	Qty.
	Unit
	Unit Price (€)
	Total price (€)
	Assumptions

	1.1
	Clearing of site including temporary site security 
	1
	lot
	
	
	State any assumptions

	1.2
	Design and installation of tower base including reinforcement
	1
	lot
	
	
	State any assumptions

	1.3
	Design and installation of crane hard stand area
	1
	Lot
	
	
	State any assumptions

	1.4
	Design and installation of tower earthing system
	1
	lot
	
	
	State any assumptions

	1.5
	Design, supply and delivery of 54m tower including, anti-climb, ladder, rest platforms and antenna support poles. 
	1
	lot
	
	
	State any assumptions

	1.6
	Supply and delivery of antenna support poles. 
	1
	lot
	
	
	State any assumptions

	1.7
	Supply of fall arrest system (Latchway)
	1
	lot
	
	
	State any assumptions

	1.8
	Provision of as-built site layout drawing in AutoCAD format
	1
	no
	
	
	State any assumptions
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	Supervision, overheads, and certification
	1
	lot
	
	
	State any assumptions
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	Ballydavid Tower Tender Price
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	No.
	Description
	Qty.
	Unit
	Unit Price (€)
	

	5.0
	Unit prices 
	
	
	
	

	5.1
	Supply and installation of ESB ducting per metre
	1
	m
	
	

	5.2
	Supply and installation of signal ducting per metre
	1
	m
	
	

	5.3
	Supply and installation of manhole to ESB standards
	1
	m
	
	

	5.4
	Supply and installation of cable gantry per metre
	1
	m
	
	

	5.5
	Rate for rock breaking
	1
	m3
	
	

	5.6
	Rate for imported fill
	1
	m3
	
	

	5.7
	Upgrade of existing access track to meet specifications
	1
	m
	
	

	5.8
	Supply and installation of 40 N/mm2 concrete per metre cube
	1
	m3
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