New woodland planting – B 2 Oak woodland areas and B1 Birch woodland DZ Cleveragh Regional Park Biodiversity Project  

PRICING DOCUMENT- 


	Item 
	Description 
	Quantity


	Total
  €


	1
	Insurances
Health & Safety 
	Item
	

	2
	Project Managment & Supervision of works


	Item
	

	3
	 Project supervisor construction stage – all duties

	Item
	

	4
	Provision of all tools, plant and equipment required to complete the works in a safe manner

Including all safety fencing / signage,/other 
	Item
	

	5
	The planting sites, B1, B2  has been pre cleared in preparation for planting in September 2026 - 

Initial site preparation works included  strimming, flailing, of long grass, slashing of briars, removal of undesirabe material / other . Areas cleared were a mix of open pastureland and overgrown briar areas 
	Not applicable – site presented as is for planting
	

	6
	OAK Woodland B2 Zone – trees at 7 metre spacings – 936 units in total 
	
	

	
	Supply and plant

Quercus robor 6-8 cm girth


	276
	

	
	Supply and plant

Quercus petraea 6-8 cm girth


	165
	

	
	Supply and plant

Pinus sylvestris 6-8 cm girth


	165
	

	
	Supply and plant

Alnus glutinosa 6-8 cm girth


	110
	

	
	Supply and plant

Betula pubescens 6-8 cm girth


	55
	

	
	Supply and plant

Betula pendula 6-8 cm girth


	55
	

	
	Supply and plant

Corylus avellana 1.5 -2m feathered plants

	110
	

	
	Suppy and install slow release fertiliser to trees as per specifcation 
	80 Kg
	

	
	Supply and install for each 6-8 cm tree a full staking unit comprising - 2 x 75mm treated stakes complete with 1 treated crossbar with adjustable rubber tree tie with spacer
	Costs for full staking  of each tree (936 staking systems – 1 per tree ) as per specification 
	

	
	Supply and install approved organic woodchip mulch in a 1.0 m diameter circular ring centred on each tree, to a consolidated depth of 75 mm, maintaining a 50 mm clearance around the stem.

	60 cubic metres
	

	
	
	
	

	
	
	
	

	7
	Birch  Woodland B1  Zone – trees at 7 metre spacings –  468 units in total
	
	

	
	Supply and plant

Quercus robor 6-8 cm girth


	74
	

	
	Supply and plant

Quercus petraea 6-8 cm girth


	49
	

	
	Supply and plant

Pinus sylvestris  6-8 cm girth


	74
	

	
	Supply and plant

Alnus glutinosa 6-8 cm girth


	49
	

	
	Supply and plant

Betula pubescens 6-8 cm girth


	123
	

	
	Supply and plant

Betula pendula 6-8 cm girth


	74
	

	
	Supply and plant

Corylus avellana  1.5 – 2 m feathered plants

	25
	

	
	Suppy and install slow release fertiliser to trees as per specifcation
	40 kg 
	

	
	Supply and install for each 6-8 cm tree a full staking unit comprising - 2 x 75mm treated stakes complete with 1 treated crossbar with adjustable rubber tree tie with spacer
	Costs for full staking  of each tree (468 staking systems – 1 per tree ) as per specification
	

	
	Supply and install approved organic woodchip mulch in a 1.0 m diameter circular ring centred on each tree, to a consolidated depth of 75 mm, maintaining a 50 mm clearance around the stem
	30 cubic metres 
	

	
	
	
	

	8
	Site De-Mobilisation

Removal of all plant, equipment, materials, waste, compound, welfare facilities, construction signage,

temporary fencing leaving site in a tidy and safe manner
	Item
	

	
	
	
	

	9
	Clean up and make good

On completion of the works clean and tidy the site
	Item
	

	10
	Handover


	Item
	

	11
	2 x return site visits in July, November 2027 to deal with maintenance checking of posts & retying, planting, replacement of any failed plants, other as per specifications.
	Item 
	

	12
	Any Item not included 
	Item
	

	
	
	
	

	Total excluding VAT
	€


	Total including VAT

	€


***
Sligo County Council, dependent on budget availability, may increase or decrease the quantity of trees, mulch etc. The average rate provided per unit will be the rate used for any proposed amendments (increases or decreases) from the quantities identified in the pricing document 

September 2026

